% $Id$ %
\section{\label{ref:SystemOptions}System}
\subsection{Start Screen}
    Set the screen that Rockbox will start in. Selecting
    \setting{Resume Playback} will resume playback where it was when the \dap{}
    was shut off if there is a playlist to resume and will then end up in the
    WPS. Selecting \setting{Previous Screen} will make Rockbox start in the
    screen it was when the \dap{} was shut off.

\subsection{Battery}
    Options relating to the \opt{archos}{batteries}\nopt{archos}{battery}%
    in the \dap.
  \begin{description}
    \item [Battery Capacity: ]This setting can be used to tell Rockbox what
      capacity (in mAh) of battery is being used inside it. The default is
      \opt{player,recorder}{1500mAh}%
      \opt{recorderv2fm}{2200mAh}%
      \opt{ondiosp,ondiofm}{1000mAh}%
      \opt{h1xx,h300}{1300mAh}%
      \opt{ipodmini}{400mAh (1G) or 630mAh (2G)}%
      \opt{ipodcolor}{700mAh}%
      \opt{ipodnano,ipodvideo,ipod4g,ipod3g}{\fixme{unknown}}%
      \opt{x5}{950mAh}%
      , which is the capacity value for the standard batteries shipped with the
      \dap. Rockbox uses this value to estimate remaining battery life for the 
      statusbar and WPS. Changing this setting has no effect what-so-ever on 
      actual battery life. This setting only affects the accuracy of the 
      battery life estimation as shown on screen.
   
      \opt{ipod}{This value is fairly meaningless in the \playerman{} family at
        present, and work is on-going into finding a better way to determine 
        battery life.}
    
    \opt{ondiosp,ondiofm}{
    \item [Battery Type: ]This setting tells Rockbox which type of battery
      that is currently used in the \dap{}. Select \setting{Alkaline} or
      \setting{NiMH} with \ButtonUp/\ButtonDown.
    }
  \end{description}

\nopt{ondiosp,ondiofm}{
\subsection{Disk}
    Options relating to the hard disk.

  \begin{description}
    \item [Disk Spindown: ]Rockbox has a timer that makes it spin down the
      hard disk after it is idle for a certain amount of time. This setting
      controls the amount of time between the last user activity and the time
      that the disk spins down. This idle time is only affected by user
      activity, like navigating through the \setting{File Browser}. When the
      hard disk spins up to fill the audio buffer, it automatically spins down
      afterwards.

    \opt{SWCODEC}{
    \item [Directory Cache: ]Rockbox has the ability to cache the contents of
      your drive in RAM. The \setting{Directory Cache} takes a small amount of
      memory away from Rockbox that would otherwise be used to buffer music,
      but it speeds up navigation in the \setting{File Browser} by eliminating
      the slight pause between the time a navigation button is pressed and the
      time Rockbox responds. Turning this setting \setting{On} activates the
      directory cache, and turning it \setting{Off} deactivates the directory
      cache.
      \note{The first time you set the directory cache to \setting{On},
      Rockbox will request a reboot of the \dap{} and upon restarting take a few
      minutes to scan the drive. Thereafter, the directory cache will work in the
      background.}
    }
  \end{description}
} % \nopt{ondiosp,ondiofm}

\opt{CONFIG_RTC}{
  \subsection{Time and Date}
  Time related menu options.
    \begin{description}
      \item [Set Time/Date: ]Set current time and date.
      \item [Time Format: ] Choose 12 or 24 Hour clock.
    \end{description}
}

\subsection{Idle Poweroff}
Rockbox can be configured to turn off power after the unit has been idle for a
defined number of minutes. The \dap{} is idle when playback is stopped or
paused. It is not idle while the USB or charger is connected, or while
recording. Settings are either \setting{Off} or \setting{1} to \setting{10}
minutes in 1 minute steps. Then \setting{15,30,45} and \setting{60} minutes are
available.

\opt{HAVE_RTC_ALARM}{
\subsection{Wake Up alarm}
    This option turns the \dap{} off and then starts it up again at the 
    specified time. This is most useful when combined with
    \setting{Start Screen} set to \setting{Resume Playback}, so 
    that the \dap{} wakes up and immediately starts playing music. Use 
    \ActionSettingInc{} and \ActionSettingDec to adjust the minutes setting,
    \ButtonLeft{} and \ButtonRight{} to adjust the HOURS.
    \ButtonPlay{} confirms the alarm and shuts your \dap{} down, and
    \opt{RECORDER_PAD}{\ButtonOff}\opt{IPOD_4G_PAD,IPOD_3G_PAD}{\ButtonMenu}
    cancels setting an alarm. If the \dap{} is turned on again before the alarm
    occurs, the alarm will be cancelled. Using this option disables the 
    \setting{Sleep Timer}.
}

\subsection{Limits}
This sub menu relates to limits in the Rockbox operating system.
  \begin{description}
    \item [Max files in dir browser: ]This setting controls the limit on
    the number of files that you can put in any particular directory in the
    \setting{File Browser}. You can configure the size to be between 50 and
    10,000 files in steps of 50. The default is 400. Higher values will shorten
    the music buffer, so you should increase this setting \emph{only} if you have
    directories with a large number of files.

    \item [Max playlist size: ]This setting controls the maximum size of 
    a playlist. The playlist size can be between 1,000 and 20,000 files,
    in steps of 1,000 (default is 10,000). Higher values will shorten the
    music buffer, so you should increase this setting \emph{only} if you
    have very large playlists.
  \end{description}

\opt{player,recorder,recorderv2fm,gigabeat,ipodvideo,iriver,iaudio,e200}{
\subsection{Car Adapter Mode}
      This option turns \setting{On} and \setting{Off} the car ignition
      auto stop function.
  \begin{description}
  \item [Car Adapter Mode: ]When using the \dap{} in a car,
  \setting{Car Adapter Mode} automatically stops playback on the \dap{} when
  power (i.e. from cigarette lighter power adapter) to the external DC in jack
  is turned off. If the \setting{Car Adapter Mode} is set to \setting{On},
  Rockbox will pause playback when the external power off condition is
  detected. Rockbox will then shutdown the \dap{} after the length of time set
  in the \setting{Idle Poweroff} setting (see above).
  If power to the DC in jack is turned back on before the \emph{Idle Poweroff}
  function has shut the \dap{} off, playback will be resumed 5 seconds after
  the power is applied. This delay is to allow for the time while the car
  engine is being started.
  \end{description}

  Once the \dap{} is shut off either manually, or automatically with the
  \setting{Idle Poweroff} function, it must be powered up manually to resume
  playback.
}

\opt{player}{
  \subsection{Line In} This option activates the line in port on \dap, which is
    off by default. This is useful for such applications as:
    \begin{itemize}
    \item Game boy $\rightarrow$ \dap $\rightarrow$ human
    \item laptop $\rightarrow$ \dap $\rightarrow$ human
    \item LAN party computer $\rightarrow$ \dap $\rightarrow$ human
    \end{itemize}
}
