No logfile was found.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

The project file (XMP) has changed on disk.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

At Local date and time: Tue Jun 30 18:36:00 2009
 make -f system.make netlistclean started...

rm -f implementation/system.ngc
rm -f platgen.log
rm -f __xps/ise/_xmsgs/platgen.xmsgs
rm -f implementation/system.bmm


Done!

At Local date and time: Tue Jun 30 18:36:05 2009
 make -f system.make bitsclean started...

rm -f implementation/system.bit
rm -f implementation/system.ncd
rm -f implementation/system_bd.bmm 
rm -f implementation/system_map.ncd 
rm -f __xps/system_routed


Done!

At Local date and time: Tue Jun 30 18:36:10 2009
 make -f system.make hwclean started...

rm -f implementation/system.ngc
rm -f platgen.log
rm -f __xps/ise/_xmsgs/platgen.xmsgs
rm -f implementation/system.bmm
rm -f implementation/system.bit
rm -f implementation/system.ncd
rm -f implementation/system_bd.bmm 
rm -f implementation/system_map.ncd 
rm -f __xps/system_routed
rm -rf implementation synthesis xst hdl
rm -rf xst.srp system.srp
rm -f __xps/ise/_xmsgs/bitinit.xmsgs


Done!

At Local date and time: Tue Jun 30 18:36:16 2009
 make -f system.make libsclean started...

rm -rf ppc440_0/
rm -f libgen.log
rm -f __xps/ise/_xmsgs/libgen.xmsgs


Done!

At Local date and time: Tue Jun 30 18:36:20 2009
 make -f system.make programclean started...

rm -f RTOSDemo/executable.elf 


Done!

At Local date and time: Tue Jun 30 18:36:25 2009
 make -f system.make swclean started...

rm -rf ppc440_0/
rm -f libgen.log
rm -f __xps/ise/_xmsgs/libgen.xmsgs
rm -f RTOSDemo/executable.elf 


Done!

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Tue Jun 30 22:00:27 2009
 make -f system.make bits started...

****************************************************
Creating system netlist for hardware specification..
****************************************************
platgen -p xc5vfx70tff1136-1 -lang vhdl   -msg __xps/ise/xmsgprops.lst system.mhs


Release 11.2 - platgen Xilinx EDK 11.2 Build EDK_LS3.47

 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.





Command Line: platgen -p xc5vfx70tff1136-1 -lang vhdl -msg

__xps/ise/xmsgprops.lst system.mhs 



Parse

C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/system.mhs

...



Read MPD definitions ...

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 298 - deprecated core for architecture 'virtex5fx'!



Overriding IP level properties ...



Performing IP level DRCs on properties...



Running DRC Tcl procedures for OPTION IPLEVEL_DRC_PROC...

Address Map for Processor ppc440_0

  (0b0000000000-0b0011111111) ppc440_0	

  (0000000000-0x0fffffff) DDR2_SDRAM	ppc440_0_PPC440MC

  (0x81000000-0x8100ffff) Ethernet_MAC	plb_v46_0

  (0x81400000-0x8140ffff) Push_Buttons_5Bit	plb_v46_0

  (0x81420000-0x8142ffff) LEDs_Positions	plb_v46_0

  (0x81440000-0x8144ffff) LEDs_8Bit	plb_v46_0

  (0x81460000-0x8146ffff) DIP_Switches_8Bit	plb_v46_0

  (0x81600000-0x8160ffff) IIC_EEPROM	plb_v46_0

  (0x81800000-0x8180ffff) xps_intc_0	plb_v46_0

  (0x83600000-0x8360ffff) SysACE_CompactFlash	plb_v46_0

  (0x84000000-0x8400ffff) RS232_Uart_1	plb_v46_0

  (0x85c00000-0x85c0ffff) PCIe_Bridge	plb_v46_0

  (0xc0000000-0xdfffffff) PCIe_Bridge	plb_v46_0

  (0xe0000000-0xefffffff) PCIe_Bridge	plb_v46_0

  (0xf8000000-0xf80fffff) SRAM	plb_v46_0

  (0xffffe000-0xffffffff) xps_bram_if_cntlr_1	plb_v46_0

INFO:EDK:1560 - IPNAME:ppc440_virtex5 INSTANCE:ppc440_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\ppc440_virtex5_v1_

   01_a\data\ppc440_virtex5_v2_1_0.mpd line 175 - tool is overriding PARAMETER

   C_SPLB0_P2P value to 0



Computing clock values...

INFO:EDK:1432 - Frequency for Top-Level Input Clock

   'fpga_0_PCIe_Diff_Clk_IBUF_DS_P_pin' is not specified. Clock DRCs will not be

   performed for IPs connected to that clock port, unless they are connected

   through the clock generator IP. 



INFO:EDK:1432 - Frequency for Top-Level Input Clock

   'fpga_0_PCIe_Diff_Clk_IBUF_DS_N_pin' is not specified. Clock DRCs will not be

   performed for IPs connected to that clock port, unless they are connected

   through the clock generator IP. 



INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 70 - tool is overriding PARAMETER

   C_PLBV46_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 71 - tool is overriding PARAMETER

   C_PLBV46_NUM_SLAVES value to 12

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 72 - tool is overriding PARAMETER

   C_PLBV46_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 74 - tool is overriding PARAMETER C_PLBV46_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_bram_if_cntlr INSTANCE:xps_bram_if_cntlr_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_bram_if_cntlr_

   v1_00_b\data\xps_bram_if_cntlr_v2_1_0.mpd line 75 - tool is overriding

   PARAMETER C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_bram_if_cntlr INSTANCE:xps_bram_if_cntlr_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_bram_if_cntlr_

   v1_00_b\data\xps_bram_if_cntlr_v2_1_0.mpd line 76 - tool is overriding

   PARAMETER C_SPLB_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:xps_bram_if_cntlr INSTANCE:xps_bram_if_cntlr_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_bram_if_cntlr_

   v1_00_b\data\xps_bram_if_cntlr_v2_1_0.mpd line 80 - tool is overriding

   PARAMETER C_SPLB_SMALLEST_MASTER value to 128

INFO:EDK:1560 - IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a

   \data\bram_block_v2_1_0.mpd line 69 - tool is overriding PARAMETER C_MEMSIZE

   value to 0x2000

INFO:EDK:1560 - IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a

   \data\bram_block_v2_1_0.mpd line 70 - tool is overriding PARAMETER

   C_PORT_DWIDTH value to 64

INFO:EDK:1560 - IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a

   \data\bram_block_v2_1_0.mpd line 72 - tool is overriding PARAMETER C_NUM_WE

   value to 8

INFO:EDK:1560 - IPNAME:xps_uartlite INSTANCE:RS232_Uart_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_uartlite_v1_01

   _a\data\xps_uartlite_v2_1_0.mpd line 73 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:LEDs_8Bit -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:LEDs_Positions -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:Push_Buttons_5Bit -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:DIP_Switches_8Bit -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_iic INSTANCE:IIC_EEPROM -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_iic_v2_01_a\da

   ta\xps_iic_v2_1_0.mpd line 79 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_mch_emc INSTANCE:SRAM -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_mch_emc_v3_00_

   a\data\xps_mch_emc_v2_1_0.mpd line 82 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_mch_emc INSTANCE:SRAM -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_mch_emc_v3_00_

   a\data\xps_mch_emc_v2_1_0.mpd line 84 - tool is overriding PARAMETER

   C_SPLB_SMALLEST_MASTER value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 86 - tool is overriding PARAMETER

   C_MPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 87 - tool is overriding PARAMETER

   C_MPLB_SMALLEST_SLAVE value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 89 - tool is overriding PARAMETER

   C_SPLB_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 90 - tool is overriding PARAMETER

   C_SPLB_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 91 - tool is overriding PARAMETER

   C_SPLB_SMALLEST_MASTER value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 95 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 70 - tool is overriding PARAMETER

   C_PLBV46_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 71 - tool is overriding PARAMETER

   C_PLBV46_NUM_SLAVES value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 72 - tool is overriding PARAMETER

   C_PLBV46_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 74 - tool is overriding PARAMETER C_PLBV46_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_ethernetlite_v

   2_01_a\data\xps_ethernetlite_v2_1_0.mpd line 75 - tool is overriding

   PARAMETER C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_sysace INSTANCE:SysACE_CompactFlash -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_sysace_v1_01_a

   \data\xps_sysace_v2_1_0.mpd line 72 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_sysace INSTANCE:SysACE_CompactFlash -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_sysace_v1_01_a

   \data\xps_sysace_v2_1_0.mpd line 74 - tool is overriding PARAMETER

   C_SPLB_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:xps_sysace INSTANCE:SysACE_CompactFlash -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_sysace_v1_01_a

   \data\xps_sysace_v2_1_0.mpd line 75 - tool is overriding PARAMETER

   C_SPLB_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:xps_intc INSTANCE:xps_intc_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_intc_v2_00_a\d

   ata\xps_intc_v2_1_0.mpd line 72 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128



Checking platform address map ...



Checking platform configuration ...

INFO:EDK:1563 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 298 - This design requires design constraints to guarantee

   performance.

   Please refer to the xps_ethernetlite_v2_00_a data sheet for details.  

   The PLB clock frequency must be greater than or equal to 50 MHz for 100 Mbs

   Ethernet operation and greater than or equal to 5.0 MHz for 10 Mbs Ethernet

   operation.

IPNAME:plb_v46 INSTANCE:plb_v46_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 109 - 1 master(s) : 12 slave(s)

IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 290 - 1 master(s) : 1 slave(s)

IPNAME:fcb_v20 INSTANCE:ppc440_0_fcb_v20 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 394 - 1 master(s) : 1 slave(s)



Checking port drivers...

WARNING:EDK:2099 - PORT:Peripheral_Reset CONNECTOR:sys_periph_reset -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 461 - floating connection!



Performing Clock DRCs...



Performing Reset DRCs...



Overriding system level properties...

INFO:EDK:1560 - IPNAME:ppc440_virtex5 INSTANCE:ppc440_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\ppc440_virtex5_v1_

   01_a\data\ppc440_virtex5_v2_1_0.mpd line 124 - tcl is overriding PARAMETER

   C_PPC440MC_ADDR_BASE value to 0x00000000

INFO:EDK:1560 - IPNAME:ppc440_virtex5 INSTANCE:ppc440_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\ppc440_virtex5_v1_

   01_a\data\ppc440_virtex5_v2_1_0.mpd line 125 - tcl is overriding PARAMETER

   C_PPC440MC_ADDR_HIGH value to 0x0fffffff

INFO:EDK:1560 - IPNAME:jtagppc_cntlr INSTANCE:jtagppc_cntlr_inst -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\jtagppc_cntlr_v2_0

   1_c\data\jtagppc_cntlr_v2_1_0.mpd line 70 - tcl is overriding PARAMETER

   C_NUM_PPC_USED value to 1

INFO:EDK:1560 - IPNAME:xps_intc INSTANCE:xps_intc_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_intc_v2_00_a\d

   ata\xps_intc_v2_1_0.mpd line 79 - tcl is overriding PARAMETER C_KIND_OF_INTR

   value to 0b00000000000000000000000000000001

INFO:EDK:1560 - IPNAME:xps_intc INSTANCE:xps_intc_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_intc_v2_00_a\d

   ata\xps_intc_v2_1_0.mpd line 80 - tcl is overriding PARAMETER C_KIND_OF_EDGE

   value to 0b00000000000000000000000000000001

INFO:EDK:1560 - IPNAME:xps_intc INSTANCE:xps_intc_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_intc_v2_00_a\d

   ata\xps_intc_v2_1_0.mpd line 81 - tcl is overriding PARAMETER C_KIND_OF_LVL

   value to 0b00000000000000000000000000000000



Running system level update procedures...



Running UPDATE Tcl procedures for OPTION SYSLEVEL_UPDATE_PROC...



Running system level DRCs...



Performing System level DRCs on properties...



Running DRC Tcl procedures for OPTION SYSLEVEL_DRC_PROC...



Running UPDATE Tcl procedures for OPTION PLATGEN_SYSLEVEL_UPDATE_PROC...

INFO: The PCIe_Bridge core has constraints automatically generated by XPS in

implementation/pcie_bridge_wrapper/pcie_bridge_wrapper.ucf.


It can be overridden by constraints placed in the system.ucf file.









INFO: The Ethernet_MAC core has constraints automatically generated by XPS in

implementation/ethernet_mac_wrapper/ethernet_mac_wrapper.ucf.


It can be overridden by constraints placed in the system.ucf file.









INFO: The DDR2_SDRAM core has constraints automatically generated by XPS in

implementation/ddr2_sdram_wrapper/ddr2_sdram_wrapper.ucf.


It can be overridden by constraints placed in the system.ucf file.











Modify defaults ...



Creating stub ...



Processing licensed instances ...

Completion time: 0.00 seconds



Creating hardware output directories ...



Managing hardware (BBD-specified) netlist files ...

IPNAME:plbv46_pcie INSTANCE:pcie_bridge -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 253 - Copying (BBD-specified) netlist files.

IPNAME:xps_ethernetlite INSTANCE:ethernet_mac -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 298 - Copying (BBD-specified) netlist files.

IPNAME:apu_fpu_virtex5 INSTANCE:ppc440_0_apu_fpu_virtex5 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 401 - Copying (BBD-specified) netlist files.



Managing cache ...



Elaborating instances ...

IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 131 - elaborating IP



Writing HDL for elaborated instances ...



Inserting wrapper level ...

Completion time: 0.00 seconds



Constructing platform-level connectivity ...

Completion time: 1.00 seconds



Writing (top-level) BMM ...



Writing (top-level and wrappers) HDL ...



Generating synthesis project file ...



Running XST synthesis ...



INFO:EDK:2502 - The following instances are synthesized with XST. The MPD option

   IMP_NETLIST=TRUE indicates that a NGC file is to be produced using XST

   synthesis. IMP_NETLIST=FALSE (default) instances are not synthesized. 

INSTANCE:ppc440_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 78 - Running XST synthesis

INSTANCE:plb_v46_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 109 - Running XST synthesis

INSTANCE:xps_bram_if_cntlr_1 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 118 - Running XST synthesis

INSTANCE:xps_bram_if_cntlr_1_bram -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 131 - Running XST synthesis

INSTANCE:rs232_uart_1 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 138 - Running XST synthesis

INSTANCE:leds_8bit -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 154 - Running XST synthesis

INSTANCE:leds_positions -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 168 - Running XST synthesis

INSTANCE:push_buttons_5bit -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 182 - Running XST synthesis

INSTANCE:dip_switches_8bit -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 196 - Running XST synthesis

INSTANCE:iic_eeprom -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 210 - Running XST synthesis

INSTANCE:sram -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 223 - Running XST synthesis

INSTANCE:pcie_bridge -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 253 - Running XST synthesis

INSTANCE:ppc440_0_splb0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 290 - Running XST synthesis

INSTANCE:ethernet_mac -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 298 - Running XST synthesis

INSTANCE:ddr2_sdram -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 317 - Running XST synthesis

INSTANCE:sysace_compactflash -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 377 - Running XST synthesis

INSTANCE:ppc440_0_fcb_v20 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 394 - Running XST synthesis

INSTANCE:ppc440_0_apu_fpu_virtex5 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 401 - Running XST synthesis

INSTANCE:clock_generator_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 407 - Running XST synthesis

INSTANCE:jtagppc_cntlr_inst -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 446 - Running XST synthesis

INSTANCE:proc_sys_reset_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 452 - Running XST synthesis

INSTANCE:xps_intc_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 464 - Running XST synthesis



Running NGCBUILD ...

IPNAME:ppc440_0_wrapper INSTANCE:ppc440_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 78 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -uc ppc440_0_wrapper.ucf -sd ..

ppc440_0_wrapper.ngc ../ppc440_0_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/ppc440_0_wrapper/ppc440_0_wrapper.ngc" ...



Applying constraints in "ppc440_0_wrapper.ucf" to the design...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../ppc440_0_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  6 sec

Total CPU time to NGCBUILD completion:   6 sec



Writing NGCBUILD log file "../ppc440_0_wrapper.blc"...



NGCBUILD done.

IPNAME:rs232_uart_1_wrapper INSTANCE:rs232_uart_1 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 138 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -sd .. rs232_uart_1_wrapper.ngc

../rs232_uart_1_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/rs232_uart_1_wrapper/rs232_uart_1_wrapper.ngc" ...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../rs232_uart_1_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  2 sec

Total CPU time to NGCBUILD completion:   2 sec



Writing NGCBUILD log file "../rs232_uart_1_wrapper.blc"...



NGCBUILD done.

IPNAME:pcie_bridge_wrapper INSTANCE:pcie_bridge -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 253 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -uc pcie_bridge_wrapper.ucf -sd ..

pcie_bridge_wrapper.ngc ../pcie_bridge_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/pcie_bridge_wrapper/pcie_bridge_wrapper.ngc" ...

Executing edif2ngd -noa

"C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\implementa

tion\pcie_bridge_wrapper_fifo_generator_v4_3.edn"

"pcie_bridge_wrapper_fifo_generator_v4_3.ngo"

Release 11.2 - edif2ngd L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

INFO:NgdBuild - Release 11.2 edif2ngd L.46 (nt)

INFO:NgdBuild - Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

PMSPEC -- Overriding Xilinx file <C:/devtools/Xilinx/11.1/EDK/data/edif2ngd.pfd>

with local file <C:/devtools/Xilinx/11.1/ISE/data/edif2ngd.pfd>

Writing module to "pcie_bridge_wrapper_fifo_generator_v4_3.ngo"...

Loading design module

"C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\implementa

tion\pcie_bridge_wrapper\pcie_bridge_wrapper_fifo_generator_v4_3.ngo"...

Loading design module

"../pcie_bridge_wrapper_fifo_generator_v4_3_fifo_generator_v4_3_xst_1.ngc"...

Loading design module

"C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\implementa

tion\pcie_bridge_wrapper/dpram_70_512.ngc"...

Loading design module

"C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\implementa

tion\pcie_bridge_wrapper/fifo_71x512.ngc"...



Applying constraints in "pcie_bridge_wrapper.ucf" to the design...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../pcie_bridge_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  13 sec

Total CPU time to NGCBUILD completion:   9 sec



Writing NGCBUILD log file "../pcie_bridge_wrapper.blc"...



NGCBUILD done.

IPNAME:ethernet_mac_wrapper INSTANCE:ethernet_mac -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 298 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -uc ethernet_mac_wrapper.ucf -sd ..

ethernet_mac_wrapper.ngc ../ethernet_mac_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/ethernet_mac_wrapper/ethernet_mac_wrapper.ngc" ...

Executing edif2ngd -noa "ethernetlite_v1_01_b_dmem_v2.edn"

"ethernetlite_v1_01_b_dmem_v2.ngo"

Release 11.2 - edif2ngd L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

INFO:NgdBuild - Release 11.2 edif2ngd L.46 (nt)

INFO:NgdBuild - Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

PMSPEC -- Overriding Xilinx file <C:/devtools/Xilinx/11.1/EDK/data/edif2ngd.pfd>

with local file <C:/devtools/Xilinx/11.1/ISE/data/edif2ngd.pfd>

Writing module to "ethernetlite_v1_01_b_dmem_v2.ngo"...

Loading design module

"C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\implementa

tion\ethernet_mac_wrapper\ethernetlite_v1_01_b_dmem_v2.ngo"...



Applying constraints in "ethernet_mac_wrapper.ucf" to the design...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../ethernet_mac_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  9 sec

Total CPU time to NGCBUILD completion:   6 sec



Writing NGCBUILD log file "../ethernet_mac_wrapper.blc"...



NGCBUILD done.

IPNAME:ddr2_sdram_wrapper INSTANCE:ddr2_sdram -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 317 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -uc ddr2_sdram_wrapper.ucf -sd ..

ddr2_sdram_wrapper.ngc ../ddr2_sdram_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/ddr2_sdram_wrapper/ddr2_sdram_wrapper.ngc" ...



Applying constraints in "ddr2_sdram_wrapper.ucf" to the design...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../ddr2_sdram_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  7 sec

Total CPU time to NGCBUILD completion:   7 sec



Writing NGCBUILD log file "../ddr2_sdram_wrapper.blc"...



NGCBUILD done.

IPNAME:ppc440_0_apu_fpu_virtex5_wrapper INSTANCE:ppc440_0_apu_fpu_virtex5 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 401 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -uc ppc440_0_apu_fpu_virtex5_wrapper.ucf -sd

.. ppc440_0_apu_fpu_virtex5_wrapper.ngc ../ppc440_0_apu_fpu_virtex5_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/ppc440_0_apu_fpu_virtex5_wrapper/ppc440_0_apu_fpu_virtex5_wrapper.ngc" ...

Loading design module

"C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\implementa

tion\ppc440_0_apu_fpu_virtex5_wrapper/apu_fpu_dp_lo.ngc"...



Applying constraints in "ppc440_0_apu_fpu_virtex5_wrapper.ucf" to the design...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../ppc440_0_apu_fpu_virtex5_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  7 sec

Total CPU time to NGCBUILD completion:   7 sec



Writing NGCBUILD log file "../ppc440_0_apu_fpu_virtex5_wrapper.blc"...



NGCBUILD done.

IPNAME:xps_intc_0_wrapper INSTANCE:xps_intc_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 464 - Running NGCBUILD

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<C:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: C:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe -p

xc5vfx70tff1136-1 -intstyle silent -sd .. xps_intc_0_wrapper.ngc

../xps_intc_0_wrapper.ngc



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/xps_intc_0_wrapper/xps_intc_0_wrapper.ngc" ...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../xps_intc_0_wrapper.ngc" ...

Total REAL time to NGCBUILD completion:  2 sec

Total CPU time to NGCBUILD completion:   2 sec



Writing NGCBUILD log file "../xps_intc_0_wrapper.blc"...



NGCBUILD done.



Rebuilding cache ...



Total run time: 1120.00 seconds

Running synthesis...
bash -c "cd synthesis; ./synthesis.sh"
xst -ifn system_xst.scr -intstyle silent
Running XST synthesis ...
XST completed
Release 11.2 - ngcbuild L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Overriding Xilinx file <ngcflow.csf> with local file

<c:/devtools/Xilinx/11.1/ISE/data/ngcflow.csf>



Command Line: c:\devtools\Xilinx\11.1\ISE\bin\nt\unwrapped\ngcbuild.exe

./system.ngc ../implementation/system.ngc -sd ../implementation -i -ise

../__xps/ise/system.ise



Reading NGO file

"c:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/synthesis/

system.ngc" ...

Loading design module "../implementation/ppc440_0_wrapper.ngc"...

Loading design module "../implementation/plb_v46_0_wrapper.ngc"...

Loading design module "../implementation/xps_bram_if_cntlr_1_wrapper.ngc"...

Loading design module

"../implementation/xps_bram_if_cntlr_1_bram_wrapper.ngc"...

Loading design module "../implementation/rs232_uart_1_wrapper.ngc"...

Loading design module "../implementation/leds_8bit_wrapper.ngc"...

Loading design module "../implementation/leds_positions_wrapper.ngc"...

Loading design module "../implementation/push_buttons_5bit_wrapper.ngc"...

Loading design module "../implementation/dip_switches_8bit_wrapper.ngc"...

Loading design module "../implementation/iic_eeprom_wrapper.ngc"...

Loading design module "../implementation/sram_wrapper.ngc"...

Loading design module "../implementation/pcie_bridge_wrapper.ngc"...

Loading design module "../implementation/ppc440_0_splb0_wrapper.ngc"...

Loading design module "../implementation/ethernet_mac_wrapper.ngc"...

Loading design module "../implementation/ddr2_sdram_wrapper.ngc"...

Loading design module "../implementation/sysace_compactflash_wrapper.ngc"...

Loading design module "../implementation/ppc440_0_fcb_v20_wrapper.ngc"...

Loading design module

"../implementation/ppc440_0_apu_fpu_virtex5_wrapper.ngc"...

Loading design module "../implementation/clock_generator_0_wrapper.ngc"...

Loading design module "../implementation/jtagppc_cntlr_inst_wrapper.ngc"...

Loading design module "../implementation/proc_sys_reset_0_wrapper.ngc"...

Loading design module "../implementation/xps_intc_0_wrapper.ngc"...



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGCBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings:   0



Writing NGC file "../implementation/system.ngc" ...

Total REAL time to NGCBUILD completion:  12 sec

Total CPU time to NGCBUILD completion:   11 sec



Writing NGCBUILD log file "../implementation/system.blc"...



NGCBUILD done.

*********************************************
Running Xilinx Implementation tools..
*********************************************
xflow -wd implementation -p xc5vfx70tff1136-1 -implement xflow.opt -ise ../__xps/ise/system.ise system.ngc
Release 11.2 - Xflow L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

xflow.exe -wd implementation -p xc5vfx70tff1136-1 -implement xflow.opt -ise

../__xps/ise/system.ise system.ngc  

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<c:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>

.... Copying flowfile c:/devtools/Xilinx/11.1/ISE/xilinx/data/fpga.flw into

working directory

C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementat

ion 



Using Flow File:

C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementat

ion/fpga.flw 

Using Option File(s): 

 C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/xflow.opt 



Creating Script File ... 



#----------------------------------------------#

# Starting program ngdbuild

# ngdbuild -ise ../__xps/ise/system.ise -p xc5vfx70tff1136-1 -nt timestamp -bm

system.bmm

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/system.ngc" -uc system.ucf system.ngd 

#----------------------------------------------#

Release 11.2 - ngdbuild L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<c:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>



Command Line: ngdbuild -ise ../__xps/ise/system.ise -p xc5vfx70tff1136-1 -nt

timestamp -bm system.bmm

C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementat

ion/system.ngc -uc system.ucf system.ngd



Reading NGO file

"C:/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/implementa

tion/system.ngc" ...

Gathering constraint information from source properties...

Done.



Applying constraints in "system.ucf" to the design...

WARNING:NgdBuild:931 - The value of SIM_DEVICE on instance

   'clock_generator_0/clock_generator_0/Using_DCM0.DCM0_INST/DCM_INST/Using_DCM_

   ADV.DCM_ADV_INST' of type DCM_ADV has been changed from 'VIRTEX4' to

   'VIRTEX5' to correct post-ngdbuild and timing simulation for this primitive. 

   In order for functional simulation to be correct, the value of SIM_DEVICE

   should be changed in this same manner in the source netlist or constraint

   file.

Resolving constraint associations...

Checking Constraint Associations...

WARNING:ConstraintSystem:3 - Constraint <TIMESPEC "TS_MC_RD_DATA_SEL" = FROM

   "TNM_RD_DATA_SEL" TO "TNM_CLK0" "TS_clk_div_slow_0_clk_div_slow_0_DDR2_CLK_i"

   * 4;> [system.ucf(264)]: This constraint will be ignored because the relative

   clock constraint named 'TS_clk_div_slow_0_clk_div_slow_0_DDR2_CLK_i' was not

   found.



INFO:ConstraintSystem:178 - TNM 'sys_clk_pin', used in period specification

   'TS_sys_clk_pin', was traced into PLL_ADV instance

   clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst.

   The following new TNM groups and period specifications were generated at the

   PLL_ADV output(s): 

   CLKOUT0: <TIMESPEC TS_clock_generator_0_clock_generator_0_PLL0_CLK_OUT_0_ =

   PERIOD "clock_generator_0_clock_generator_0_PLL0_CLK_OUT_0_" TS_sys_clk_pin *

   1.25 PHASE 2 ns HIGH 50%>



INFO:ConstraintSystem:178 - TNM 'sys_clk_pin', used in period specification

   'TS_sys_clk_pin', was traced into PLL_ADV instance

   clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst.

   The following new TNM groups and period specifications were generated at the

   PLL_ADV output(s): 

   CLKOUT1: <TIMESPEC TS_clock_generator_0_clock_generator_0_PLL0_CLK_OUT_1_ =

   PERIOD "clock_generator_0_clock_generator_0_PLL0_CLK_OUT_1_" TS_sys_clk_pin *

   1.25 HIGH 50%>



INFO:ConstraintSystem:178 - TNM 'sys_clk_pin', used in period specification

   'TS_sys_clk_pin', was traced into PLL_ADV instance

   clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst.

   The following new TNM groups and period specifications were generated at the

   PLL_ADV output(s): 

   CLKOUT2: <TIMESPEC TS_clock_generator_0_clock_generator_0_PLL0_CLK_OUT_2_ =

   PERIOD "clock_generator_0_clock_generator_0_PLL0_CLK_OUT_2_" TS_sys_clk_pin *

   1.25 HIGH 50%>



INFO:ConstraintSystem:178 - TNM 'sys_clk_pin', used in period specification

   'TS_sys_clk_pin', was traced into PLL_ADV instance

   clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst.

   The following new TNM groups and period specifications were generated at the

   PLL_ADV output(s): 

   CLKOUT3: <TIMESPEC TS_clock_generator_0_clock_generator_0_PLL0_CLK_OUT_3_ =

   PERIOD "clock_generator_0_clock_generator_0_PLL0_CLK_OUT_3_" TS_sys_clk_pin *

   2 HIGH 50%>



INFO:ConstraintSystem:178 - TNM 'sys_clk_pin', used in period specification

   'TS_sys_clk_pin', was traced into PLL_ADV instance

   clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst.

   The following new TNM groups and period specifications were generated at the

   PLL_ADV output(s): 

   CLKOUT4: <TIMESPEC TS_clock_generator_0_clock_generator_0_PLL0_CLK_OUT_4_ =

   PERIOD "clock_generator_0_clock_generator_0_PLL0_CLK_OUT_4_" TS_sys_clk_pin *

   0.625 HIGH 50%>



Done...

Checking Partitions ...



Processing BMM file ...



WARNING:NgdBuild:1212 - User specified non-default attribute value

   (8.0000000000000000) was detected for the CLKIN_PERIOD attribute on DCM

   "clock_generator_0/Using_DCM0.DCM0_INST/DCM_INST/Using_DCM_ADV.DCM_ADV_INST".

    This does not match the PERIOD constraint value (5 ns.).  The uncertainty

   calculation will use the non-default attribute value.  This could result in

   incorrect uncertainty calculated for DCM output clocks.

Checking expanded design ...

WARNING:NgdBuild:443 - SFF primitive

   'xps_bram_if_cntlr_1/xps_bram_if_cntlr_1/INCLUDE_BURST_SUPPORT.I_SLAVE_BURST_

   ATTACH/I_DBEAT_CONTROL/I_DBEAT_CNTR/STRUCTURAL_A_GEN.I_ADDSUB_GEN[4].FDRE_I'

   has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/EMC_CTRL_I/MEM_STEER_I/SYNC_MEM_DQT.REG_DQT_GEN[2].DQT_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/EMC_CTRL_I/MEM_STEER_I/GSYNC_MEM_RDACK_GEN.ADDR_ALIGN_PIPE_GEN[3].

   ALIGN_PIPE' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_DECODER/GEN_CE_FOR_SHARED.GEN_BKEND_CE_REGISTERS[0].I_BKEND_WRCE_REG'

   has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_DECODER/GEN_CE_FOR_SHARED.GEN_BKEND_CE_REGISTERS[0].I_BKEND_RDCE_REG'

   has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BURST_SUPPORT/RESPONSE_DBEAT_CNTR_I/STRUCTURAL_A_GEN.I_ADDSUB_GEN[7].FD

   RE_I' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BURST_SUPPORT/CONTROL_DBEAT_CNTR_I/STRUCTURAL_A_GEN.I_ADDSUB_GEN[7].FDR

   E_I' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[0].I_FDRSE_BE0to3

   ' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[1].I_FDRSE_BE0to3

   ' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[2].I_FDRSE_BE0to3

   ' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[3].I_FDRSE_BE0to3

   ' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_BUS_ADDRESS_COUNTER/GEN_FOR_SHARED.GEN_S_H_SIZE_REG[0].I_SIZE_S_H_REG'

   has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'SRAM/SRAM/MCH_PLB_IPIF_I/NO_CHNL_IF_GEN.PLBV46_SLAVE_BURST_I/I_SLAVE_ATTACHM

   ENT/I_STEER_ADDRESS_COUNTER/GEN_FOR_SHARED.GEN_S_H_SIZE_REG[0].I_SIZE_S_H_REG

   ' has unconnected output pin

WARNING:NgdBuild:486 - Attribute "CLK_FEEDBACK" is not allowed on symbol

   "PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/use_pll.pll_ad

   v_i" of type "PLL_ADV".  This attribute will be ignored.

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_STEER_ADDRESS_COUNTER/GEN_S_H_SIZE_REG[0].I_SIZE_S_H_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/GEN_S_H_SIZE_REG[0].I_SIZE_S_H_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/GEN_DWIDTH_64_128.LDMUX_FDRSE

   _4to7[7].I_FDRSE_BE4to7' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/GEN_DWIDTH_64_128.LDMUX_FDRSE

   _4to7[6].I_FDRSE_BE4to7' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/GEN_DWIDTH_64_128.LDMUX_FDRSE

   _4to7[5].I_FDRSE_BE4to7' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/GEN_DWIDTH_64_128.LDMUX_FDRSE

   _4to7[4].I_FDRSE_BE4to7' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[3].I_FDRSE_B

   E0to3' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[2].I_FDRSE_B

   E0to3' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[1].I_FDRSE_B

   E0to3' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/GEN_FAST_MODE_B

   URSTXFER.I_BUS_ADDRESS_COUNTER/I_FLEX_ADDR_CNTR/LDMUX_FDRSE_0to3[0].I_FDRSE_B

   E0to3' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_S

   _H_ADDR_REG[6].I_ADDR_S_H_REG' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_S

   _H_ADDR_REG[7].I_ADDR_S_H_REG' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[0].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[0].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[0].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[1].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[1].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[1].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[2].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[2].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[2].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[3].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[3].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[3].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[4].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[4].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[4].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[5].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[5].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[5].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[6].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[6].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[6].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[7].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[7].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[7].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[8].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[8].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[8].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[9].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[9].I_BKend_RDCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[9].I_BKend_WRCE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[10].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[10].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[10].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[11].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[11].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[11].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[12].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[12].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[12].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[13].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[13].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[13].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[14].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[14].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[14].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[15].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[15].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[15].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[16].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[16].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[16].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[17].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[17].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[17].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[18].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[18].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[18].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[19].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[19].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[19].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[20].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[20].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[20].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[21].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[21].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[21].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[22].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[22].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[22].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[23].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[23].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[23].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[24].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[24].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[24].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[25].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[25].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[25].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[26].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[26].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[26].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[27].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[27].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[27].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[28].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[28].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[28].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[29].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[29].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[29].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[30].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[30].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[30].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[31].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[31].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[31].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[32].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[33].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[34].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[35].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[36].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[37].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[38].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[39].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[40].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[41].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[42].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[43].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[44].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[44].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[44].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[45].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[45].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[45].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[46].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[46].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[46].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[47].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[47].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[47].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[48].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[48].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[48].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[49].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[49].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[49].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[50].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[50].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[50].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[51].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[51].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[51].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[52].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[52].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[52].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[53].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[53].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[53].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[54].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[54].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[54].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[55].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[55].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[55].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[56].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[57].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[58].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[59].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[60].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[61].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[61].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[61].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[62].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[62].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[62].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[63].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[63].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[0].GEN_USER_CE.GEN_ALL_CEs[63].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[1].GEN_USER_CE.GEN_ALL_CEs[64].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[1].GEN_USER_CE.GEN_ALL_CEs[64].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[1].GEN_USER_CE.GEN_ALL_CEs[64].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[65].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[66].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[66].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[67].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[68].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[68].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[68].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[69].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[69].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[69].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[70].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[70].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[70].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[71].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[71].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[72].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[73].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[74].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[74].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[74].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[75].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[76].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[76].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[76].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[77].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[77].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[77].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[78].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[78].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[78].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[79].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[79].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[79].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[80].I_BKend_CE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[80].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[2].GEN_INTRPT_CE.GEN_ALL_CEs[80].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[3].GEN_RESET_CE.I_BKend_CE_REG' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[3].GEN_RESET_CE.I_BKend_RDCE_REG' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[4].GEN_USER_CE.GEN_ALL_CEs[82].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[4].GEN_USER_CE.GEN_ALL_CEs[82].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[4].GEN_USER_CE.GEN_ALL_CEs[82].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[5].GEN_USER_CE.GEN_ALL_CEs[83].I_BKend_CE_REG' has unconnected

   output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[5].GEN_USER_CE.GEN_ALL_CEs[83].I_BKend_RDCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/GEN_C

   E_ASSIGNMENTS[5].GEN_USER_CE.GEN_ALL_CEs[83].I_BKend_WRCE_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/I_CS_

   SIZE2_REG0' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/I_CS_

   SIZE2_REG1' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_slave/I_SLAVE_ATTACHMENT/I_DECODER/I_CS_

   SIZE2_REG2' has unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'PCIe_Bridge/PCIe_Bridge/comp_plbv46_master/I_RD_CONTROL/I_RD_ABORT_REG' has

   unconnected output pin

WARNING:NgdBuild:443 - SFF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/COLLISION_SYNC' has unconnected

   output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU10'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU15'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU20'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU25'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU30'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU35'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU130'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/TX/inst_tx_intrfce/I_TX_FIFO/BU237'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU10'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU15'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU20'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU25'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU30'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU35'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU130'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'Ethernet_MAC/Ethernet_MAC/XEMAC_I/EMAC_I/RX/inst_rx_intrfce/I_RX_FIFO/BU237'

   has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[1].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[2].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[3].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[4].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[5].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[6].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/u_phy_calib

   /gen_rden[7].u_calib_rden_r' has unconnected output pin

WARNING:NgdBuild:440 - FF primitive

   'ppc440_0_apu_fpu_virtex5/ppc440_0_apu_fpu_virtex5/gen_apu_fpu_dp_lo.netlist/

   fpu_is_full.sqrt_sqrt_flt_pt_op_sqrt_op.spd.op_round_logic.rnd2_carrys_q_del.

   no_rlocs.fast_del.carry_fd' has unconnected output pin

WARNING:NgdBuild:486 - Attribute "CLK_FEEDBACK" is not allowed on symbol

   "clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst"

   of type "PLL_ADV".  This attribute will be ignored.

WARNING:NgdBuild:452 - logical net 'N194' has no driver

WARNING:NgdBuild:452 - logical net 'N195' has no driver

WARNING:NgdBuild:452 - logical net 'N196' has no driver

WARNING:NgdBuild:452 - logical net 'N197' has no driver

WARNING:NgdBuild:452 - logical net 'N198' has no driver

WARNING:NgdBuild:452 - logical net 'N199' has no driver

WARNING:NgdBuild:452 - logical net 'N200' has no driver

WARNING:NgdBuild:452 - logical net 'N201' has no driver

WARNING:NgdBuild:452 - logical net 'N202' has no driver

WARNING:NgdBuild:452 - logical net 'N203' has no driver

WARNING:NgdBuild:452 - logical net 'N204' has no driver

WARNING:NgdBuild:452 - logical net 'N205' has no driver

WARNING:NgdBuild:452 - logical net 'N206' has no driver

WARNING:NgdBuild:452 - logical net 'N207' has no driver

WARNING:NgdBuild:452 - logical net 'N208' has no driver

WARNING:NgdBuild:452 - logical net 'N209' has no driver

WARNING:NgdBuild:452 - logical net 'N210' has no driver

WARNING:NgdBuild:452 - logical net 'N211' has no driver

WARNING:NgdBuild:452 - logical net 'N212' has no driver

WARNING:NgdBuild:452 - logical net 'N213' has no driver

WARNING:NgdBuild:452 - logical net 'N214' has no driver

WARNING:NgdBuild:452 - logical net 'N215' has no driver

WARNING:NgdBuild:452 - logical net 'N216' has no driver

WARNING:NgdBuild:452 - logical net 'N217' has no driver

WARNING:NgdBuild:452 - logical net 'N218' has no driver

WARNING:NgdBuild:452 - logical net 'N219' has no driver

WARNING:NgdBuild:452 - logical net 'N220' has no driver

WARNING:NgdBuild:452 - logical net 'N221' has no driver

WARNING:NgdBuild:452 - logical net 'N222' has no driver

WARNING:NgdBuild:452 - logical net 'N223' has no driver

WARNING:NgdBuild:452 - logical net 'N224' has no driver

WARNING:NgdBuild:452 - logical net 'N225' has no driver

WARNING:NgdBuild:452 - logical net 'N226' has no driver

WARNING:NgdBuild:452 - logical net 'N227' has no driver

WARNING:NgdBuild:452 - logical net 'N228' has no driver

WARNING:NgdBuild:452 - logical net 'N229' has no driver

WARNING:NgdBuild:452 - logical net 'N230' has no driver

WARNING:NgdBuild:452 - logical net 'N231' has no driver

WARNING:NgdBuild:452 - logical net 'N232' has no driver

WARNING:NgdBuild:452 - logical net 'N233' has no driver

WARNING:NgdBuild:452 - logical net 'N234' has no driver

WARNING:NgdBuild:452 - logical net 'N235' has no driver

WARNING:NgdBuild:452 - logical net 'N236' has no driver

WARNING:NgdBuild:452 - logical net 'N237' has no driver

WARNING:NgdBuild:452 - logical net 'N238' has no driver

WARNING:NgdBuild:452 - logical net 'N239' has no driver

WARNING:NgdBuild:452 - logical net 'N240' has no driver

WARNING:NgdBuild:452 - logical net 'N241' has no driver

WARNING:NgdBuild:452 - logical net 'N242' has no driver

WARNING:NgdBuild:452 - logical net 'N243' has no driver

WARNING:NgdBuild:452 - logical net 'N244' has no driver

WARNING:NgdBuild:452 - logical net 'N245' has no driver

WARNING:NgdBuild:452 - logical net 'N246' has no driver

WARNING:NgdBuild:452 - logical net 'N247' has no driver

WARNING:NgdBuild:452 - logical net 'N248' has no driver

WARNING:NgdBuild:452 - logical net 'N249' has no driver

WARNING:NgdBuild:452 - logical net 'N250' has no driver

WARNING:NgdBuild:452 - logical net 'N251' has no driver

WARNING:NgdBuild:452 - logical net 'N252' has no driver

WARNING:NgdBuild:452 - logical net 'N253' has no driver

WARNING:NgdBuild:452 - logical net 'N254' has no driver

WARNING:NgdBuild:452 - logical net 'N255' has no driver

WARNING:NgdBuild:452 - logical net 'N256' has no driver

WARNING:NgdBuild:452 - logical net 'N257' has no driver

WARNING:NgdBuild:452 - logical net 'N266' has no driver

WARNING:NgdBuild:452 - logical net 'N267' has no driver

WARNING:NgdBuild:452 - logical net 'N268' has no driver

WARNING:NgdBuild:452 - logical net 'N269' has no driver

WARNING:NgdBuild:452 - logical net 'N270' has no driver

WARNING:NgdBuild:452 - logical net 'N271' has no driver

WARNING:NgdBuild:452 - logical net 'N272' has no driver

WARNING:NgdBuild:452 - logical net 'N273' has no driver

WARNING:NgdBuild:452 - logical net 'N306' has no driver

WARNING:NgdBuild:452 - logical net 'N307' has no driver

WARNING:NgdBuild:452 - logical net 'N308' has no driver

WARNING:NgdBuild:452 - logical net 'N309' has no driver

WARNING:NgdBuild:452 - logical net 'N310' has no driver

WARNING:NgdBuild:452 - logical net 'N311' has no driver

WARNING:NgdBuild:452 - logical net 'N312' has no driver

WARNING:NgdBuild:452 - logical net 'N313' has no driver

WARNING:NgdBuild:452 - logical net 'PCIe_Bridge/PCIe_Bridge/sig_trn_terrfwd_n'

   has no driver

WARNING:NgdBuild:452 - logical net 'PCIe_Bridge/PCIe_Bridge/sig_trn_rerrfwd_n'

   has no driver

WARNING:NgdBuild:452 - logical net 'PCIe_Bridge/PCIe_Bridge/sig_trn_tsrc_dsc_n'

   has no driver

WARNING:NgdBuild:452 - logical net 'PCIe_Bridge/PCIe_Bridge/sig_trn_tbuf_av<3>'

   has no driver

WARNING:NgdBuild:452 - logical net 'PCIe_Bridge/PCIe_Bridge/sig_trn_trem_n<4>'

   has no driver



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



NGDBUILD Design Results Summary:

  Number of errors:     0

  Number of warnings: 349



Writing NGD file "system.ngd" ...

Total REAL time to NGDBUILD completion: 2 min  20 sec

Total CPU time to NGDBUILD completion:  1 min  50 sec



Writing NGDBUILD log file "system.bld"...



NGDBUILD done.







#----------------------------------------------#

# Starting program map

# map -ise ../__xps/ise/system.ise -o system_map.ncd -w -pr b -ol high -timing

system.ngd system.pcf 

#----------------------------------------------#

Release 11.2 - Map L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/data/Xdh_PrimTypeLib.xda> with local file

<c:/devtools/Xilinx/11.1/ISE/data/Xdh_PrimTypeLib.xda>

Using target part "5vfx70tff1136-1".

WARNING:LIT:243 - Logical network N194 has no load.

WARNING:LIT:395 - The above warning message is repeated 1028 more times for the

   following (max. 5 shown):

   N195,

   N196,

   N197,

   N198,

   N199

   To see the details of these warning messages, please use the -detail switch.

Mapping design into LUTs...

WARNING:MapLib:701 - Signal fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin

   connected to top level port fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin has

   been removed.

WARNING:MapLib:701 - Signal fpga_0_Ethernet_MAC_PHY_col_pin connected to top

   level port fpga_0_Ethernet_MAC_PHY_col_pin has been removed.

WARNING:MapLib:41 - All members of TNM group "ppc440_0_PPCS0PLBMBUSY" have been

   optimized out of the design.

Writing file system_map.ngm...

WARNING:Pack:2874 - Trimming timing constraints from pin

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_0

   of frag REGCLKAU connected to power/ground net

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_0_REGCLKAU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_0

   of frag REGCLKAL connected to power/ground net

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_0_REGCLKAL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_1

   of frag REGCLKAU connected to power/ground net

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_1_REGCLKAU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_1

   of frag REGCLKAL connected to power/ground net

   xps_bram_if_cntlr_1_bram/xps_bram_if_cntlr_1_bram/ramb36_1_REGCLKAL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[0].ram_tdp2_inst

   of frag REGCLKAU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[0].ram_tdp2_inst_REGCLKAU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[0].ram_tdp2_inst

   of frag REGCLKAL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[0].ram_tdp2_inst_REGCLKAL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[1].ram_tdp2_inst

   of frag REGCLKAU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[1].ram_tdp2_inst_REGCLKAU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[1].ram_tdp2_inst

   of frag REGCLKAL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/pcie_mim_wrapp

   er_i/bram_tl_tx/generate_tdp2[1].ram_tdp2_inst_REGCLKAL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk_if/ll_bridge/r

   x_bridge/fifo_inst/oq_fifo/Mram_regBank

   of frag RDRCLKU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk_if/ll_bridge/r

   x_bridge/fifo_inst/oq_fifo/Mram_regBank_RDRCLKU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk_if/ll_bridge/r

   x_bridge/fifo_inst/oq_fifo/Mram_regBank

   of frag RDRCLKL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk_if/ll_bridge/r

   x_bridge/fifo_inst/oq_fifo/Mram_regBank_RDRCLKL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/Comp_FIFO/CompFIFO_64.dpram/BU2/U0

   /blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM36.

   noeccerr.SDP

   of frag RDRCLKU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/Comp_FIFO/CompFIFO_64.dpram/BU2/U0

   /blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM36.

   noeccerr.SDP_RDRCLKU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/Comp_FIFO/CompFIFO_64.dpram/BU2/U0

   /blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM36.

   noeccerr.SDP

   of frag RDRCLKL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/Comp_FIFO/CompFIFO_64.dpram/BU2/U0

   /blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM36.

   noeccerr.SDP_RDRCLKL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/RxSFIFO_64.RxSFIFO/BU2/U0/grf.rf/m

   em/gbm.gbmg.gbmga.ngecc.bmg/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5.

   ram/SDP.WIDE_PRIM36.noeccerr.SDP

   of frag RDRCLKU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/RxSFIFO_64.RxSFIFO/BU2/U0/grf.rf/m

   em/gbm.gbmg.gbmga.ngecc.bmg/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5.

   ram/SDP.WIDE_PRIM36.noeccerr.SDP_RDRCLKU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/RxSFIFO_64.RxSFIFO/BU2/U0/grf.rf/m

   em/gbm.gbmg.gbmga.ngecc.bmg/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5.

   ram/SDP.WIDE_PRIM36.noeccerr.SDP

   of frag RDRCLKL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_master_bridge/RxSFIFO_64.RxSFIFO/BU2/U0/grf.rf/m

   em/gbm.gbmg.gbmga.ngecc.bmg/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5.

   ram/SDP.WIDE_PRIM36.noeccerr.SDP_RDRCLKL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/GEN_TX_64_FIFO.comp_tx_pkt_fifo/COM

   P_TX_RAM_70.dpram/BU2/U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noi

   nit.ram/SDP.WIDE_PRIM36.noeccerr.SDP

   of frag RDRCLKU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/GEN_TX_64_FIFO.comp_tx_pkt_fifo/COM

   P_TX_RAM_70.dpram/BU2/U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noi

   nit.ram/SDP.WIDE_PRIM36.noeccerr.SDP_RDRCLKU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/GEN_TX_64_FIFO.comp_tx_pkt_fifo/COM

   P_TX_RAM_70.dpram/BU2/U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noi

   nit.ram/SDP.WIDE_PRIM36.noeccerr.SDP

   of frag RDRCLKL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/GEN_TX_64_FIFO.comp_tx_pkt_fifo/COM

   P_TX_RAM_70.dpram/BU2/U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noi

   nit.ram/SDP.WIDE_PRIM36.noeccerr.SDP_RDRCLKL_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/comp_rx_fifo/GEN_64.COMP_RX_RAM/BU2

   /U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM

   36.noeccerr.SDP

   of frag RDRCLKU connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/comp_rx_fifo/GEN_64.COMP_RX_RAM/BU2

   /U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM

   36.noeccerr.SDP_RDRCLKU_tiesig

WARNING:Pack:2874 - Trimming timing constraints from pin

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/comp_rx_fifo/GEN_64.COMP_RX_RAM/BU2

   /U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM

   36.noeccerr.SDP

   of frag RDRCLKL connected to power/ground net

   PCIe_Bridge/PCIe_Bridge/comp_slave_bridge/comp_rx_fifo/GEN_64.COMP_RX_RAM/BU2

   /U0/blk_mem_generator/valid.cstr/ramloop[0].ram.r/v5_noinit.ram/SDP.WIDE_PRIM

   36.noeccerr.SDP_RDRCLKL_tiesig

Running directed packing...

Running delay-based LUT packing...

Updating timing models...

WARNING:Timing:3223 - Timing constraint TS_MC_RDEN_SEL_MUX = MAXDELAY FROM

   TIMEGRP "TNM_RDEN_SEL_MUX" TO TIMEGRP "TNM_CLK0" TS_MC_CLK * 4 ignored during

   timing analysis.

INFO:Map:215 - The Interim Design Summary has been generated in the MAP Report

   (.mrp).

Running timing-driven placement...

Total REAL time at the beginning of Placer: 2 mins 24 secs 

Total CPU  time at the beginning of Placer: 2 mins 19 secs 



Phase 1.1  Initial Placement Analysis

Phase 1.1  Initial Placement Analysis (Checksum:3a0b7697) REAL time: 2 mins 44 secs 



Phase 2.7  Design Feasibility Check

WARNING:Place:838 - An IO Bus with more than one IO standard is found.

   Components associated with this bus are as follows: 

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<7>   IOSTANDARD = LVCMOS25

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<6>   IOSTANDARD = LVCMOS25

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<5>   IOSTANDARD = LVCMOS25

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<4>   IOSTANDARD = LVCMOS18

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<3>   IOSTANDARD = LVCMOS25

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<2>   IOSTANDARD = LVCMOS18

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<1>   IOSTANDARD = LVCMOS18

   	 Comp: fpga_0_LEDs_8Bit_GPIO_IO_pin<0>   IOSTANDARD = LVCMOS18





WARNING:Place:838 - An IO Bus with more than one IO standard is found.

   Components associated with this bus are as follows: 

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<31>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<30>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<29>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<28>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<27>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<26>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<25>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<24>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<23>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<22>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<21>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<20>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<19>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<18>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<17>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<16>   IOSTANDARD = LVDCI_33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<15>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<14>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<13>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<12>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<11>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<10>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<9>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<8>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<7>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<6>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<5>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<4>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<3>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<2>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<1>   IOSTANDARD = LVCMOS33

   	 Comp: fpga_0_SRAM_Mem_DQ_pin<0>   IOSTANDARD = LVCMOS33





Phase 2.7  Design Feasibility Check (Checksum:3a0b7697) REAL time: 2 mins 45 secs 



Phase 3.31  Local Placement Optimization

Phase 3.31  Local Placement Optimization (Checksum:c9fd22c3) REAL time: 2 mins 45 secs 



Phase 4.37  Local Placement Optimization

Phase 4.37  Local Placement Optimization (Checksum:c9fd22c3) REAL time: 2 mins 45 secs 



Phase 5.33  Local Placement Optimization

Phase 5.33  Local Placement Optimization (Checksum:c9fd22c3) REAL time: 10 mins 47 secs 



Phase 6.32  Local Placement Optimization

Phase 6.32  Local Placement Optimization (Checksum:c9fd22c3) REAL time: 10 mins 52 secs 



Phase 7.2  Initial Clock and IO Placement







There are 16 clock regions on the target FPGA device:

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y7:                        | CLOCKREGION_X1Y7:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 0 in use      |   4 edge BUFIOs available, 0 in use      |

|   4 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y6:                        | CLOCKREGION_X1Y6:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 3 in use      |   4 edge BUFIOs available, 0 in use      |

|   0 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y5:                        | CLOCKREGION_X1Y5:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 0 in use      |   4 edge BUFIOs available, 0 in use      |

|   2 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y4:                        | CLOCKREGION_X1Y4:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 0 in use      |   4 edge BUFIOs available, 0 in use      |

|   2 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y3:                        | CLOCKREGION_X1Y3:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 0 in use      |   4 edge BUFIOs available, 0 in use      |

|   2 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y2:                        | CLOCKREGION_X1Y2:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 3 in use      |   4 edge BUFIOs available, 0 in use      |

|   2 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y1:                        | CLOCKREGION_X1Y1:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use
      |

|   4 edge BUFIOs available, 2 in use      |   4 edge BUFIOs available, 0 in use      |

|   0 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|

| CLOCKREGION_X0Y0:                        | CLOCKREGION_X1Y0:                        |

|   2 BUFRs available, 0 in use            |   2 BUFRs available, 0 in use            |

|   4 Regional Clock Spines, 0 in use      |   4 Regional Clock Spines, 0 in use      |

|   4 edge BUFIOs available, 0 in use      |   4 edge BUFIOs available, 0 in use      |

|   4 center BUFIOs available, 0 in use    |                                          |

|                                          |                                          |

|------------------------------------------|------------------------------------------|





Clock-Region: <CLOCKREGION_X0Y1>

  key resource utilizations (used/available): edge-bufios - 2/4; bufrs - 0/2; regional-clock-spines - 0/4

|-----------------------------------------------------------------------------------------------------------------------------------------------------------

|       |    clock    | BRAM |     |    |        |        |       |       |       |      |      |     |      |

|       |    region   | FIFO | DCM | GT | ILOGIC | OLOGIC |   FF  |  LUTM |  LUTL | MULT | EMAC | PPC | PCIe | <- (Types of Resources in Clock Region)

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       | Upper Region|  24  |  2  |  0 |   60   |   60   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the upper region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       |CurrentRegion|  24  |  4  |  0 |   40   |   40   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the current region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       | Lower Region|  24  |  0  |  0 |   80   |   80   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the lower region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| clock |    region   |                                                                                      -----------------------------------------------

|  type |  expansion  |                                                                                      | <IO/Regional clock Net Name>

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------





Clock-Region: <CLOCKREGION_X0Y2>

  key resource utilizations (used/available): edge-bufios - 3/4; center-bufios - 0/2; bufrs - 0/2; regional-clock-spines - 0/4

|-----------------------------------------------------------------------------------------------------------------------------------------------------------

|       |    clock    | BRAM |     |    |        |        |       |       |       |      |      |     |      |

|       |    region   | FIFO | DCM | GT | ILOGIC | OLOGIC |   FF  |  LUTM |  LUTL | MULT | EMAC | PPC | PCIe | <- (Types of Resources in Clock Region)

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       | Upper Region|   8  |  0  |  0 |   60   |   60   |  1280 |   640 |  1920 |   0  |   0  |  1  |   0  | <- Available resources in the upper region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       |CurrentRegion|  24  |  2  |  0 |   60   |   60   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the current region

|-------|-------------|------|-----|----|--------|-------
-|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       | Lower Region|  24  |  4  |  0 |   40   |   40   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the lower region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| clock |    region   |                                                                                      -----------------------------------------------

|  type |  expansion  |                                                                                      | <IO/Regional clock Net Name>

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------





Clock-Region: <CLOCKREGION_X0Y6>

  key resource utilizations (used/available): edge-bufios - 3/4; bufrs - 0/2; regional-clock-spines - 0/4

|-----------------------------------------------------------------------------------------------------------------------------------------------------------

|       |    clock    | BRAM |     |    |        |        |       |       |       |      |      |     |      |

|       |    region   | FIFO | DCM | GT | ILOGIC | OLOGIC |   FF  |  LUTM |  LUTL | MULT | EMAC | PPC | PCIe | <- (Types of Resources in Clock Region)

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       | Upper Region|  24  |  0  |  0 |   80   |   80   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the upper region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       |CurrentRegion|  24  |  4  |  0 |   40   |   40   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the current region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

|       | Lower Region|  24  |  2  |  0 |   60   |   60   |  3200 |  1600 |  4800 |   0  |   0  |  0  |   0  | <- Available resources in the lower region

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| clock |    region   |                                                                                      -----------------------------------------------

|  type |  expansion  |                                                                                      | <IO/Regional clock Net Name>

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 | 
    0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------

| BUFIO |             |   0  |  0  |  0 |    9   |    0   |     0 |     0 |     0 |   0  |   0  |  0  |   0  | "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>"

|-------|-------------|------|-----|----|--------|--------|-------|-------|-------|------|------|-----|------|----------------------------------------------









######################################################################################

# REGIONAL CLOCKING RESOURCE DISTRIBUTION UCF REPORT:

#

# Number of Regional Clocking Regions in the device: 16  (4 clock spines in each)

# Number of Regional Clock Networks used in this design: 8 (each network can be

# composed of up to 3 clock spines and cover up to 3 regional clock regions)

# 

######################################################################################



# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>" driven by "BUFIO_X0Y27"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[7].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y27" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<7>" RANGE =

CLOCKREGION_X0Y6;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>" driven by "BUFIO_X0Y9"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[0].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y9" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<0>" RANGE =

CLOCKREGION_X0Y2;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>" driven by "BUFIO_X0Y11"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[4].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y11" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<4>" RANGE =

CLOCKREGION_X0Y2;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>" driven by "BUFIO_X0Y4"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[1].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y4" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<1>" RANGE =

CLOCKREGION_X0Y1;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>" driven by "BUFIO_X0Y25"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[5].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y25" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<5>" RANGE =

CLOCKREGION_X0Y6;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>" driven by "BUFIO_X0Y7"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[2].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y7" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<2>" RANGE =

CLOCKREGION_X0Y1;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>" driven by "BUFIO_X0Y26"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[6].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y26" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<6>" RANGE =

CLOCKREGION_X0Y6;





# IO-Clock "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>" driven by "BUFIO_X0Y10"

INST "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_dqs[3].u_iob_dqs/u_bufio_dqs" LOC =

"BUFIO_X0Y10" ;

NET "DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>" TNM_NET =

"TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>" ;

TIMEGRP "TN_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>" AREA_GROUP =

"CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>" ;

AREA_GROUP "CLKAG_DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/delayed_dqs<3>" RANGE =

CLOCKREGION_X0Y2;





Phase 7.2  Initial Clock and IO Placement (Checksum:b5943100) REAL time: 11 mins 10 secs 



Phase 8.36  Local Placement Optimization

Phase 8.36  Local Placement Optimization (Checksum:b5943100) REAL time: 11 mins 10 secs 



.........
..............
.......

....
......
......
......
......
......
.......
.......
......
........
......
........
.......
........
........
......

Phase 9.30  Global Clock Region Assignment





######################################################################################

# GLOBAL CLOCK NET DISTRIBUTION UCF REPORT:

#

# Number of Global Clock Regions : 16

# Number of Global Clock Networks: 15

#

# Clock Region Assignment: SUCCESSFUL



# Location of Clock Components

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/Using_BUFG_for_CLKOUT1.CLKOUT1_BUFG_INST" LOC = "BUFGCTRL_X0Y1" ;

INST "fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP/BUFG" LOC = "BUFGCTRL_X0Y30" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/use_pll.gtxclk_pll_bufg" LOC = "BUFGCTRL_X0Y29" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/use_pll.coreclk_pll_bufg" LOC = "BUFGCTRL_X0Y27" ;

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/Using_BUFG_for_CLKOUT2.CLKOUT2_BUFG_INST" LOC = "BUFGCTRL_X0Y2" ;

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_BUFG_for_CLKFBOUT.CLKFB_BUFG_INST" LOC = "BUFGCTRL_X0Y3" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/notsame.usrclk_pll_bufg" LOC = "BUFGCTRL_X0Y28" ;

INST "fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP/BUFG" LOC = "BUFGCTRL_X0Y8" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/use_pll.clkfbin_pll_bufg" LOC = "BUFGCTRL_X0Y26" ;

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/Using_BUFG_for_CLKOUT3.CLKOUT3_BUFG_INST" LOC = "BUFGCTRL_X0Y4" ;

INST "clock_generator_0/clock_generator_0/Using_DCM0.DCM0_INST/Using_BUFG_for_CLK0.CLK0_BUFG_INST" LOC = "BUFGCTRL_X0Y7" ;

INST "fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP/BUFG" LOC = "BUFGCTRL_X0Y31" ;

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/Using_BUFG_for_CLKOUT0.CLKOUT0_BUFG_INST" LOC = "BUFGCTRL_X0Y5" ;

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/Using_BUFG_for_CLKOUT4.CLKOUT4_BUFG_INST" LOC = "BUFGCTRL_X0Y6" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/SIO/.pcie_gt_wrapper_i/bufg2" LOC = "BUFGCTRL_X0Y0" ;

INST "clock_generator_0/clock_generator_0/Using_DCM0.DCM0_INST/DCM_INST/Using_DCM_ADV.DCM_ADV_INST" LOC = "DCM_ADV_X0Y0" ;

INST "fpga_0_SRAM_ZBT_CLK_FB_pin" LOC = "IOB_X1Y111" ;

INST "fpga_0_clk_1_sys_clk_pin" LOC = "IOB_X1Y109" ;

INST "fpga_0_Ethernet_MAC_PHY_rx_clk_pin" LOC = "IOB_X1Y219" ;

INST "fpga_0_Ethernet_MAC_PHY_tx_clk_pin" LOC = "IOB_X1Y217" ;

INST "fpga_0_SysACE_CompactFlash_SysACE_CLK_pin" LOC = "IOB_X1Y105" ;

INST "fpga_0_PCIe_Bridge_RXN_pin" LOC = "IPAD_X1Y12" ;

INST "fpga_0_PCIe_Bridge_RXP_pin" LOC = "IPAD_X1Y13" ;

INST "fpga_0_PCIe_Diff_Clk_IBUF_DS_N_pin" LOC = "IPAD_X1Y16" ;

INST "fpga_0_PCIe_Diff_Clk_IBUF_DS_P_pin" LOC = "IPAD_X1Y17" ;

INST "fpga_0_PCIe_Bridge_TXN_pin" LOC = "OPAD_X0Y8" ;

INST "fpga_0_PCIe_Bridge_TXP_pin" LOC = "OPAD_X0Y9" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/use_pll.pll_adv_i" LOC = "PLL_ADV_X0Y5" ;

INST "clock_generator_0/clock_generator_0/Using_PLL0.PLL0_INST/PLL_INST/Using_PLL_ADV.PLL_ADV_inst" LOC = "PLL_ADV_X0Y0" ;

INST "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/SIO/.pcie_gt_wrapper_i/GTD[0].GT_i" LOC = "GTX_DUAL_X0Y2" ;

INST "ibufgds_76" LOC = "BUFDS_X0Y2" ;



# clk_125_0000MHzPLL0 driven by BUFGCTRL_X0Y1

NET "clk_125_0000MHzPLL0" TNM_NET = "TN_clk_125_0000MHzPLL0" ;

TIMEGRP "TN_clk_125_0000MHzPLL0" AREA_GROUP = "CLKAG_clk_125_0000MHzPLL0" ;

AREA_GROUP "CLKAG_clk_125_0000MHzPLL0" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP driven by BUFGCTRL_X0Y30

NET "fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP" TNM_NET = "TN_fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP" ;

TIMEGRP "TN_fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP" AREA_GROUP = "CLKAG_fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP" ;

AREA_GROUP "CLKAG_fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk driven by BUFGCTRL_X0Y29

NET "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk" TNM_NET = "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk" ;

TIMEGRP "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk" AREA_GROUP = "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk" ;

AREA_GROUP "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5 ;



# PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk driven by BUFGCTRL_X0Y27

NET "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk" TNM_NET = "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk" ;

TIMEGRP "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk" AREA_GROUP = "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk" ;

AREA_GROUP "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# clk_125_0000MHzPLL0_ADJUST driven by BUFGCTRL_X0Y2

NET "clk_125_0000MHzPLL0_ADJUST" TNM_NET = "TN_clk_125_0000MHzPLL0_ADJUST" ;

TIMEGRP "TN_clk_125_0000MHzPLL0_ADJUST" AREA_GROUP = "CLKAG_clk_125_0000MHzPLL0_ADJUST" ;

AREA_GROUP "CLKAG_clk_125_0000MHzPLL0_ADJUST" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6> driven by BUFGCTRL_X0Y3

NET "clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6>" TNM_NET = "TN_clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6>" ;

TIMEGRP "TN_clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6>" AREA_GROUP = "CLKAG_clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6>" ;

AREA_GROUP "CLKAG_clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6>" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X0Y1, CLOCKREGION_X0Y2, CLOCKREGION_X0Y3 ;



# PCIe_Bridge/Bridge_Clk driven by BUFGCTRL_X0Y28

NET "PCIe_Bridge/Bridge_Clk" TNM_NET = "TN_PCIe_Bridge/Bridge_Clk" ;

TIMEGRP "TN_PCIe_Bridge/Bridge_Clk" AREA_GROUP = "CLKAG_PCIe_Bridge/Bridge_Clk" ;

AREA_GROUP "CLKAG_PCIe_Bridge/Bridge_Clk" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP driven by BUFGCTRL_X0Y8

NET "fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP" TNM_NET = "TN_fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP" ;

TIMEGRP "TN_fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP" AREA_GROUP = "CLKAG_fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP" ;

AREA_GROUP "CLKAG_fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP" RANGE =   CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5 ;



# PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin driven by BUFGCTRL_X0Y26

NET "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin" TNM_NET = "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin" ;

TIMEGRP "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin" AREA_GROUP = "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin" ;

AREA_GROUP "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin" RANGE =   CLOCKREGION_X0Y6, CLOCKREGION_X0Y7 ;



# clk_200_0000MHz driven by BUFGCTRL_X0Y4

NET "clk_200_0000MHz" TNM_NET = "TN_clk_200_0000MHz" ;

TIMEGRP "TN_clk_200_0000MHz" AREA_GROUP = "CLKAG_clk_200_0000MHz" ;

AREA_GROUP "CLKAG_clk_200_0000MHz" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# fpga_0_SRAM_ZBT_CLK_OUT_pin_OBUF driven by BUFGCTRL_X0Y7

NET "fpga_0_SRAM_ZBT_CLK_OUT_pin_OBUF" TNM_NET = "TN_fpga_0_SRAM_ZBT_CLK_OUT_pin_OBUF" ;

TIMEGRP "TN_fpga_0_SRAM_ZBT_CLK_OUT_pin_OBUF" AREA_GROUP = "CLKAG_fpga_0_SRAM_ZBT_CLK_OUT_pin_OBUF" ;

AREA_GROUP "CLKAG_fpga_0_SRAM_ZBT_CLK_OUT_pin_OBUF" RANGE =   CLOCKREGION_X1Y6, CLOCKREGION_X1Y7 ;



# fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP driven by BUFGCTRL_X0Y31

NET "fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP" TNM_NET = "TN_fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP" ;

TIMEGRP "TN_fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP" AREA_GROUP = "CLKAG_fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP" ;

AREA_GROUP "CLKAG_fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP" RANGE =   CLOCKREGION_X1Y0, CLOCKREGION_X1Y1, CLOCKREGION_X1Y2, CLOCKREGION_X1Y3, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5 ;



# clk_125_0000MHz90PLL0_ADJUST driven by BUFGCTRL_X0Y5

NET "clk_125_0000MHz90PLL0_ADJUST" TNM_NET = "TN_clk_125_0000MHz90PLL0_ADJUST" ;

TIMEGRP "TN_clk_125_0000MHz90PLL0_ADJUST" AREA_GROUP = "CLKAG_clk_125_0000MHz90PLL0_ADJUST" ;

AREA_GROUP "CLKAG_clk_125_0000MHz90PLL0_ADJUST" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# clk_62_5000MHzPLL0_ADJUST driven by BUFGCTRL_X0Y6

NET "clk_62_5000MHzPLL0_ADJUST" TNM_NET = "TN_clk_62_5000MHzPLL0_ADJUST" ;

TIMEGRP "TN_clk_62_5000MHzPLL0_ADJUST" AREA_GROUP = "CLKAG_clk_62_5000MHzPLL0_ADJUST" ;

AREA_GROUP "CLKAG_clk_62_5000MHzPLL0_ADJUST" RANGE =   CLOCKREGION_X0Y0, CLOCKREGION_X1Y0, CLOCKREGION_X0Y1, CLOCKREGION_X1Y1, CLOCKREGION_X0Y2, CLOCKREGION_X1Y2, CLOCKREGION_X0Y3, CLOCKREGION_X1Y3, CLOCKREGION_X0Y4, CLOCKREGION_X1Y4, CLOCKREGION_X0Y5, CLOCKREGION_X1Y5, CLOCKREGION_X0Y6, CLOCKREGION_X1Y6, CLOCKREGION_X0Y7, CLOCKREGION_X1Y7 ;



# PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg driven by BUFGCTRL_X0Y0

NET "PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg" TNM_NET = "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg" ;

TIMEGRP "TN_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg" AREA_GROUP = "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg" ;

AREA_GROUP "CLKAG_PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg" RANGE =   CLOCKREGION_X0Y6, CLOCKREGION_X0Y7 ;



# NOTE: 

# This report is provided to help reproduce successful clock-region 

# assignments. The report provides range constraints for all global 

# clock networks, in a format that is directly usable in ucf files. 

#

#END of Global Clock Net Distribution UCF Constraints

######################################################################################





######################################################################################

GLOBAL CLOCK NET LOADS DISTRIBUTION REPORT:



Number of Global Clock Regions : 16

Number of Global Clock Networks: 15



Clock Region Assignment: SUCCESSFUL



Clock-Region: <CLOCKREGION_X0Y0> 

 key resource utilizations (used/available): global-clocks - 2/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     12 |      0 |      0 |      0 |     80 |     80 |      0 |      0 |      0 |      0 |      2 |      0 |   1600 |   3200 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     38 |    676 |PCIe_Bridge/Bridge_Clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      2 |    329 |clk_125_0000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     40 |   1005 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y0> 

 key resource utilizations (used/available): global-clocks - 3/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |     40 |     40 |     16 |      0 |      0 |      1 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      4 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |      0 |      0 |     55 |   1130 |PCIe_Bridge/Bridge_Clk

      4 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |      0 |      0 |     24 |     52 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     29 |clk_125_0000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      2 |      0 |      0 |     79 |   1211 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y1> 

 key resource utilizations (used/available): global-clocks - 6/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     12 |      4 |      2 |      0 |     40 |     40 |      0 |      0 |      0 |      0 |      1 |      0 |   1600 |   3200 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      2 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     18 |    164 |PCIe_Bridge/Bridge_Clk

      0 |      0 |      0 |      0 |      0 |     18 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |clk_125_0000MHz90PLL0_ADJUST

      2 |      1 |      0 |      0 |      0 |     17 |      0 |      0 |      0 |      0 |      0 |      0 |     33 |    942 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |      0 |      0 |      0 |clk_200_0000MHz

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      3 |clk_62_5000MHzPLL0_ADJUST

      0 |      0 |      1 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |clock_generator_0/clock_generator_0/PLL0_CLK_OUT<6>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      4 |      1 |      1 |      0 |      0 |     35 |      0 |      0 |      0 |      0 |      1 |      0 |     51 |   1110 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y1> 

 key resource utilizations (used/available): global-clocks - 4/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |     40 |     40 |     16 |      0 |      0 |      0 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    104 |    750 |PCIe_Bridge/Bridge_Clk

      1 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     15 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    312 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      5 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      1 |      0 |      0 |      0 |      0 |      5 |      0 |      0 |      0 |      0 |      0 |      0 |    104 |   1077 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y2> 

 key resource utilizations (used/available): global-clocks - 5/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     12 |      2 |      1 |      0 |     60 |     60 |      0 |      0 |      0 |      0 |      2 |      0 |   1600 |   3200 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      6 |      4 |PCIe_Bridge/Bridge_Clk

      0 |      0 |      0 |      0 |      0 |     27 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     20 |clk_125_0000MHz90PLL0_ADJUST

      3 |      0 |      0 |      0 |      9 |     15 |      0 |      0 |      0 |      0 |      0 |      0 |     41 |   1074 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |      0 |      0 |      0 |clk_200_0000MHz

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    109 |clk_62_5000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      3 |      0 |      0 |      0 |      9 |     42 |      0 |      0 |      0 |      0 |      1 |      0 |     47 |   1207 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y2> 

 key resource utilizations (used/available): global-clocks - 4/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |     40 |     40 |     16 |      0 |      0 |      1 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      1 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    150 |    685 |PCIe_Bridge/Bridge_Clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     59 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      2 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/gt_usrclk

      0 |      0 |      0 |      0 |      0 |      5 |      0 |      0 |      0 |      0 |      0 |      0 |     28 |    407 |clk_125_0000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      1 |      0 |      0 |      0 |      0 |      5 |      0 |      0 |      0 |      0 |      0 |      0 |    178 |   1153 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y3> 

 key resource utilizations (used/available): global-clocks - 4/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      4 |      0 |      0 |      0 |     60 |     60 |      0 |      0 |      1 |      0 |      2 |     16 |    640 |   1280 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     79 |clk_125_0000MHz90PLL0_ADJUST

      0 |      0 |      0 |      0 |      8 |     17 |      0 |      0 |      1 |      0 |      0 |      0 |     20 |    286 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      3 |clk_200_0000MHz

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     79 |clk_62_5000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      8 |     17 |      0 |      0 |      1 |      0 |      0 |      0 |     20 |    447 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y3> 

 key resource utilizations (used/available): global-clocks - 3/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |     40 |     40 |     16 |      0 |      0 |      0 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      2 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    126 |PCIe_Bridge/Bridge_Clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     27 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/core_clk

      6 |      0 |      0 |      0 |      0 |      0 |     13 |      0 |      0 |      0 |      0 |      0 |    116 |    933 |clk_125_0000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |      0 |      0 |     13 |      0 |      0 |      0 |      0 |      0 |    116 |   1086 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y4> 

 key resource utilizations (used/available): global-clocks - 4/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      4 |      0 |      0 |      0 |     60 |     60 |      0 |      0 |      1 |      0 |      2 |     16 |    640 |   1280 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      2 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     33 |clk_125_0000MHz90PLL0_ADJUST

      4 |      0 |      0 |      0 |      1 |     20 |      0 |      0 |      0 |      0 |      0 |      0 |     51 |    262 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     34 |clk_62_5000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      6 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      6 |      0 |      0 |      0 |      7 |     20 |      0 |      0 |      0 |      0 |      0 |      0 |     51 |    329 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y4> 

 key resource utilizations (used/available): global-clocks - 3/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     10 |      0 |      0 |      0 |     40 |     40 |     16 |      1 |      0 |      0 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     20 |PCIe_Bridge/Bridge_Clk

      3 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     76 |   1046 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |     16 |     26 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     23 |fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      3 |      0 |      0 |      0 |     16 |     26 |      0 |      0 |      0 |      0 |      0 |      0 |     76 |   1089 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y5> 

 key resource utilizations (used/available): global-clocks - 3/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     12 |      2 |      1 |      0 |     60 |     60 |      0 |      0 |      0 |      0 |      2 |      0 |   1600 |   3200 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     49 |clk_125_0000MHz90PLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |     27 |      0 |      0 |      0 |      0 |      0 |      0 |     72 |    601 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     99 |clk_62_5000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |     27 |      0 |      0 |      0 |      0 |      0 |      0 |     72 |    749 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y5> 

 key resource utilizations (used/available): global-clocks - 4/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     10 |      0 |      0 |      0 |     40 |     40 |     16 |      1 |      0 |      0 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     28 |PCIe_Bridge/Bridge_Clk

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    126 |    746 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |fpga_0_Ethernet_MAC_PHY_tx_clk_pin_BUFGP

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     14 |fpga_0_SysACE_CompactFlash_SysACE_CLK_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    126 |    789 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y6> 

 key resource utilizations (used/available): global-clocks - 7/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     12 |      4 |      2 |      0 |     40 |     40 |      0 |      0 |      0 |      0 |      1 |      0 |   1600 |   3200 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      1 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/REFCLKOUT_bufg

      0 |      0 |      1 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/clocking_i/clkfbin

      0 |      0 |      0 |      0 |      0 |     27 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      2 |clk_125_0000MHz90PLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      8 |      0 |      0 |      0 |      0 |      0 |      0 |     91 |    751 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |      0 |      0 |      0 |clk_200_0000MHz

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    249 |clk_62_5000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     15 |      8 |fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      2 |      0 |      0 |     35 |      0 |      0 |      0 |      0 |      1 |      0 |    106 |   1010 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y6> 

 key resource utilizations (used/available): global-clocks - 2/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |     40 |     40 |     16 |      0 |      0 |      1 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |     19 |     23 |      0 |      0 |      0 |      0 |      0 |      0 |     97 |    796 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      4 |fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |     19 |     23 |      0 |      0 |      0 |      0 |      0 |      0 |     97 |    800 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X0Y7> 

 key resource utilizations (used/available): global-clocks - 3/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

     12 |      0 |      0 |      0 |     80 |     80 |      0 |      0 |      0 |      0 |      2 |      0 |   1600 |   3200 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    106 |    471 |clk_125_0000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |     10 |    310 |clk_62_5000MHzPLL0_ADJUST

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      1 |fpga_0_Ethernet_MAC_PHY_rx_clk_pin_BUFGP

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    116 |    782 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------





Clock-Region: <CLOCKREGION_X1Y7> 

 key resource utilizations (used/available): global-clocks - 1/10 ;

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

   BRAM |    DCM |    PLL |     GT | ILOGIC | OLOGIC |   MULT |  TEMAC |    PPC |   PCIE | IDLYCT | BUFGCT |    LUT |     FF | <- (Types of Resources in this  Region)

   FIFO |        |        |        |        |        |        |        |        |        |        |        |        |        |

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      8 |      0 |      0 |      0 |     40 |     40 |     16 |      0 |      0 |      0 |      1 |      0 |   1920 |   2880 | <- (Available Resources in this Region)

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

        |        |        |        |        |        |        |        |        |        |        |        |        |        | <Global clock Net Name>

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    146 |    674 |clk_125_0000MHzPLL0_ADJUST

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------

      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |      0 |    146 |    674 | Total 

--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+--------+----------------------------------------



NOTE:

The above detailed report is the initial placement of the logic after the clock region assignment. The final placement

may be significantly different because of the various optimization steps which will follow. Specifically, logic blocks

maybe moved to adjacent clock-regions as long as the "number of clocks per region" constraint is not violated.





# END of Global Clock Net Loads Distribution Report:

######################################################################################





Phase 9.30  Global Clock Region Assignment (Checksum:b5943100) REAL time: 12 mins 45 secs 



Phase 10.3  Local Placement Optimization

Phase 10.3  Local Placement Optimization (Checksum:b5943100) REAL time: 12 mins 46 secs 



Phase 11.5  Local Placement Optimization

Phase 11.5  Local Placement Optimization (Checksum:b5943100) REAL time: 12 mins 47 secs 



Phase 12.8  Global Placement

..
...........
...........
.........

......
....
.....
.....
.....
.....
.....
.....
....
.....
.....
.....
....
......
.....
......
.......
......
.......
.......
.......
........
...

.
.....
.....
.....
.....
......
......
......
......
......
.....

.....
....
.....
....
....
....
....
...
...
....
...
...
..
.
...
...
...
..
...
.
.
...
..
...
..
...
...
...
....
...
....
...
.
...
...
...
..
....
..
...
..
...
....

.
.
.
..
...
.
..
..
...
...
...
.
...
...
..
...
...
...
...
.

.
.
..
...
..
.
....
....
....
.
..
.....

.
...
....
...
.......
.....

.
....
....
....
.....
......
.....
....
....
....
....

Phase 12.8  Global Placement (Checksum:64c223c7) REAL time: 20 mins 44 secs 



Phase 13.29  Local Placement Optimization

Phase 13.29  Local Placement Optimization (Checksum:64c223c7) REAL time: 20 mins 44 secs 



Phase 14.5  Local Placement Optimization

Phase 14.5  Local Placement Optimization (Checksum:64c223c7) REAL time: 20 mins 49 secs 



Phase 15.18  Placement Optimization

Phase 15.18  Placement Optimization (Checksum:d0a37aa3) REAL time: 23 mins 25 secs 



Phase 16.5  Local Placement Optimization

Phase 16.5  Local Placement Optimization (Checksum:d0a37aa3) REAL time: 23 mins 28 secs 



Phase 17.34  Placement Validation

Phase 17.34  Placement Validation (Checksum:d0a37aa3) REAL time: 23 mins 30 secs 



Total REAL time to Placer completion: 23 mins 34 secs 

Total CPU  time to Placer completion: 22 mins 30 secs 

Running post-placement packing...

Writing output files...



Design Summary:

Number of errors:      0

Number of warnings:   52

Slice Logic Utilization:

  Number of Slice Registers:                14,755 out of  44,800   32%

    Number used as Flip Flops:              14,754

    Number used as Latches:                      1

  Number of Slice LUTs:                     16,419 out of  44,800   36%

    Number used as logic:                   15,565 out of  44,800   34%

      Number using O6 output only:          14,103

      Number using O5 output only:             371

      Number using O5 and O6:                1,091

    Number used as Memory:                     724 out of  13,120    5%

      Number used as Dual Port RAM:            228

        Number using O6 output only:            12

        Number using O5 output only:            32

        Number using O5 and O6:                184

      Number used as Single Port RAM:            4

        Number using O6 output only:             4

      Number used as Shift Register:           492

        Number using O6 output only:           492

    Number used as exclusive route-thru:       130

  Number of route-thrus:                       581

    Number using O6 output only:               490

    Number using O5 output only:                81

    Number using O5 and O6:                     10



Slice Logic Distribution:

  Number of occupied Slices:                 7,735 out of  11,200   69%

  Number of LUT Flip Flop pairs used:       21,404

    Number with an unused Flip Flop:         6,649 out of  21,404   31%

    Number with an unused LUT:               4,985 out of  21,404   23%

    Number of fully used LUT-FF pairs:       9,770 out of  21,404   45%

    Number of unique control sets:           1,397

    Number of slice register sites lost

      to control set restrictions:           3,281 out of  44,800    7%



  A LUT Flip Flop pair for this architecture represents one LUT paired with

  one Flip Flop within a slice.  A control set is a unique combination of

  clock, reset, set, and enable signals for a registered element.

  The Slice Logic Distribution report is not meaningful if the design is

  over-mapped for a non-slice resource or if Placement fails.

  OVERMAPPING of BRAM resources should be ignored if the design is

  over-mapped for a non-BRAM resource or if placement fails.



IO Utilization:

  Number of bonded IOBs:                       255 out of     640   39%

    Number of LOCed IOBs:                      255 out of     255  100%

    IOB Flip Flops:                            494

    Number of bonded IPADs:                      4 out of      50    8%

    Number of bonded OPADs:                      2 out of      32    6%



Specific Feature Utilization:

  Number of BlockRAM/FIFO:                      22 out of     148   14%

    Number using BlockRAM only:                 20

    Number using FIFO only:                      2

    Total primitives used:

      Number of 36k BlockRAM used:              16

      Number of 18k BlockRAM used:               6

      Number of 36k FIFO used:                   2

    Total Memory used (KB):                    756 out of   5,328   14%

  Number of BUFG/BUFGCTRLs:                     15 out of      32   46%

    Number used as BUFGs:                       15

  Number of IDELAYCTRLs:                         3 out of      22   13%

  Number of BUFDSs:                              1 out of       8   12%

  Number of BUFIOs:                              8 out of      80   10%

  Number of DCM_ADVs:                            1 out of      12    8%

  Number of DSP48Es:                            13 out of     128   10%

  Number of GTX_DUALs:                           1 out of       8   12%

  Number of PCIEs:                               1 out of       3   33%

    Number of LOCed PCIEs:                       1 out of       1  100%

  Number of PLL_ADVs:                            2 out of       6   33%

  Number of PPC440s:                             1 out of       1  100%



  Number of RPM macros:           64

Average Fanout of Non-Clock Nets:                3.80



Peak Memory Usage:  888 MB

Total REAL time to MAP completion:  24 mins 23 secs 

Total CPU time to MAP completion:   23 mins 18 secs 



Mapping completed.

See MAP report file "system_map.mrp" for details.







#----------------------------------------------#

# Starting program par

# par -ise ../__xps/ise/system.ise -w -ol high system_map.ncd system.ncd

system.pcf 

#----------------------------------------------#

Release 11.2 - par L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

PMSPEC -- Overriding Xilinx file <C:/devtools/Xilinx/11.1/EDK/data/parBmgr.acd> with local file

<c:/devtools/Xilinx/11.1/ISE/data/parBmgr.acd>





Loading device for application Rf_Device from file '5vfx70t.nph' in environment

c:\devtools\Xilinx\11.1\ISE;C:\devtools\Xilinx\11.1\EDK.

   "system" is an NCD, version 3.2, device xc5vfx70t, package ff1136, speed -1



Constraints file: system.pcf.

   "system" is an NCD, version 3.2, device xc5vfx70t, package ff1136, speed -1

WARNING:ConstraintSystem:65 - Constraint <NET "PCIe_Bridge/Bridge_Clk" PERIOD = 8 ns HIGH 50%;> [system.pcf(90242)]

   overrides constraint <NET "PCIe_Bridge/Bridge_Clk" PERIOD = 8 ns HIGH 50%;> [system.pcf(90241)].





Initializing temperature to 85.000 Celsius. (default - Range: 0.000 to 85.000 Celsius)

Initializing voltage to 0.950 Volts. (default - Range: 0.950 to 1.050 Volts)



WARNING:Timing:3223 - Timing constraint TS_MC_RDEN_SEL_MUX = MAXDELAY FROM TIMEGRP "TNM_RDEN_SEL_MUX" TO TIMEGRP       

   "TNM_CLK0" TS_MC_CLK * 4; ignored during timing analysis.

INFO:Timing:3386 - Intersecting Constraints found and resolved.  For more information, see the TSI report.  Please

   consult the Xilinx Command Line Tools User Guide for information on generating a TSI report.



Device speed data version:  "PRODUCTION 1.65 2009-06-01".







Device Utilization Summary:



   Number of BUFDSs                          1 out of 8      12%

   Number of BUFGs                          15 out of 32     46%

   Number of BUFIOs                          8 out of 80     10%

   Number of DCM_ADVs                        1 out of 12      8%

   Number of DSP48Es                        13 out of 128    10%

   Number of FIFO36_72_EXPs                  2 out of 148     1%

      Number of LOCed FIFO36_72_EXPs         2 out of 2     100%



   Number of GTX_DUALs                       1 out of 8      12%

   Number of IDELAYCTRLs                     3 out of 22     13%

      Number of LOCed IDELAYCTRLs            3 out of 3     100%



   Number of ILOGICs                       131 out of 800    16%

      Number of LOCed ILOGICs                8 out of 131     6%



   Number of External IOBs                 255 out of 640    39%

      Number of LOCed IOBs                 255 out of 255   100%



   Number of IODELAYs                       80 out of 800    10%

      Number of LOCed IODELAYs               8 out of 80     10%



   Number of External IPADs                  4 out of 690     1%

      Number of LOCed IPADs                  4 out of 4     100%



   Number of JTAGPPCs                        1 out of 1     100%

   Number of OLOGICs                       236 out of 800    29%

   Number of External OPADs                  2 out of 32      6%

      Number of LOCed OPADs                  2 out of 2     100%



   Number of PCIEs                           1 out of 3      33%

      Number of LOCed PCIEs                  1 out of 1     100%



   Number of PLL_ADVs                        2 out of 6      33%

   Number of PPC440s                         1 out of 1     100%

   Number of RAMB18X2SDPs                    4 out of 148     2%

   Number of RAMB36SDP_EXPs                  6 out of 148     4%

      Number of LOCed RAMB36SDP_EXPs         1 out of 6      16%



   Number of RAMB36_EXPs                    10 out of 148     6%

      Number of LOCed RAMB36_EXPs            6 out of 10     60%



   Number of Slice Registers             14755 out of 44800  32%

      Number used as Flip Flops          14754

      Number used as Latches                 1

      Number used as LatchThrus              0



   Number of Slice LUTS                  16419 out of 44800  36%

   Number of Slice LUT-Flip Flop pairs   21404 out of 44800  47%





Overall effort level (-ol):   High 

Router effort level (-rl):    High 



Starting initial Timing Analysis.  REAL time: 1 mins 25 secs 

Finished initial Timing Analysis.  REAL time: 1 mins 27 secs 



WARNING:Par:288 - The signal PCIe_Bridge/PCIe_Bridge/sig_sb_txrem_n<0> has no load.  PAR will not attempt to route this

   signal.

WARNING:Par:288 - The signal PCIe_Bridge/PCIe_Bridge/sig_MB_TxREMn<0> has no load.  PAR will not attempt to route this

   signal.

WARNING:Par:288 - The signal xps_bram_if_cntlr_1_port_BRAM_Addr<31> has no load.  PAR will not attempt to route this

   signal.

WARNING:Par:288 - The signal xps_bram_if_cntlr_1_port_BRAM_Addr<30> has no load.  PAR will not attempt to route this

   signal.

WARNING:Par:288 - The signal PCIe_Bridge/PCIe_Bridge/sig_MB_RxFull has no load.  PAR will not attempt to route this

   signal.

Starting Router



INFO:Route:501 - One or more directed routing (DIRT) constraints generated for a specific device have been found. Note

   that DIRT strings are guaranteed to work only on the same device they were created for. If the DIRT constraints fail,

   verify that the same connectivity is available in the target device for this implementation. 



Phase  1  : 106522 unrouted;      REAL time: 1 mins 45 secs 



Phase  2  : 93293 unrouted;      REAL time: 2 mins 



Phase  3  : 39046 unrouted;      REAL time: 4 mins 11 secs 



Phase  4  : 39025 unrouted; (Setup:0, Hold:89741, Component Switching Limit:0)     REAL time: 4 mins 40 secs 



Updating file: system.ncd with current fully routed design.



Phase  5  : 0 unrouted; (Setup:0, Hold:90756, Component Switching Limit:0)     REAL time: 6 mins 33 secs 



Phase  6  : 0 unrouted; (Setup:0, Hold:90756, Component Switching Limit:0)     REAL time: 6 mins 33 secs 



Phase  7  : 0 unrouted; (Setup:0, Hold:90756, Component Switching Limit:0)     REAL time: 6 mins 33 secs 



Phase  8  : 0 unrouted; (Setup:0, Hold:90756, Component Switching Limit:0)     REAL time: 6 mins 33 secs 



Phase  9  : 0 unrouted; (Setup:0, Hold:0, Component Switching Limit:0)     REAL time: 8 mins 30 secs 



Phase 10  : 0 unrouted; (Setup:0, Hold:0, Component Switching Limit:0)     REAL time: 9 mins 7 secs 

Total REAL time to Router completion: 9 mins 7 secs 

Total CPU time to Router completion: 8 mins 54 secs 



Partition Implementation Status

-------------------------------



  No Partitions were found in this design.



-------------------------------



Generating "PAR" statistics.



**************************

Generating Clock Report

**************************



+---------------------+--------------+------+------+------------+-------------+

|        Clock Net    |   Resource   |Locked|Fanout|Net Skew(ns)|Max Delay(ns)|

+---------------------+--------------+------+------+------------+-------------+

|clk_125_0000MHzPLL0_ |              |      |      |            |             |

|              ADJUST | BUFGCTRL_X0Y2| No   | 4263 |  0.532     |  2.076      |

+---------------------+--------------+------+------+------------+-------------+

|PCIe_Bridge/Bridge_C |              |      |      |            |             |

|                  lk |BUFGCTRL_X0Y28| No   | 1472 |  0.444     |  2.085      |

+---------------------+--------------+------+------+------------+-------------+

|clk_62_5000MHzPLL0_A |              |      |      |            |             |

|               DJUST | BUFGCTRL_X0Y6| No   |  490 |  0.318     |  2.057      |

+---------------------+--------------+------+------+------------+-------------+

|clk_125_0000MHz90PLL |              |      |      |            |             |

|            0_ADJUST | BUFGCTRL_X0Y5| No   |  162 |  0.254     |  2.028      |

+---------------------+--------------+------+------+------------+-------------+

|fpga_0_SysACE_Compac |              |      |      |            |             |

|tFlash_SysACE_CLK_pi |              |      |      |            |             |

|             n_BUFGP | BUFGCTRL_X0Y8| No   |   55 |  0.150     |  1.770      |

+---------------------+--------------+------+------+------------+-------------+

|PCIe_Bridge/PCIe_Bri |              |      |      |            |             |

|dge/comp_block_plus/ |              |      |      |            |             |

|comp_endpoint/core_c |              |      |      |            |             |

|                  lk |BUFGCTRL_X0Y27| No   |   94 |  0.260     |  2.085      |

+---------------------+--------------+------+------+------------+-------------+

|fpga_0_Ethernet_MAC_ |              |      |      |            |             |

|PHY_rx_clk_pin_BUFGP |              |      |      |            |             |

|                     |BUFGCTRL_X0Y30| No   |   12 |  0.093     |  1.934      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<0> |        IO Clk| No   |   18 |  0.095     |  0.419      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<1> |        IO Clk| No   |   18 |  0.083     |  0.380      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<2> |        IO Clk| No   |   18 |  0.101     |  0.425      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<3> |        IO Clk| No   |   18 |  0.107     |  0.404      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |
      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<5> |        IO Clk| No   |   18 |  0.101     |  0.425      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<4> |        IO Clk| No   |   18 |  0.101     |  0.425      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<6> |        IO Clk| No   |   18 |  0.096     |  0.393      |

+---------------------+--------------+------+------+------------+-------------+

|DDR2_SDRAM/DDR2_SDRA |              |      |      |            |             |

|M/u_ddr2_top/u_mem_i |              |      |      |            |             |

|f_top/u_phy_top/u_ph |              |      |      |            |             |

| y_io/delayed_dqs<7> |        IO Clk| No   |   18 |  0.101     |  0.425      |

+---------------------+--------------+------+------+------------+-------------+

|fpga_0_Ethernet_MAC_ |              |      |      |            |             |

|PHY_tx_clk_pin_BUFGP |              |      |      |            |             |

|                     |BUFGCTRL_X0Y31| No   |    6 |  0.004     |  1.941      |

+---------------------+--------------+------+------+------------+-------------+

| clk_125_0000MHzPLL0 | BUFGCTRL_X0Y1| No   |    2 |  0.000     |  1.739      |

+---------------------+--------------+------+------+------------+-------------+

|PCIe_Bridge/PCIe_Bri |              |      |      |            |             |

|dge/comp_block_plus/ |              |      |      |            |             |

|comp_endpoint/pcie_b |              |      |      |            |             |

|        lk/gt_usrclk |BUFGCTRL_X0Y29| No   |    6 |  0.096     |  1.916      |

+---------------------+--------------+------+------+------------+-------------+

|     clk_200_0000MHz | BUFGCTRL_X0Y4| No   |    4 |  0.128     |  1.879      |

+---------------------+--------------+------+------+------------+-------------+

|RS232_Uart_1_Interru |              |      |      |            |             |

|                  pt |         Local|      |    1 |  0.000     |  1.071      |

+---------------------+--------------+------+------+------------+-------------+

|Ethernet_MAC/Etherne |              |      |      |            |             |

|  t_MAC/phy_tx_clk_i |         Local|      |    9 |  2.410     |  3.454      |

+---------------------+--------------+------+------+------------+-------------+

|ppc440_0_jtagppc_bus |              |      |      |            |             |

|         _JTGC405TCK |         Local|      |    1 |  0.000     |  1.678      |

+---------------------+--------------+------+------+------------+-------------+

|PCIe_Bridge/PCIe_Bri |              |      |      |            |             |

|dge/comp_block_plus/ |              |      |      |            |             |

|comp_endpoint/pcie_b |              |      |      |            |             |

|lk/SIO/.pcie_gt_wrap |              |      |      |            |             |

|  per_i/icdrreset<0> |         Local|      |    1 |  0.000     |  0.590      |

+---------------------+--------------+------+------+------------+-------------+



* Net Skew is the difference between the minimum and maximum routing

only delays for the net. Note this is different from Clock Skew which

is reported in TRCE timing report. Clock Skew is the difference between

the minimum and maximum path delays which includes logic delays.



Timing Score: 0 (Setup: 0, Hold: 0, Component Switching Limit: 0)



Number of Timing Constraints that were not applied: 5



Asterisk (*) preceding a constraint indicates it was not met.

   This may be due to a setup or hold violation.



----------------------------------------------------------------------------------------------------------

  Constraint                                |    Check    | Worst Case |  Best Case | Timing |   Timing   

                                            |             |    Slack   | Achievable | Errors |    Score   

----------------------------------------------------------------------------------------------------------

  NET "PCIe_Bridge/Bridge_Clk" PERIOD = 8 n | SETUP       |     0.030ns|     7.970ns|       0|           0

  s HIGH 50%                                | HOLD        |     0.030ns|            |       0|           0

                                            | MINPERIOD   |     0.000ns|     8.000ns|       0|           0

------------------------------------------------------------------------------------------------------

  NET "PCIe_Bridge/PCIe_Bridge/comp_block_p | SETUP       |     0.075ns|     3.925ns|       0|           0

  lus/comp_endpoint/core_clk" PERIOD =      | HOLD        |     0.366ns|            |       0|           0

      4 ns HIGH 50%                         | MINPERIOD   |     0.000ns|     4.000ns|       0|           0

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.012ns|     0.838ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[2].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_DQ_CE = MAXDELAY FROM TIMEGRP "TNM_DQ_ | SETUP       |     0.021ns|     1.879ns|       0|           0

  CE_IDDR" TO TIMEGRP "TNM_DQS_FLOPS"       | HOLD        |     1.026ns|            |       0|           0

     1.9 ns                                 |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_clock_generator_0_clock_generator_0_PL | SETUP       |     0.026ns|     7.974ns|       0|           0

  L0_CLK_OUT_2_ = PERIOD TIMEGRP         "c | HOLD        |     0.079ns|            |       0|           0

  lock_generator_0_clock_generator_0_PLL0_C |             |            |            |        |            

  LK_OUT_2_" TS_sys_clk_pin *         1.25  |             |            |            |        |            

  HIGH 50%                                  |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.045ns|     0.805ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[0].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.045ns|     0.805ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[1].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.045ns|     0.805ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[5].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.047ns|     0.803ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[3].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.047ns|     0.803ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[4].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.047ns|     0.803ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[6].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.047ns|     0.803ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/gen_ |             |            |            |        |            

  dqs[7].u_iob_dqs/en_dqs_sync"         MAX |             |            |            |        |            

  DELAY = 0.85 ns                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.068ns|     0.532ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<0>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<1>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<2>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<3>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<4>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<5>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<6>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET         "DDR2_SDRAM/DDR2_SDRAM/u_ddr2 | MAXDELAY    |     0.071ns|     0.529ns|       0|           0

  _top/u_mem_if_top/u_phy_top/u_phy_io/en_d |             |            |            |        |            

  qs<7>"         MAXDELAY = 0.6 ns          |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_PLB_PCIe = MAXDELAY FROM TIMEGRP "SPLB | SETUP       |     0.449ns|     7.551ns|       0|           0

  _Clk" TO TIMEGRP "Bridge_Clk" 8 ns        | HOLD        |     0.456ns|            |       0|           0

    DATAPATHONLY                            |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_PCIe_PLB = MAXDELAY FROM TIMEGRP "Brid | SETUP       |     0.639ns|     7.361ns|       0|           0

  ge_Clk" TO TIMEGRP "SPLB_Clk" 8 ns        | HOLD        |     0.465ns|            |       0|           0

    DATAPATHONLY                            |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_MC_CLK = PERIOD TIMEGRP "mc_clk" 5 ns  | MINPERIOD   |     1.010ns|     3.990ns|       0|           0

  HIGH 50%                                  |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TSRXIN_Ethernet_MAC = MAXDELAY FROM TIMEG | MAXDELAY    |     1.640ns|     4.360ns|       0|           0

  RP "PADS" TO TIMEGRP         "RXCLK_GRP_E | HOLD        |     1.060ns|            |       0|           0

  thernet_MAC" 6 ns                         |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_clock_generator_0_clock_generator_0_PL | SETUP       |     2.000ns|     4.973ns|       0|           0

  L0_CLK_OUT_0_ = PERIOD TIMEGRP         "c | HOLD        |     0.476ns|            |       0|           0

  lock_generator_0_clock_generator_0_PLL0_C |             |            |            |        |            

  LK_OUT_0_" TS_sys_clk_pin *         1.25  |             |            |            |        |            

  PHASE 2 ns HIGH 50%                       |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_sys_clk_pin = PERIOD TIMEGRP "sys_clk_ | MINLOWPULSE |     6.000ns|     4.000ns|       0|           0

  pin" 100 MHz HIGH 50%                     |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_clock_generator_0_clock_generator_0_PL | SETUP       |     3.644ns|     1.356ns|       0|           0

  L0_CLK_OUT_3_ = PERIOD TIMEGRP         "c | HOLD        |     0.476ns|            |       0|           0

  lock_generator_0_clock_generator_0_PLL0_C |             |            |            |        |            

  LK_OUT_3_" TS_sys_clk_pin *         2 HIG |             |            |            |        |            

  H 50%                                     |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_clock_generator_0_clock_generator_0_PL | SETUP       |     4.149ns|     8.008ns|       0|           0

  L0_CLK_OUT_4_ = PERIOD TIMEGRP         "c | HOLD        |     0.172ns|            |       0|           0

  lock_generator_0_clock_generator_0_PLL0_C |             |            |            |        |            

  LK_OUT_4_" TS_sys_clk_pin *         0.625 |             |            |            |        |            

   HIGH 50%                                 |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET "fpga_0_Ethernet_MAC_PHY_tx_clk_pin_B | NETSKEW     |     4.422ns|     0.578ns|       0|           0

  UFGP" MAXSKEW = 5 ns                      |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET "fpga_0_Ethernet_MAC_PHY_rx_clk_pin_B | NETSKEW     |     4.778ns|     0.222ns|       0|           0

  UFGP" MAXSKEW = 5 ns                      |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_clock_generator_0_clock_generator_0_PL | MINPERIOD   |     4.900ns|     3.100ns|       0|           0

  L0_CLK_OUT_1_ = PERIOD TIMEGRP         "c |             |            |            |        |            

  lock_generator_0_clock_generator_0_PLL0_C |             |            |            |        |            

  LK_OUT_1_" TS_sys_clk_pin *         1.25  |             |            |            |        |            

  HIGH 50%                                  |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TSTXOUT_Ethernet_MAC = MAXDELAY FROM TIME | MAXDELAY    |     7.423ns|     2.577ns|       0|           0

  GRP "TXCLK_GRP_Ethernet_MAC" TO         T |             |            |            |        |            

  IMEGRP "PADS" 10 ns                       |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET "fpga_0_Ethernet_MAC_PHY_rx_clk_pin_B | SETUP       |     9.210ns|    13.685ns|       0|           0

  UFGP" PERIOD = 40 ns HIGH 14 ns           | HOLD        |     0.479ns|            |       0|           0

------------------------------------------------------------------------------------------------------

  TS_MC_PHY_INIT_DATA_SEL_90 = MAXDELAY FRO | SETUP       |    13.663ns|     6.337ns|       0|           0

  M TIMEGRP "TNM_PHY_INIT_DATA_SEL" TO      | HOLD        |     0.290ns|            |       0|           0

      TIMEGRP "TNM_CLK90" TS_MC_CLK * 4     |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_MC_PHY_INIT_DATA_SEL_0 = MAXDELAY FROM | SETUP       |    15.735ns|     4.265ns|       0|           0

   TIMEGRP "TNM_PHY_INIT_DATA_SEL" TO       | HOLD        |     0.915ns|            |       0|           0

     TIMEGRP "TNM_CLK0" TS_MC_CLK * 4       |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_MC_GATE_DLY = MAXDELAY FROM TIMEGRP "T | SETUP       |    17.698ns|     2.302ns|       0|           0

  NM_GATE_DLY" TO TIMEGRP "TNM_CLK0"        | HOLD        |     0.003ns|            |       0|           0

    TS_MC_CLK * 4                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_MC_CAL_RDEN_DLY = MAXDELAY FROM TIMEGR | SETUP       |    18.121ns|     1.879ns|       0|           0

  P "TNM_CAL_RDEN_DLY" TO TIMEGRP         " | HOLD        |     0.001ns|            |       0|           0

  TNM_CLK0" TS_MC_CLK * 4                   |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  TS_MC_RDEN_DLY = MAXDELAY FROM TIMEGRP "T | SETUP       |    18.132ns|     1.868ns|       0|           0

  NM_RDEN_DLY" TO TIMEGRP "TNM_CLK0"        | HOLD        |     0.023ns|            |       0|           0

    TS_MC_CLK * 4                           |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET "fpga_0_SysACE_CompactFlash_SysACE_CL | SETUP       |    26.579ns|     3.421ns|       0|           0

  K_pin_BUFGP/IBUFG" PERIOD = 30 ns         | HOLD        |     0.465ns|            |       0|           0

   HIGH 50%                                 |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET "fpga_0_Ethernet_MAC_PHY_tx_clk_pin_B | SETUP       |    32.855ns|     7.145ns|       0|           0

  UFGP" PERIOD = 40 ns HIGH 14 ns           | HOLD        |     0.357ns|            |       0|           0

------------------------------------------------------------------------------------------------------

  Pin to Pin Skew Constraint                | MAXDELAY    | 2106523.523ns| 2106523.837ns|       0|           0

------------------------------------------------------------------------------------------------------

  TS_MC_RDEN_SEL_MUX = MAXDELAY FROM TIMEGR | N/A         |         N/A|         N/A|     N/A|         N/A

  P "TNM_RDEN_SEL_MUX" TO TIMEGRP         " |             |            |            |        |            

  TNM_CLK0" TS_MC_CLK * 4                   |             |            |            |        |            

------------------------------------------------------------------------------------------------------

  NET "PCIe_Bridge/Bridge_Clk" PERIOD = 8 n | N/A         |         N/A|         N/A|     N/A|         N/A

  s HIGH 50%                                |             |            |            |        |            

------------------------------------------------------------------------------------------------------





Derived Constraint Report

Derived Constraints for TS_MC_CLK

+-------------------------------+-------------+-------------+-------------+-------------+-------------+-------------+-------------+

|                               |   Period    |       Actual Period       |      Timing Errors        |      Paths Analyzed       |

|           Constraint          | Requirement |-------------+-------------|-------------+-------------|-------------+-------------|

|                               |             |   Direct    | Derivative  |   Direct    | Derivative  |   Direct    | Derivative  |

+-------------------------------+-------------+-------------+-------------+-------------+-------------+-------------+-------------+

|TS_MC_CLK                      |      5.000ns|      3.990ns|      1.584ns|            0|            0|            0|          345|

| TS_MC_PHY_INIT_DATA_SEL_0     |     20.000ns|      4.265ns|          N/A|            0|            0|           21|            0|

| TS_MC_PHY_INIT_DATA_SEL_90    |     20.000ns|      6.337ns|          N/A|            0|            0|          274|            0|

| TS_MC_GATE_DLY                |     20.000ns|      2.302ns|          N/A|            0|            0|           40|            0|

| TS_MC_RDEN_DLY                |     20.000ns|      1.868ns|          N/A|            0|            0|            5|            0|

| TS_MC_CAL_RDEN_DLY            |     20.000ns|      1.879ns|          N/A|            0|            0|            5|            0|

| TS_MC_RDEN_SEL_MUX            |     20.000ns|          N/A|          N/A|            0|            0|            0|            0|

+-------------------------------+-------------+-------------+-------------+-------------+-------------+-------------+-------------+



Derived Constraints for TS_sys_clk_pin

+-------------------------------+-------------+-------------+-------------+-------------+-------------+-------------+-------------+

|                               |   Period    |       Actual Period       |      Timing Errors        |      Paths Analyzed       |

|           Constraint          | Requirement |-------------+-------------|-------------+-------------|-------------+-------------|

|                               |             |   Direct    | Derivative  |   Direct    | Derivative  |   Direct    | Derivative  |

+-------------------------------+-------------+-------------+-------------+-------------+-------------+-------------+-------------+

|TS_sys_clk_pin                 |     10.000ns|      4.000ns|      9.967ns|            0|            0|            0|      4043451|

| TS_clock_generator_0_clock_gen|      8.000ns|      4.973ns|          N/A|            0|            0|          626|            0|

| erator_0_PLL0_CLK_OUT_0_      |             |             |             |             |             |             |             |

| TS_clock_generator_0_clock_gen|      8.000ns|      3.100ns|          N/A|            0|            0|            0|            0|

| erator_0_PLL0_CLK_OUT_1_      |             |             |             |             |             |             |             |

| TS_clock_generator_0_clock_gen|      8.000ns|      7.974ns|          N/A|            0|            0|      4031781|            0|

| erator_0_PLL0_CLK_OUT_2_      |             |             |             |             |             |             |             |

| TS_clock_generator_0_clock_gen|      5.000ns|      1.356ns|          N/A|            0|            0|            2|            0|

| erator_0_PLL0_CLK_OUT_3_      |             |             |             |             |             |             |             |

| TS_clock_generator_0_clock_gen|     16.000ns|      8.008ns|          N/A|            0|            0|        11042|            0|

| erator_0_PLL0_CLK_OUT_4_      |             |             |             |             |             |             |             |

+-------------------------------+-------------+-------------+-------------+-------------+-------------+-------------+-------------+



All constraints were met.

INFO:Timing:2761 - N/A entries in the Constraints list may indicate that the 

   constraint does not cover any paths or that it has no requested value.





Generating Pad Report.



All signals are completely routed.



WARNING:Par:283 - There are 5 loadless signals in this design. This design will cause Bitgen to issue DRC warnings.



Loading device for application Rf_Device from file '5vlx50t.nph' in environment

c:\devtools\Xilinx\11.1\ISE;C:\devtools\Xilinx\11.1\EDK.

INFO:ParHelpers:197 - Number of "Exact" mode Directed Routing Constraints: 128

INFO:ParHelpers:199 - All "EXACT" mode Directed Routing constrained nets successfully routed. The number of constraints

   found: 128, number successful: 128

Total REAL time to PAR completion: 10 mins 4 secs 

Total CPU time to PAR completion: 9 mins 36 secs 



Peak Memory Usage:  754 MB



Placer: Placement generated during map.

Routing: Completed - No errors found.

Timing: Completed - No errors found.



Number of error messages: 0

Number of warning messages: 9

Number of info messages: 4



Writing design to file system.ncd







PAR done!







#----------------------------------------------#

# Starting program post_par_trce

# trce -ise ../__xps/ise/system.ise -e 3 -xml system.twx system.ncd system.pcf 

#----------------------------------------------#

Release 11.2 - Trace  (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.





PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<c:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>

Loading device for application Rf_Device from file '5vfx70t.nph' in environment

c:\devtools\Xilinx\11.1\ISE;C:\devtools\Xilinx\11.1\EDK.

   "system" is an NCD, version 3.2, device xc5vfx70t, package ff1136, speed -1

WARNING:ConstraintSystem:65 - Constraint <NET "PCIe_Bridge/Bridge_Clk" PERIOD =

   8 ns HIGH 50%;> [system.pcf(90242)] overrides constraint <NET

   "PCIe_Bridge/Bridge_Clk" PERIOD = 8 ns HIGH 50%;> [system.pcf(90241)].



WARNING:Timing:3223 - Timing constraint TS_MC_RDEN_SEL_MUX = MAXDELAY FROM

   TIMEGRP "TNM_RDEN_SEL_MUX" TO TIMEGRP        "TNM_CLK0" TS_MC_CLK * 4;

   ignored during timing analysis.

INFO:Timing:3386 - Intersecting Constraints found and resolved.  For more

   information, see the TSI report.  Please consult the Xilinx Command Line

   Tools User Guide for information on generating a TSI report.

--------------------------------------------------------------------------------

Release 11.2 Trace  (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.



trce -ise ../__xps/ise/system.ise -e 3 -xml system.twx system.ncd system.pcf





Design file:              system.ncd

Physical constraint file: system.pcf

Device,speed:             xc5vfx70t,-1 (PRODUCTION 1.65 2009-06-01, STEPPING

level 0)

Report level:             error report

--------------------------------------------------------------------------------



INFO:Timing:2752 - To get complete path coverage, use the unconstrained paths

   option. All paths that are not constrained will be reported in the

   unconstrained paths section(s) of the report.

INFO:Timing:3339 - The clock-to-out numbers in this timing report are based on a

   50 Ohm transmission line loading model.  For the details of this model, and

   for more information on accounting for different loading conditions, please

   see the device datasheet.





Timing summary:

---------------



Timing errors: 0  Score: 0 (Setup/Max: 0, Hold: 0)



Constraints cover 4233435 paths, 18 nets, and 96471 connections



Design statistics:

   Minimum period:  13.685ns (Maximum frequency:  73.073MHz)

   Maximum path delay from/to any node:   7.551ns

   Maximum net delay:   0.838ns

   Maximum net skew:   0.578ns





Analysis completed Tue Jun 30 23:01:07 2009

--------------------------------------------------------------------------------



Generating Report ...



Number of warnings: 2

Number of info messages: 3

Total time: 1 mins 41 secs 





xflow done!

touch __xps/system_routed
xilperl C:/devtools/Xilinx/11.1/EDK/data/fpga_impl/observe_par.pl -error yes implementation/system.par
Analyzing implementation/system.par

*********************************************
Running Bitgen..
*********************************************
cd implementation; bitgen -w -f bitgen.ut system; cd ..
Release 11.2 - Bitgen L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

PMSPEC -- Overriding Xilinx file

<C:/devtools/Xilinx/11.1/EDK/virtex5/data/virtex5.acd> with local file

<c:/devtools/Xilinx/11.1/ISE/virtex5/data/virtex5.acd>

Loading device for application Rf_Device from file '5vfx70t.nph' in environment

c:\devtools\Xilinx\11.1\ISE;C:\devtools\Xilinx\11.1\EDK.

   "system" is an NCD, version 3.2, device xc5vfx70t, package ff1136, speed -1

Opened constraints file system.pcf.



Tue Jun 30 23:01:40 2009



Running DRC.

WARNING:PhysDesignRules:1842 - One or more GTXs are being used in this design.

   Evaluate the SelectIO-To-GTX Crosstalk section of the Virtex-5 RocketIO GTX

   Transceiver User Guide to ensure that the design SelectIO usage meets the

   guidelines to minimize the impact on GTX performance. 

WARNING:PhysDesignRules:372 - Gated clock. Clock net

   Ethernet_MAC/Ethernet_MAC/phy_tx_clk_i is sourced by a combinatorial pin.

   This is not good design practice. Use the CE pin to control the loading of

   data into the flip-flop.

WARNING:PhysDesignRules:372 - Gated clock. Clock net

   PCIe_Bridge/PCIe_Bridge/comp_block_plus/comp_endpoint/pcie_blk/SIO/.pcie_gt_w

   rapper_i/icdrreset<0> is sourced by a combinatorial pin. This is not good

   design practice. Use the CE pin to control the loading of data into the

   flip-flop.

WARNING:PhysDesignRules:367 - The signal

   <PCIe_Bridge/PCIe_Bridge/sig_sb_txrem_n<0>> is incomplete. The signal does

   not drive any load pins in the design.

WARNING:PhysDesignRules:367 - The signal

   <PCIe_Bridge/PCIe_Bridge/sig_MB_TxREMn<0>> is incomplete. The signal does not

   drive any load pins in the design.

WARNING:PhysDesignRules:367 - The signal

   <xps_bram_if_cntlr_1_port_BRAM_Addr<31>> is incomplete. The signal does not

   drive any load pins in the design.

WARNING:PhysDesignRules:367 - The signal

   <xps_bram_if_cntlr_1_port_BRAM_Addr<30>> is incomplete. The signal does not

   drive any load pins in the design.

WARNING:PhysDesignRules:367 - The signal <PCIe_Bridge/PCIe_Bridge/sig_MB_RxFull>

   is incomplete. The signal does not drive any load pins in the design.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[1].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[1].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[4].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[4].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[7].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[7].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[2].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[2].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[5].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[5].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[0].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[0].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[3].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[3].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:1269 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[6].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The Q1 output pin of IFF is not

   used.

WARNING:PhysDesignRules:1273 - Dangling pins on

   block:<DDR2_SDRAM/DDR2_SDRAM/u_ddr2_top/u_mem_if_top/u_phy_top/u_phy_io/gen_d

   qs[6].u_iob_dqs/u_iddr_dq_ce>:<ILOGIC_IFF>.  The SR pin is used for the IFF

   Flip-flop but the SRVAL_Q1 set/reset value is not configured.

WARNING:PhysDesignRules:367 - The signal

   <ppc440_0_apu_fpu_virtex5/ppc440_0_apu_fpu_virtex5/gen_apu_fpu_dp_lo.netlist/

   fpu_is_full.sqrt_sqrt_flt_pt_op_sqrt_op.spd.op_exp_exp_sig_del_delay_55_2/Pro

   toComp7000.C6LUT.O6> is incomplete. The signal does not drive any load pins

   in the design.

WARNING:PhysDesignRules:367 - The signal

   <ppc440_0_apu_fpu_virtex5/ppc440_0_apu_fpu_virtex5/gen_apu_fpu_dp_lo.netlist/

   fpu_is_full.sqrt_sqrt_flt_pt_op_sqrt_op.spd.op_exp_exp_sig_del_delay_55_1/Pro

   toComp7000.C6LUT.O6> is incomplete. The signal does not drive any load pins

   in the design.

DRC detected 0 errors and 26 warnings.  Please see the previously displayed

individual error or warning messages for more details.

Creating bit map...

Saving bit stream in "system.bit".

Bitstream generation is complete.



Done!

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Wed Jul 01 10:06:56 2009
 make -f system.make download started...

cp -f /cygdrive/c/devtools/Xilinx/11.1/EDK/sw/lib/ppc440/ppc440_bootloop.elf bootloops/ppc440_0.elf
*********************************************
Initializing BRAM contents of the bitstream
*********************************************
bitinit -p xc5vfx70tff1136-1 system.mhs  -pe ppc440_0  bootloops/ppc440_0.elf  \
-bt implementation/system.bit -o implementation/download.bit


bitinit version Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) Xilinx Inc. 2002.



Parsing MHS File system.mhs...

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 298 - deprecated core for architecture 'virtex5fx'!



Overriding IP level properties ...



Performing IP level DRCs on properties...



Running DRC Tcl procedures for OPTION IPLEVEL_DRC_PROC...

Address Map for Processor ppc440_0

  (0b0000000000-0b0011111111) ppc440_0	

  (0000000000-0x0fffffff) DDR2_SDRAM	ppc440_0_PPC440MC

  (0x81000000-0x8100ffff) Ethernet_MAC	plb_v46_0

  (0x81400000-0x8140ffff) Push_Buttons_5Bit	plb_v46_0

  (0x81420000-0x8142ffff) LEDs_Positions	plb_v46_0

  (0x81440000-0x8144ffff) LEDs_8Bit	plb_v46_0

  (0x81460000-0x8146ffff) DIP_Switches_8Bit	plb_v46_0

  (0x81600000-0x8160ffff) IIC_EEPROM	plb_v46_0

  (0x81800000-0x8180ffff) xps_intc_0	plb_v46_0

  (0x83600000-0x8360ffff) SysACE_CompactFlash	plb_v46_0

  (0x84000000-0x8400ffff) RS232_Uart_1	plb_v46_0

  (0x85c00000-0x85c0ffff) PCIe_Bridge	plb_v46_0

  (0xc0000000-0xdfffffff) PCIe_Bridge	plb_v46_0

  (0xe0000000-0xefffffff) PCIe_Bridge	plb_v46_0

  (0xf8000000-0xf80fffff) SRAM	plb_v46_0

  (0xffffe000-0xffffffff) xps_bram_if_cntlr_1	plb_v46_0

INFO:EDK:1560 - IPNAME:ppc440_virtex5 INSTANCE:ppc440_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\ppc440_virtex5_v1_

   01_a\data\ppc440_virtex5_v2_1_0.mpd line 175 - tool is overriding PARAMETER

   C_SPLB0_P2P value to 0



Computing clock values...

INFO:EDK:1432 - Frequency for Top-Level Input Clock

   'fpga_0_PCIe_Diff_Clk_IBUF_DS_P_pin' is not specified. Clock DRCs will not be

   performed for IPs connected to that clock port, unless they are connected

   through the clock generator IP. 



INFO:EDK:1432 - Frequency for Top-Level Input Clock

   'fpga_0_PCIe_Diff_Clk_IBUF_DS_N_pin' is not specified. Clock DRCs will not be

   performed for IPs connected to that clock port, unless they are connected

   through the clock generator IP. 



INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 70 - tool is overriding PARAMETER

   C_PLBV46_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 71 - tool is overriding PARAMETER

   C_PLBV46_NUM_SLAVES value to 12

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 72 - tool is overriding PARAMETER

   C_PLBV46_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:plb_v46_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 74 - tool is overriding PARAMETER C_PLBV46_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_bram_if_cntlr INSTANCE:xps_bram_if_cntlr_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_bram_if_cntlr_

   v1_00_b\data\xps_bram_if_cntlr_v2_1_0.mpd line 75 - tool is overriding

   PARAMETER C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_bram_if_cntlr INSTANCE:xps_bram_if_cntlr_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_bram_if_cntlr_

   v1_00_b\data\xps_bram_if_cntlr_v2_1_0.mpd line 76 - tool is overriding

   PARAMETER C_SPLB_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:xps_bram_if_cntlr INSTANCE:xps_bram_if_cntlr_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_bram_if_cntlr_

   v1_00_b\data\xps_bram_if_cntlr_v2_1_0.mpd line 80 - tool is overriding

   PARAMETER C_SPLB_SMALLEST_MASTER value to 128

INFO:EDK:1560 - IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a

   \data\bram_block_v2_1_0.mpd line 69 - tool is overriding PARAMETER C_MEMSIZE

   value to 0x2000

INFO:EDK:1560 - IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a

   \data\bram_block_v2_1_0.mpd line 70 - tool is overriding PARAMETER

   C_PORT_DWIDTH value to 64

INFO:EDK:1560 - IPNAME:bram_block INSTANCE:xps_bram_if_cntlr_1_bram -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a

   \data\bram_block_v2_1_0.mpd line 72 - tool is overriding PARAMETER C_NUM_WE

   value to 8

INFO:EDK:1560 - IPNAME:xps_uartlite INSTANCE:RS232_Uart_1 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_uartlite_v1_01

   _a\data\xps_uartlite_v2_1_0.mpd line 73 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:LEDs_8Bit -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:LEDs_Positions -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:Push_Buttons_5Bit -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_gpio INSTANCE:DIP_Switches_8Bit -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_gpio_v2_00_a\d

   ata\xps_gpio_v2_1_0.mpd line 71 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_iic INSTANCE:IIC_EEPROM -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_iic_v2_01_a\da

   ta\xps_iic_v2_1_0.mpd line 79 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_mch_emc INSTANCE:SRAM -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_mch_emc_v3_00_

   a\data\xps_mch_emc_v2_1_0.mpd line 82 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_mch_emc INSTANCE:SRAM -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_mch_emc_v3_00_

   a\data\xps_mch_emc_v2_1_0.mpd line 84 - tool is overriding PARAMETER

   C_SPLB_SMALLEST_MASTER value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 86 - tool is overriding PARAMETER

   C_MPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 87 - tool is overriding PARAMETER

   C_MPLB_SMALLEST_SLAVE value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 89 - tool is overriding PARAMETER

   C_SPLB_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 90 - tool is overriding PARAMETER

   C_SPLB_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 91 - tool is overriding PARAMETER

   C_SPLB_SMALLEST_MASTER value to 128

INFO:EDK:1560 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plbv46_pcie_v3_00_

   b\data\plbv46_pcie_v2_1_0.mpd line 95 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 70 - tool is overriding PARAMETER

   C_PLBV46_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 71 - tool is overriding PARAMETER

   C_PLBV46_NUM_SLAVES value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 72 - tool is overriding PARAMETER

   C_PLBV46_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\plb_v46_v1_04_a\da

   ta\plb_v46_v2_1_0.mpd line 74 - tool is overriding PARAMETER C_PLBV46_DWIDTH

   value to 128

INFO:EDK:1560 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_ethernetlite_v

   2_01_a\data\xps_ethernetlite_v2_1_0.mpd line 75 - tool is overriding

   PARAMETER C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_sysace INSTANCE:SysACE_CompactFlash -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_sysace_v1_01_a

   \data\xps_sysace_v2_1_0.mpd line 72 - tool is overriding PARAMETER

   C_SPLB_DWIDTH value to 128

INFO:EDK:1560 - IPNAME:xps_sysace INSTANCE:SysACE_CompactFlash -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_sysace_v1_01_a

   \data\xps_sysace_v2_1_0.mpd line 74 - tool is overriding PARAMETER

   C_SPLB_MID_WIDTH value to 1

INFO:EDK:1560 - IPNAME:xps_sysace INSTANCE:SysACE_CompactFlash -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_sysace_v1_01_a

   \data\xps_sysace_v2_1_0.mpd line 75 - tool is overriding PARAMETER

   C_SPLB_NUM_MASTERS value to 1

INFO:EDK:1560 - IPNAME:xps_intc INSTANCE:xps_intc_0 -

   C:\devtools\Xilinx\11.1\EDK\hw\XilinxProcessorIPLib\pcores\xps_intc_v2_00_a\d

   ata\xps_intc_v2_1_0.mpd line 72 - tool is overriding PARAMETER C_SPLB_DWIDTH

   value to 128



Checking platform address map ...



Initializing Memory...

Running Data2Mem with the following command:

data2mem -bm "implementation/system_bd" -bt "implementation/system.bit"  -bd

"bootloops/ppc440_0.elf" tag ppc440_0  -o b implementation/download.bit 

Memory Initialization completed successfully.



*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

write (count, cmdBuffer, dataBuffer) failed C0000004.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2301.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

Downloading c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex.

Downloaded firmware version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      1 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

5: Device Temperature: Current Reading:   41.02 C, Min. Reading:   27.73 C, Max.

Reading:   41.02 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.502 V, Max.

Reading:   2.508 V

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

At Local date and time: Wed Jul 01 10:07:40 2009
 make -f system.make program started...

*********************************************
Creating software libraries...
*********************************************
libgen -mhs system.mhs -p xc5vfx70tff1136-1  -msg __xps/ise/xmsgprops.lst system.mss
libgen

Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.



Command Line: libgen -mhs system.mhs -p xc5vfx70tff1136-1 -msg

__xps/ise/xmsgprops.lst system.mss 



Release 11.2 - psf2Edward EDK_LS3.47 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 298 - deprecated core for architecture 'virtex5fx'!



Checking platform configuration ...

IPNAME:plb_v46 INSTANCE:plb_v46_0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 109 - 1 master(s) : 12 slave(s)

IPNAME:plb_v46 INSTANCE:ppc440_0_SPLB0 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 290 - 1 master(s) : 1 slave(s)

IPNAME:fcb_v20 INSTANCE:ppc440_0_fcb_v20 -

C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs

line 394 - 1 master(s) : 1 slave(s)



Checking port drivers...

WARNING:EDK:2099 - PORT:Peripheral_Reset CONNECTOR:sys_periph_reset -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   hs line 461 - floating connection!



Performing Clock DRCs...



Performing Reset DRCs...



Overriding system level properties...



Running system level update procedures...



Running UPDATE Tcl procedures for OPTION SYSLEVEL_UPDATE_PROC...



Running system level DRCs...



Performing System level DRCs on properties...



Running DRC Tcl procedures for OPTION SYSLEVEL_DRC_PROC...

WARNING:EDK:411 - pcie -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   ss line 77 - deprecated driver!

WARNING:EDK:411 - emaclite -

   C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.m

   ss line 83 - deprecated driver!

INFO:EDK:1740 - List of peripherals connected to processor instance ppc440_0: 

  - DDR2_SDRAM

  - DIP_Switches_8Bit

  - Ethernet_MAC

  - IIC_EEPROM

  - LEDs_8Bit

  - LEDs_Positions

  - PCIe_Bridge

  - Push_Buttons_5Bit

  - RS232_Uart_1

  - SRAM

  - SysACE_CompactFlash

  - ppc440_0_apu_fpu_virtex5

  - xps_bram_if_cntlr_1

  - xps_intc_0



-- Generating libraries for processor: ppc440_0 --





Staging source files.

Running DRCs.

Running generate.

Running post_generate.

Running include - 'make -s include "COMPILER=powerpc-eabi-gcc"

"ARCHIVER=powerpc-eabi-ar" "COMPILER_FLAGS=-mfpu=dp_full -mcpu=440  -O2 -c"

"EXTRA_COMPILER_FLAGS=-g"'.



Running libs - 'make -s libs "COMPILER=powerpc-eabi-gcc"

"ARCHIVER=powerpc-eabi-ar" "COMPILER_FLAGS=-mfpu=dp_full -mcpu=440  -O2 -c"

"EXTRA_COMPILER_FLAGS=-g"'.

Compiling common
powerpc-eabi-ar: creating ../../../lib/libxil.a

Compiling lldma
Compiling standalone
Compiling gpio
Compiling emaclite
Compiling iic
Compiling pci
Compiling uartlite
Compiling sysace
Compiling intc
Compiling cpu_ppc440
Running execs_generate.

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51202	    372	  87844	 139418	  2209a	RTOSDemo/executable.elf


Done!

At Local date and time: Wed Jul 01 11:26:01 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      1 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   33.15 C, Min. Reading:   30.69 C, Max.

Reading:   33.64 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.502 V, Max.

Reading:   2.508 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

Done.

Done.

Done.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

Done.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

Done.

Done.

Done.

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Wed Jul 01 17:11:24 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 150 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      3 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   42.99 C, Min. Reading:   34.13 C, Max.

Reading:   42.99 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.502 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     12 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.

----------------------------------------------------------------------

----------------------------------------------------------------------



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

At Local date and time: Wed Jul 01 17:17:34 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 150 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      0 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...
INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   62.68 C, Min. Reading:   62.68 C, Max.

Reading:   66.13 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.996 V, Max.

Reading:   0.999 V

5: VCCAUX Supply: Current Reading:   2.502 V, Min. Reading:   2.502 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

Done.

Done.

Done.

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

At Local date and time: Wed Jul 01 18:45:58 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      3 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   42.99 C, Min. Reading:   37.58 C, Max.

Reading:   42.99 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   0.999 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.502 V, Max.

Reading:   2.505 V

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Thu Jul 02 09:58:07 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51202	    372	  87844	 139418	  2209a	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 09:58:40 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

write (count, cmdBuffer, dataBuffer) failed C0000004.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2301.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

Downloading c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex.

Downloaded firmware version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...
INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      2 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   32.16 C, Min. Reading:   30.20 C, Max.

Reading:   32.66 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.505 V, Max.

Reading:   2.508 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

At Local date and time: Thu Jul 02 10:23:31 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50962	    372	  87844	 139178	  21faa	RTOSDemo/executable.elf


Done!

Done.

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

At Local date and time: Thu Jul 02 10:27:44 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      1 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   41.02 C, Min. Reading:   36.10 C, Max.

Reading:   41.02 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.502 V, Min. Reading:   2.502 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

At Local date and time: Thu Jul 02 11:09:53 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51014	    372	  87852	 139238	  21fe6	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 11:19:46 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50970	    372	  87852	 139194	  21fba	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 11:36:56 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50962	    372	  87844	 139178	  21faa	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 11:45:58 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51002	    372	  87852	 139226	  21fda	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 11:50:02 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51010	    372	  87860	 139242	  21fea	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 11:55:33 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51006	    372	  87860	 139238	  21fe6	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 13:28:01 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51250	    372	  87860	 139482	  220da	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 13:29:26 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51242	    372	  87852	 139466	  220ca	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 13:31:57 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      1 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   74.00 C, Min. Reading:   41.02 C, Max.

Reading:   74.49 C

5: VCCINT Supply: Current Reading:   0.993 V, Min. Reading:   0.993 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.496 V, Min. Reading:   2.493 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

At Local date and time: Thu Jul 02 13:35:43 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...
INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      1 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   73.02 C, Min. Reading:   70.06 C, Max.

Reading:   74.00 C

5: VCCINT Supply: Current Reading:   0.993 V, Min. Reading:   0.993 V, Max.

Reading:   0.999 V

5: VCCAUX Supply: Current Reading:   2.496 V, Min. Reading:   2.493 V, Max.

Reading:   2.502 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     12 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

At Local date and time: Thu Jul 02 13:38:54 2009
 make -f system.make program started...

make: Nothing to be done for `program'.


Done!

At Local date and time: Thu Jul 02 13:39:15 2009
 make -f system.make programclean started...

rm -f RTOSDemo/executable.elf 


Done!

At Local date and time: Thu Jul 02 13:39:21 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50774	    372	  87852	 138998	  21ef6	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 13:52:39 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50566	    372	  87852	 138790	  21e26	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 13:53:08 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50542	    372	  87860	 138774	  21e16	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 14:02:13 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50222	    372	  87860	 138454	  21cd6	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 14:20:50 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50298	    372	  87852	 138522	  21d1a	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 15:31:05 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c: In function 'vSecondaryBlockTimeTestTask':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c:426: error: 'tskTCB' has no member named 'xEventTaskList'

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1542: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1543: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGiveMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:348: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueTakeMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:394: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGenericReceive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:839: warning: assignment from incompatible pointer type

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:31:42 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c: In function 'vSecondaryBlockTimeTestTask':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c:426: error: 'tskTCB' has no member named 'xEventList'

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1542: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1543: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGiveMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:348: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueTakeMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:394: warning: comparison of distinct pointer types lacks a cast

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGenericReceive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:839: warning: assignment from incompatible pointer type

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:32:24 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1542: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1543: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGiveMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:348: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueTakeMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:394: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGenericReceive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:839: warning: assignment from incompatible pointer type

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51246	    372	  87844	 139462	  220c6	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 15:38:48 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1548: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1549: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskPlaceOnEventList':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1591: error: 'xSecondary' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1591: error: (Each undeclared identifier is reported only once
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1591: error: for each function it appears in.)

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGiveMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:348: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueTakeMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:394: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGenericReceive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:839: warning: assignment from incompatible pointer type

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:46:20 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1548: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1549: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskPlaceOnEventList':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1591: error: 'xSecondary' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1591: error: (Each undeclared identifier is reported only once
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1591: error: for each function it appears in.)

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGiveMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:348: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueTakeMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:394: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGenericReceive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:839: warning: assignment from incompatible pointer type

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:47:05 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1550: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1551: warning: passing argument 1 of 'vApplicationStackOverflowHook' from incompatible pointer type

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGiveMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:348: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueTakeMutexRecursive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:394: warning: comparison of distinct pointer types lacks a cast
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c: In function 'xQueueGenericReceive':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c:839: warning: assignment from incompatible pointer type

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51334	    372	  87852	 139558	  22126	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 15:48:10 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      0 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   69.08 C, Min. Reading:   66.62 C, Max.

Reading:   75.48 C

5: VCCINT Supply: Current Reading:   0.993 V, Min. Reading:   0.990 V, Max.

Reading:   0.999 V

5: VCCAUX Supply: Current Reading:   2.496 V, Min. Reading:   2.493 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

At Local date and time: Thu Jul 02 15:52:34 2009
 make -f system.make program started...

make: Nothing to be done for `program'.


Done!

At Local date and time: Thu Jul 02 15:54:04 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c: In function 'vSecondaryBlockTimeTestTask':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c:426: warning: dereferencing 'void *' pointer
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c:426: error: request for member 'xEventListItem' in something not a structure or union

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSuspend':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:844: warning: dereferencing 'void *' pointer
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:844: error: request for member 'xEventListItem' in something not a structure or union

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskPlaceOnEventList':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1593: error: invalid operands to binary ==

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:55:43 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskSuspend':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:844: warning: dereferencing 'void *' pointer
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:844: error: request for member 'xEventListItem' in something not a structure or union

/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskPlaceOnEventList':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1593: error: invalid operands to binary ==

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:57:13 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c: In function 'vTaskPlaceOnEventList':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1593: error: cannot convert to a pointer type

make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 15:58:01 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51338	    372	  87852	 139562	  2212a	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 16:00:52 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51338	    372	  87852	 139562	  2212a	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 16:32:08 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51878	    372	  87852	 140102	  22346	RTOSDemo/executable.elf


Done!

Done.

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Thu Jul 02 17:37:11 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51910	    372	  87852	 140134	  22366	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 17:37:43 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

write (count, cmdBuffer, dataBuffer) failed C0000004.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2301.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

Downloading c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex.

Downloaded firmware version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      2 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   42.99 C, Min. Reading:   37.58 C, Max.

Reading:   44.47 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.502 V, Max.

Reading:   2.508 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

At Local date and time: Thu Jul 02 18:25:53 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  51950	    372	  87844	 140166	  22386	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:25:21 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'xTaskCheckForTimeOut':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:71: error: 'xNumOfOverflows' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:71: error: (Each undeclared identifier is reported only once
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:71: error: for each function it appears in.)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:77: error: 'pdTRUE' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:84: error: 'pdFALSE' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: At top level:
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:96: warning: conflicting types for 'vTaskSetTimeOutState'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:83: warning: previous implicit declaration of 'vTaskSetTimeOutState' was here
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'vTaskSetTimeOutState':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:97: error: 'xNumOfOverflows' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:109: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:111: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:116: error: expected expression before 'xTimeOutType'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:132: error: 'pdTRUE' undeclared (first use in this function)
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:134: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:142: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:150: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:103: warning: return type of 'main' is not 'int'
make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 20:27:35 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:53:19: error: conio.h: No such file or directory
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:113: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:115: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:184: warning: incompatible implicit declaration of built-in function 'exit'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:107: warning: return type of 'main' is not 'int'
make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 20:28:16 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:111: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:113: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:136: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:144: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:152: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:157: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:176: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:181: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:182: warning: incompatible implicit declaration of built-in function 'exit'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:105: warning: return type of 'main' is not 'int'

/
cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccpw6KfT.o: In function `vTaskSetTimeOutState':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:71: multiple definition of `vTaskSetTimeOutState'
/cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccwVIJA2.o:/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1697: first defined here
/cygdrive/c/devtools/Xilinx/11.1/EDK/gnu/powerpc-eabi/nt/bin/../lib/gcc/powerpc-eabi/4.1.1/../../../../powerpc-eabi/bin/ld: Warning: size of symbol `vTaskSetTimeOutState' changed from 68 in /cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccwVIJA2.o to 72 in /cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccpw6KfT.o
/cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccpw6KfT.o: In function `xTaskCheckForTimeOut':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:77: multiple definition of `xTaskCheckForTimeOut'
/cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccwVIJA2.o:/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1704: first defined here
/cygdrive/c/devtools/Xilinx/11.1/EDK/gnu/powerpc-eabi/nt/bin/../lib/gcc/powerpc-eabi/4.1.1/../../../../powerpc-eabi/bin/ld: Warning: size of symbol `xTaskCheckForTimeOut' changed from 388 in /cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccwVIJA2.o to 276 in /cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccpw6KfT.o
/cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccwVIJA2.o: In function `vTaskSwitchContext':
tasks.c:(.text+0x1798): undefined reference to `vApplicationStackOverflowHook'
tasks.c:(.text+0x17e8): undefined reference to `vApplicationStackOverflowHook'
/cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccpw6KfT.o: In function `main':
main.c:(.text+0x2f4): undefined reference to `kbhit'
main.c:(.text+0x304): undefined reference to `getch'
collect2: ld returned 1 exit status
make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 20:31:20 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:117: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:143: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:105: warning: return type of 'main' is not 'int'

/cygdrive/c/DOCUME~1/RICHAR~1.DOM/LOCALS~1/Temp/ccZOTZW1.o: In function `vTaskSwitchContext':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1556: undefined reference to `vApplicationStackOverflowHook'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c:1557: undefined reference to `vApplicationStackOverflowHook'
collect2: ld returned 1 exit status
make: *** [RTOSDemo/executable.elf] Error 1



Done!

At Local date and time: Thu Jul 02 20:31:50 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:123: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:146: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50578	    368	  87832	 138778	  21e1a	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 20:32:59 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:123: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:148: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50706	    368	  87832	 138906	  21e9a	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:38:30 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:123: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:148: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50706	    368	  87832	 138906	  21e9a	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 20:40:24 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:151: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50730	    368	  87840	 138938	  21eba	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:43:10 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:151: warning: incompatible implicit declaration of built-in function 'printf'
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50730	    368	  87840	 138938	  21eba	RTOSDemo/executable.elf


Done!

At Local date and time: Thu Jul 02 20:46:15 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50694	    368	  87840	 138902	  21e96	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:49:41 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50730	    368	  87840	 138938	  21eba	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:54:28 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50802	    368	  87832	 139002	  21efa	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:58:12 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:120: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50846	    368	  87832	 139046	  21f26	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 20:59:39 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c: In function 'main':
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:122: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:124: warning: comparison is always true due to limited range of data type
/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c:108: warning: return type of 'main' is not 'int'

powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50866	    368	  87832	 139066	  21f3a	RTOSDemo/executable.elf


Done!

Done.

At Local date and time: Thu Jul 02 21:29:34 2009
 make -f system.make program started...

powerpc-eabi-gcc -O0 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  50622	    372	  87856	 138850	  21e62	RTOSDemo/executable.elf


Done!

Done.

Done.

At Local date and time: Fri Jul 03 02:08:31 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      1 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   38.07 C, Min. Reading:   35.12 C, Max.

Reading:   38.56 C

5: VCCINT Supply: Current Reading:   0.999 V, Min. Reading:   0.999 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.505 V, Min. Reading:   2.502 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

Done.

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

Xilinx Platform Studio (XPS)
Xilinx EDK 11.2 Build EDK_LS3.47

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Fri Jul 03 18:19:28 2009
 make -f system.make download started...

*********************************************
Downloading Bitstream onto the target board
*********************************************
impact -batch etc/download.cmd
Release 11.2 - iMPACT L.46 (nt)

Copyright (c) 1995-2009 Xilinx, Inc.  All rights reserved.

Preference Table

Name                 Setting             

StartupClock         Auto_Correction     

AutoSignature        False               

KeepSVF              False               

ConcurrentMode       False               

UseHighz             False               

ConfigOnFailure      Stop                

UserLevel            Novice              

MessageLevel         Detailed            

svfUseTime           false               

SpiByteSwap          Auto_Correction     

AutoDetecting cable. Please wait.

Connecting to cable (Usb Port - USB21).

Checking cable driver.

 Driver file xusb_xp2.sys found.

 Driver version: src=2301, dest=2301.

 Driver windrvr6.sys version = 9.0.0.0. WinDriver v9.00 Jungo (c) 1997 - 2007 Build Date: Mar 27 2007 X86 32bit SYS

13:58:07, version = 900.

 Cable PID = 0008.

 Max current requested during enumeration is 300 mA.

Type = 0x0005.

 Cable Type = 3, Revision = 0.

 Setting cable speed to 6 MHz.

Cable connection established.

Firmware version = 2401.

File version of c:/devtools/Xilinx/11.1/ISE/data/xusb_xp2.hex = 2401.

Firmware hex file version = 2401.

PLD file version = 200Dh.

 PLD version = 200Dh.

Identifying chain contents...'0': : Manufacturer's ID = Xilinx xc5vfx70t, Version : 6

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/virtex5/data/xc5vfx70t.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'1': : Manufacturer's ID = Xilinx xccace, Version : 0

----------------------------------------------------------------------

----------------------------------------------------------------------

'2': : Manufacturer's ID = Xilinx xc95144xl, Version : 5

INFO:iMPACT:501 - '1': Added Device xc5vfx70t successfully.
INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/acecf/data/xccace.bsd...
INFO:iMPACT:501 - '1': Added Device xccace successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xc9500xl/data/xc95144xl.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'3': : Manufacturer's ID = Xilinx xcf32p, Version : 15

INFO:iMPACT:501 - '1': Added Device xc95144xl successfully.

INFO:iMPACT:1777 - 
   Reading c:/devtools/Xilinx/11.1/ISE/xcfp/data/xcf32p.bsd...

----------------------------------------------------------------------

----------------------------------------------------------------------

'4': : Manufacturer's ID = Xilinx xcf32p, Version : 15

----------------------------------------------------------------------

----------------------------------------------------------------------

done.

Elapsed time =      5 sec.

Elapsed time =      0 sec.

'5': Loading file 'implementation/download.bit' ...

INFO:iMPACT:501 - '1': Added Device xcf32p successfully.
INFO:iMPACT:501 - '1': Added Device xcf32p successfully.

done.

UserID read from the bitstream file = 0xFFFFFFFF.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

Maximum TCK operating frequency for this device chain: 10000000.

Validating chain...

Boundary-scan chain validated successfully.

5: Device Temperature: Current Reading:   59.23 C, Min. Reading:   38.07 C, Max.

Reading:   74.99 C

5: VCCINT Supply: Current Reading:   0.996 V, Min. Reading:   0.993 V, Max.

Reading:   1.002 V

5: VCCAUX Supply: Current Reading:   2.496 V, Min. Reading:   2.493 V, Max.

Reading:   2.505 V

INFO:iMPACT:501 - '5': Added Device xc5vfx70t successfully.

'5': Programming device...

 Match_cycle = 2.

done.

'5': Reading status register contents...

CRC error                                         :         0

Decryptor security set                            :         0

DCM locked                                        :         1

DCI matched                                       :         1

End of startup signal from Startup block          :         1

status of GTS_CFG_B                               :         1

status of GWE                                     :         1

status of GHIGH                                   :         1

value of MODE pin M0                              :         1

value of MODE pin M1                              :         0

Value of MODE pin M2                              :         1

Internal signal indicates when housecleaning is completed:         1

Value driver in from INIT pad                     :         1

Internal signal indicates that chip is configured :         1

Value of DONE pin                                 :         1

Indicates when ID value written does not match chip ID:         0

Decryptor error Signal                            :         0

System Monitor Over-Temperature Alarm             :         0

startup_state[18] CFG startup state machine       :         0

startup_state[19] CFG startup state machine       :         0

startup_state[20] CFG startup state machine       :         1

E-fuse program voltage available                  :         0

SPI Flash Type[22] Select                         :         1

SPI Flash Type[23] Select                         :         1

SPI Flash Type[24] Select                         :         1

CFG bus width auto detection result               :         0

CFG bus width auto detection result               :         0

Reserved                                          :         0

BPI address wrap around error                     :         0

IPROG pulsed                                      :         0

read back crc error                               :         0

Indicates that efuse logic is busy                :         0

 Match_cycle = 2.

'5': Programmed successfully.

Elapsed time =     11 sec.

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

----------------------------------------------------------------------

INFO:iMPACT:2219 - Status register values:
INFO:iMPACT - 0011 1111 1011 1110 0000 1011 1000 0000 
INFO:iMPACT:579 - '5': Completed downloading bit file to device.
INFO:iMPACT - '5': Programing completed successfully.
INFO:iMPACT - '5': Checking done pin....done.



Done!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

At Local date and time: Fri Jul 03 18:20:05 2009
 make -f system.make program started...

powerpc-eabi-gcc -O3 /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/BlockQ.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/blocktim.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/comtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/countsem.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/death.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/dynamic.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/flash.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/GenQTest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/integer.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/QPeek.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/recmutex.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../Common/Minimal/semtest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/tasks.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/list.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/queue.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/croutine.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/portasm.S /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/GCC/PPC440_Xilinx/port.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/../../../Source/portable/MemMang/heap_2.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop-reg-test.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/flop/flop.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/partest/partest.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/serial/serial.c /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/main.c  -o RTOSDemo/executable.elf \
    -mfpu=dp_full -mcpu=440  -Wl,-T -Wl,/cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/RTOSDemo/RTOSDemo_linker_script.ld  -g    -I./ppc440_0/include/   -I../../Source/include -I../../Source/portable/GCC/PPC440_Xilinx -I../Common/include -I./RTOSDemo -I./RTOSDemo/flop  -L./ppc440_0/lib/  \
-D USE_DP_FPU -D GCC_PPC440 -mregnames  
powerpc-eabi-size RTOSDemo/executable.elf 
   text	   data	    bss	    dec	    hex	filename
  44758	    372	  87852	 132982	  20776	RTOSDemo/executable.elf


Done!

start xbash -noblock -q -c "cd /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; xmd -xmp system.xmp -opt etc/xmd_ppc440_0.opt -lp /cygdrive/c/E/Dev/FreeRTOS/WorkingCopy3/Demo/PPC440_DP_FPU_Xilinx_Virtex5_GCC/; exit;"

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 253 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\system.mhs line 298 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

WARNING:EDK:1582 - IPNAME:plbv46_pcie INSTANCE:PCIe_Bridge - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 239 - deprecated core for architecture 'virtex5fx'!

WARNING:EDK:1582 - IPNAME:xps_ethernetlite INSTANCE:Ethernet_MAC - C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\_xps_tempmhsfilename.mhs line 284 - deprecated core for architecture 'virtex5fx'!

Generating Block Diagram to Buffer 

Generated Block Diagram SVG

At Local date and time: Sun Jul 05 09:36:55 2009
 make -f system.make hwclean started...

rm -f implementation/system.ngc
rm -f platgen.log
rm -f __xps/ise/_xmsgs/platgen.xmsgs
rm -f implementation/system.bmm
rm -f implementation/system.bit
rm -f implementation/system.ncd
rm -f implementation/system_bd.bmm 
rm -f implementation/system_map.ncd 
rm -f __xps/system_routed
rm -rf implementation synthesis xst hdl
rm -rf xst.srp system.srp
rm -f __xps/ise/_xmsgs/bitinit.xmsgs


Done!

At Local date and time: Sun Jul 05 09:37:10 2009
 make -f system.make swclean started...

rm -rf ppc440_0/
rm -f libgen.log
rm -f __xps/ise/_xmsgs/libgen.xmsgs
rm -f RTOSDemo/executable.elf 


Done!

Writing filter settings....

Done writing filter settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.filters

Done writing Tab View settings to:
	C:\E\Dev\FreeRTOS\WorkingCopy3\Demo\PPC440_DP_FPU_Xilinx_Virtex5_GCC\__xps\system.gui

