
# ##############################################################################
# Created by Base System Builder Wizard for Xilinx EDK 11.1 Build EDK_L.29.1
# Sat Jun 13 13:14:11 2009
# Target Board:  Xilinx Virtex 5 ML507 Evaluation Platform Rev A
# Family:    virtex5
# Device:    xc5vfx70t
# Package:   ff1136
# Speed Grade:  -1
# Processor number: 1
# Processor 1: ppc440_0
# Processor clock frequency: 125.0
# Bus clock frequency: 125.0
# Debug Interface: FPGA JTAG
# ##############################################################################
 PARAMETER VERSION = 2.1.0


 PORT fpga_0_RS232_Uart_1_RX_pin = fpga_0_RS232_Uart_1_RX_pin, DIR = I
 PORT fpga_0_RS232_Uart_1_TX_pin = fpga_0_RS232_Uart_1_TX_pin, DIR = O
 PORT fpga_0_LEDs_8Bit_GPIO_IO_pin = fpga_0_LEDs_8Bit_GPIO_IO_pin, DIR = IO, VEC = [0:7]
 PORT fpga_0_LEDs_Positions_GPIO_IO_pin = fpga_0_LEDs_Positions_GPIO_IO_pin, DIR = IO, VEC = [0:4]
 PORT fpga_0_Push_Buttons_5Bit_GPIO_IO_pin = fpga_0_Push_Buttons_5Bit_GPIO_IO_pin, DIR = IO, VEC = [0:4]
 PORT fpga_0_DIP_Switches_8Bit_GPIO_IO_pin = fpga_0_DIP_Switches_8Bit_GPIO_IO_pin, DIR = IO, VEC = [0:7]
 PORT fpga_0_IIC_EEPROM_Sda_pin = fpga_0_IIC_EEPROM_Sda_pin, DIR = IO
 PORT fpga_0_IIC_EEPROM_Scl_pin = fpga_0_IIC_EEPROM_Scl_pin, DIR = IO
 PORT fpga_0_SRAM_Mem_A_pin = fpga_0_SRAM_Mem_A_pin_vslice_7_30_concat, DIR = O, VEC = [7:30]
 PORT fpga_0_SRAM_Mem_CEN_pin = fpga_0_SRAM_Mem_CEN_pin, DIR = O
 PORT fpga_0_SRAM_Mem_OEN_pin = fpga_0_SRAM_Mem_OEN_pin, DIR = O
 PORT fpga_0_SRAM_Mem_WEN_pin = fpga_0_SRAM_Mem_WEN_pin, DIR = O
 PORT fpga_0_SRAM_Mem_BEN_pin = fpga_0_SRAM_Mem_BEN_pin, DIR = O, VEC = [0:3]
 PORT fpga_0_SRAM_Mem_ADV_LDN_pin = fpga_0_SRAM_Mem_ADV_LDN_pin, DIR = O
 PORT fpga_0_SRAM_Mem_DQ_pin = fpga_0_SRAM_Mem_DQ_pin, DIR = IO, VEC = [0:31]
 PORT fpga_0_SRAM_ZBT_CLK_OUT_pin = SRAM_CLK_OUT_s, DIR = O
 PORT fpga_0_SRAM_ZBT_CLK_FB_pin = SRAM_CLK_FB_s, DIR = I, SIGIS = CLK, CLK_FREQ = 125000000
 PORT fpga_0_PCIe_Bridge_RXN_pin = fpga_0_PCIe_Bridge_RXN_pin, DIR = I
 PORT fpga_0_PCIe_Bridge_RXP_pin = fpga_0_PCIe_Bridge_RXP_pin, DIR = I
 PORT fpga_0_PCIe_Bridge_TXN_pin = fpga_0_PCIe_Bridge_TXN_pin, DIR = O
 PORT fpga_0_PCIe_Bridge_TXP_pin = fpga_0_PCIe_Bridge_TXP_pin, DIR = O
 PORT fpga_0_Ethernet_MAC_PHY_tx_clk_pin = fpga_0_Ethernet_MAC_PHY_tx_clk_pin, DIR = I
 PORT fpga_0_Ethernet_MAC_PHY_rx_clk_pin = fpga_0_Ethernet_MAC_PHY_rx_clk_pin, DIR = I
 PORT fpga_0_Ethernet_MAC_PHY_crs_pin = fpga_0_Ethernet_MAC_PHY_crs_pin, DIR = I
 PORT fpga_0_Ethernet_MAC_PHY_dv_pin = fpga_0_Ethernet_MAC_PHY_dv_pin, DIR = I
 PORT fpga_0_Ethernet_MAC_PHY_rx_data_pin = fpga_0_Ethernet_MAC_PHY_rx_data_pin, DIR = I, VEC = [3:0]
 PORT fpga_0_Ethernet_MAC_PHY_col_pin = fpga_0_Ethernet_MAC_PHY_col_pin, DIR = I
 PORT fpga_0_Ethernet_MAC_PHY_rx_er_pin = fpga_0_Ethernet_MAC_PHY_rx_er_pin, DIR = I
 PORT fpga_0_Ethernet_MAC_PHY_rst_n_pin = fpga_0_Ethernet_MAC_PHY_rst_n_pin, DIR = O
 PORT fpga_0_Ethernet_MAC_PHY_tx_en_pin = fpga_0_Ethernet_MAC_PHY_tx_en_pin, DIR = O
 PORT fpga_0_Ethernet_MAC_PHY_tx_data_pin = fpga_0_Ethernet_MAC_PHY_tx_data_pin, DIR = O, VEC = [3:0]
 PORT fpga_0_Ethernet_MAC_MDINT_pin = fpga_0_Ethernet_MAC_MDINT_pin, DIR = I, SIGIS = INTERRUPT, SENSITIVITY = LEVEL_LOW, INTERRUPT_PRIORITY = MEDIUM
 PORT fpga_0_DDR2_SDRAM_DDR2_DQ_pin = fpga_0_DDR2_SDRAM_DDR2_DQ_pin, DIR = IO, VEC = [63:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_DQS_pin = fpga_0_DDR2_SDRAM_DDR2_DQS_pin, DIR = IO, VEC = [7:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_DQS_N_pin = fpga_0_DDR2_SDRAM_DDR2_DQS_N_pin, DIR = IO, VEC = [7:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_A_pin = fpga_0_DDR2_SDRAM_DDR2_A_pin, DIR = O, VEC = [12:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_BA_pin = fpga_0_DDR2_SDRAM_DDR2_BA_pin, DIR = O, VEC = [1:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_RAS_N_pin = fpga_0_DDR2_SDRAM_DDR2_RAS_N_pin, DIR = O
 PORT fpga_0_DDR2_SDRAM_DDR2_CAS_N_pin = fpga_0_DDR2_SDRAM_DDR2_CAS_N_pin, DIR = O
 PORT fpga_0_DDR2_SDRAM_DDR2_WE_N_pin = fpga_0_DDR2_SDRAM_DDR2_WE_N_pin, DIR = O
 PORT fpga_0_DDR2_SDRAM_DDR2_CS_N_pin = fpga_0_DDR2_SDRAM_DDR2_CS_N_pin, DIR = O
 PORT fpga_0_DDR2_SDRAM_DDR2_ODT_pin = fpga_0_DDR2_SDRAM_DDR2_ODT_pin, DIR = O, VEC = [1:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_CKE_pin = fpga_0_DDR2_SDRAM_DDR2_CKE_pin, DIR = O
 PORT fpga_0_DDR2_SDRAM_DDR2_DM_pin = fpga_0_DDR2_SDRAM_DDR2_DM_pin, DIR = O, VEC = [7:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_CK_pin = fpga_0_DDR2_SDRAM_DDR2_CK_pin, DIR = O, VEC = [1:0]
 PORT fpga_0_DDR2_SDRAM_DDR2_CK_N_pin = fpga_0_DDR2_SDRAM_DDR2_CK_N_pin, DIR = O, VEC = [1:0]
 PORT fpga_0_SysACE_CompactFlash_SysACE_MPA_pin = fpga_0_SysACE_CompactFlash_SysACE_MPA_pin, DIR = O, VEC = [6:0]
 PORT fpga_0_SysACE_CompactFlash_SysACE_CLK_pin = fpga_0_SysACE_CompactFlash_SysACE_CLK_pin, DIR = I
 PORT fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin = fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin, DIR = I
 PORT fpga_0_SysACE_CompactFlash_SysACE_CEN_pin = fpga_0_SysACE_CompactFlash_SysACE_CEN_pin, DIR = O
 PORT fpga_0_SysACE_CompactFlash_SysACE_OEN_pin = fpga_0_SysACE_CompactFlash_SysACE_OEN_pin, DIR = O
 PORT fpga_0_SysACE_CompactFlash_SysACE_WEN_pin = fpga_0_SysACE_CompactFlash_SysACE_WEN_pin, DIR = O
 PORT fpga_0_SysACE_CompactFlash_SysACE_MPD_pin = fpga_0_SysACE_CompactFlash_SysACE_MPD_pin, DIR = IO, VEC = [15:0]
 PORT fpga_0_clk_1_sys_clk_pin = dcm_clk_s, DIR = I, SIGIS = CLK, CLK_FREQ = 100000000
 PORT fpga_0_rst_1_sys_rst_pin = sys_rst_s, DIR = I, SIGIS = RST, RST_POLARITY = 0
 PORT fpga_0_PCIe_Diff_Clk_IBUF_DS_P_pin = PCIe_Diff_Clk, DIR = I, DIFFERENTIAL_POLARITY = P, SIGIS = CLK
 PORT fpga_0_PCIe_Diff_Clk_IBUF_DS_N_pin = PCIe_Diff_Clk, DIR = I, DIFFERENTIAL_POLARITY = N, SIGIS = CLK


BEGIN ppc440_virtex5
 PARAMETER INSTANCE = ppc440_0
 PARAMETER C_IDCR_BASEADDR = 0b0000000000
 PARAMETER C_IDCR_HIGHADDR = 0b0011111111
 PARAMETER C_APU_CONTROL = 0b00000010000000001
 PARAMETER C_PPC440MC_ROW_CONFLICT_MASK = 0x003FFE00
 PARAMETER C_PPC440MC_BANK_CONFLICT_MASK = 0x00C00000
 PARAMETER C_PPC440MC_CONTROL = 0xF810008F
 PARAMETER C_SPLB0_USE_MPLB_ADDR = 1
 PARAMETER C_SPLB0_NUM_MPLB_ADDR_RNG = 1
 PARAMETER C_SPLB1_NUM_MPLB_ADDR_RNG = 0
 PARAMETER HW_VER = 1.01.a
 PARAMETER C_SPLB0_RNG0_MPLB_BASEADDR = 0x80000000
 PARAMETER C_SPLB0_RNG0_MPLB_HIGHADDR = 0xffffffff
 PARAMETER C_SPLB0_RNG_MC_BASEADDR = 0x00000000
 PARAMETER C_SPLB0_RNG_MC_HIGHADDR = 0x0fffffff
 BUS_INTERFACE MPLB = plb_v46_0
 BUS_INTERFACE SPLB0 = ppc440_0_SPLB0
 BUS_INTERFACE PPC440MC = ppc440_0_PPC440MC
 BUS_INTERFACE MFCB = ppc440_0_fcb_v20
 BUS_INTERFACE JTAGPPC = ppc440_0_jtagppc_bus
 BUS_INTERFACE RESETPPC = ppc_reset_bus
 PORT CPMC440CLK = clk_125_0000MHzPLL0
 PORT CPMINTERCONNECTCLK = clk_125_0000MHzPLL0
 PORT CPMINTERCONNECTCLKNTO1 = net_vcc
 PORT EICC440EXTIRQ = ppc440_0_EICC440EXTIRQ
 PORT CPMMCCLK = clk_125_0000MHzPLL0_ADJUST
 PORT CPMPPCMPLBCLK = clk_125_0000MHzPLL0_ADJUST
 PORT CPMPPCS0PLBCLK = clk_125_0000MHzPLL0_ADJUST
END

BEGIN plb_v46
 PARAMETER INSTANCE = plb_v46_0
 PARAMETER C_DCR_INTFCE = 0
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 1.04.a
 PORT PLB_Clk = clk_125_0000MHzPLL0_ADJUST
 PORT SYS_Rst = sys_bus_reset
END

BEGIN xps_bram_if_cntlr
 PARAMETER INSTANCE = xps_bram_if_cntlr_1
 PARAMETER C_SPLB_NATIVE_DWIDTH = 64
 PARAMETER C_SPLB_SUPPORT_BURSTS = 1
 PARAMETER C_SPLB_P2P = 0
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 1.00.b
 PARAMETER C_BASEADDR = 0xffffe000
 PARAMETER C_HIGHADDR = 0xffffffff
 BUS_INTERFACE SPLB = plb_v46_0
 BUS_INTERFACE PORTA = xps_bram_if_cntlr_1_port
END

BEGIN bram_block
 PARAMETER INSTANCE = xps_bram_if_cntlr_1_bram
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 1.00.a
 BUS_INTERFACE PORTA = xps_bram_if_cntlr_1_port
END

BEGIN xps_uartlite
 PARAMETER INSTANCE = RS232_Uart_1
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_BAUDRATE = 9600
 PARAMETER C_DATA_BITS = 8
 PARAMETER C_USE_PARITY = 0
 PARAMETER C_ODD_PARITY = 0
 PARAMETER HW_VER = 1.01.a
 PARAMETER C_BASEADDR = 0x84000000
 PARAMETER C_HIGHADDR = 0x8400ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT RX = fpga_0_RS232_Uart_1_RX_pin
 PORT TX = fpga_0_RS232_Uart_1_TX_pin
 PORT Interrupt = RS232_Uart_1_Interrupt
END

BEGIN xps_gpio
 PARAMETER INSTANCE = LEDs_8Bit
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_ALL_INPUTS = 0
 PARAMETER C_GPIO_WIDTH = 8
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81440000
 PARAMETER C_HIGHADDR = 0x8144ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT GPIO_IO = fpga_0_LEDs_8Bit_GPIO_IO_pin
END

BEGIN xps_gpio
 PARAMETER INSTANCE = LEDs_Positions
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_ALL_INPUTS = 0
 PARAMETER C_GPIO_WIDTH = 5
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81420000
 PARAMETER C_HIGHADDR = 0x8142ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT GPIO_IO = fpga_0_LEDs_Positions_GPIO_IO_pin
END

BEGIN xps_gpio
 PARAMETER INSTANCE = Push_Buttons_5Bit
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_ALL_INPUTS = 1
 PARAMETER C_GPIO_WIDTH = 5
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81400000
 PARAMETER C_HIGHADDR = 0x8140ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT GPIO_IO = fpga_0_Push_Buttons_5Bit_GPIO_IO_pin
END

BEGIN xps_gpio
 PARAMETER INSTANCE = DIP_Switches_8Bit
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_ALL_INPUTS = 1
 PARAMETER C_GPIO_WIDTH = 8
 PARAMETER C_INTERRUPT_PRESENT = 0
 PARAMETER C_IS_DUAL = 0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81460000
 PARAMETER C_HIGHADDR = 0x8146ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT GPIO_IO = fpga_0_DIP_Switches_8Bit_GPIO_IO_pin
END

BEGIN xps_iic
 PARAMETER INSTANCE = IIC_EEPROM
 PARAMETER C_IIC_FREQ = 100000
 PARAMETER C_TEN_BIT_ADR = 0
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 2.01.a
 PARAMETER C_BASEADDR = 0x81600000
 PARAMETER C_HIGHADDR = 0x8160ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT Sda = fpga_0_IIC_EEPROM_Sda_pin
 PORT Scl = fpga_0_IIC_EEPROM_Scl_pin
END

BEGIN xps_mch_emc
 PARAMETER INSTANCE = SRAM
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_NUM_BANKS_MEM = 1
 PARAMETER C_NUM_CHANNELS = 0
 PARAMETER C_MEM0_WIDTH = 32
 PARAMETER C_MAX_MEM_WIDTH = 32
 PARAMETER C_INCLUDE_DATAWIDTH_MATCHING_0 = 0
 PARAMETER C_SYNCH_MEM_0 = 1
 PARAMETER C_TCEDV_PS_MEM_0 = 0
 PARAMETER C_TAVDV_PS_MEM_0 = 0
 PARAMETER C_THZCE_PS_MEM_0 = 0
 PARAMETER C_THZOE_PS_MEM_0 = 0
 PARAMETER C_TWC_PS_MEM_0 = 0
 PARAMETER C_TWP_PS_MEM_0 = 0
 PARAMETER C_TLZWE_PS_MEM_0 = 0
 PARAMETER HW_VER = 3.00.a
 PARAMETER C_MEM0_BASEADDR = 0xf8000000
 PARAMETER C_MEM0_HIGHADDR = 0xf80fffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT RdClk = clk_125_0000MHzPLL0_ADJUST
 PORT Mem_A = 0b0000000 & fpga_0_SRAM_Mem_A_pin_vslice_7_30_concat & 0b0
 PORT Mem_CEN = fpga_0_SRAM_Mem_CEN_pin
 PORT Mem_OEN = fpga_0_SRAM_Mem_OEN_pin
 PORT Mem_WEN = fpga_0_SRAM_Mem_WEN_pin
 PORT Mem_BEN = fpga_0_SRAM_Mem_BEN_pin
 PORT Mem_ADV_LDN = fpga_0_SRAM_Mem_ADV_LDN_pin
 PORT Mem_DQ = fpga_0_SRAM_Mem_DQ_pin
END

BEGIN plbv46_pcie
 PARAMETER INSTANCE = PCIe_Bridge
 PARAMETER C_FAMILY = virtex5
 PARAMETER C_IPIFBAR_NUM = 2
 PARAMETER C_PCIBAR_NUM = 1
 PARAMETER C_DEVICE_ID = 0x0505
 PARAMETER C_VENDOR_ID = 0x10EE
 PARAMETER C_CLASS_CODE = 0x058000
 PARAMETER C_REV_ID = 0x00
 PARAMETER C_SUBSYSTEM_ID = 0x0000
 PARAMETER C_SUBSYSTEM_VENDOR_ID = 0x0000
 PARAMETER C_COMP_TIMEOUT = 1
 PARAMETER C_IPIFBAR2PCIBAR_0 = 0x00000000
 PARAMETER C_IPIFBAR2PCIBAR_1 = 0x00000000
 PARAMETER C_PCIBAR2IPIFBAR_0 = 0xf8000000
 PARAMETER C_PCIBAR2IPIFBAR_1 = 0x00000000
 PARAMETER C_PCIBAR_LEN_0 = 20
 PARAMETER C_PCIBAR_LEN_1 = 28
 PARAMETER C_BOARD = ml507
 PARAMETER HW_VER = 3.00.b
 PARAMETER C_BASEADDR = 0x85c00000
 PARAMETER C_HIGHADDR = 0x85c0ffff
 PARAMETER C_IPIFBAR_0 = 0xc0000000
 PARAMETER C_IPIFBAR_HIGHADDR_0 = 0xdfffffff
 PARAMETER C_IPIFBAR_1 = 0xe0000000
 PARAMETER C_IPIFBAR_HIGHADDR_1 = 0xefffffff
 BUS_INTERFACE SPLB = plb_v46_0
 BUS_INTERFACE MPLB = ppc440_0_SPLB0
 PORT PERSTN = net_vcc
 PORT REFCLK = PCIe_Diff_Clk
 PORT RXN = fpga_0_PCIe_Bridge_RXN_pin
 PORT RXP = fpga_0_PCIe_Bridge_RXP_pin
 PORT TXN = fpga_0_PCIe_Bridge_TXN_pin
 PORT TXP = fpga_0_PCIe_Bridge_TXP_pin
 PORT MSI_request = net_gnd
END

BEGIN plb_v46
 PARAMETER INSTANCE = ppc440_0_SPLB0
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 1.04.a
 PORT PLB_Clk = clk_125_0000MHzPLL0_ADJUST
 PORT SYS_Rst = sys_bus_reset
END

BEGIN xps_ethernetlite
 PARAMETER INSTANCE = Ethernet_MAC
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 2.01.a
 PARAMETER C_BASEADDR = 0x81000000
 PARAMETER C_HIGHADDR = 0x8100ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT PHY_tx_clk = fpga_0_Ethernet_MAC_PHY_tx_clk_pin
 PORT PHY_rx_clk = fpga_0_Ethernet_MAC_PHY_rx_clk_pin
 PORT PHY_crs = fpga_0_Ethernet_MAC_PHY_crs_pin
 PORT PHY_dv = fpga_0_Ethernet_MAC_PHY_dv_pin
 PORT PHY_rx_data = fpga_0_Ethernet_MAC_PHY_rx_data_pin
 PORT PHY_col = fpga_0_Ethernet_MAC_PHY_col_pin
 PORT PHY_rx_er = fpga_0_Ethernet_MAC_PHY_rx_er_pin
 PORT PHY_rst_n = fpga_0_Ethernet_MAC_PHY_rst_n_pin
 PORT PHY_tx_en = fpga_0_Ethernet_MAC_PHY_tx_en_pin
 PORT PHY_tx_data = fpga_0_Ethernet_MAC_PHY_tx_data_pin
END

BEGIN ppc440mc_ddr2
 PARAMETER INSTANCE = DDR2_SDRAM
 PARAMETER C_DDR_BAWIDTH = 2
 PARAMETER C_NUM_CLK_PAIRS = 2
 PARAMETER C_DDR_DWIDTH = 64
 PARAMETER C_DDR_CAWIDTH = 10
 PARAMETER C_NUM_RANKS_MEM = 1
 PARAMETER C_CS_BITS = 0
 PARAMETER C_DDR_DM_WIDTH = 8
 PARAMETER C_DQ_BITS = 8
 PARAMETER C_DDR2_ODT_WIDTH = 2
 PARAMETER C_DDR2_ADDT_LAT = 0
 PARAMETER C_INCLUDE_ECC_SUPPORT = 0
 PARAMETER C_DDR2_ODT_SETTING = 1
 PARAMETER C_DQS_BITS = 3
 PARAMETER C_DDR_DQS_WIDTH = 8
 PARAMETER C_DDR_RAWIDTH = 13
 PARAMETER C_DDR_BURST_LENGTH = 4
 PARAMETER C_DDR_CAS_LAT = 4
 PARAMETER C_REG_DIMM = 0
 PARAMETER C_MIB_MC_CLOCK_RATIO = 1
 PARAMETER C_DDR_TREFI = 3900
 PARAMETER C_DDR_TRAS = 40000
 PARAMETER C_DDR_TRCD = 15000
 PARAMETER C_DDR_TRFC = 75000
 PARAMETER C_DDR_TRP = 15000
 PARAMETER C_DDR_TRTP = 7500
 PARAMETER C_DDR_TWR = 15000
 PARAMETER C_DDR_TWTR = 7500
 PARAMETER C_MC_MIBCLK_PERIOD_PS = 8000
 PARAMETER C_IDEL_HIGH_PERF = TRUE
 PARAMETER C_NUM_IDELAYCTRL = 3
 PARAMETER C_IDELAYCTRL_LOC = IDELAYCTRL_X0Y6-IDELAYCTRL_X0Y2-IDELAYCTRL_X0Y1
 PARAMETER C_DQS_IO_COL = 0b000000000000000000
 PARAMETER C_DQ_IO_MS = 0b000000000111010100111101000011110001111000101110110000111100000110111100
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_MEM_BASEADDR = 0x00000000
 PARAMETER C_MEM_HIGHADDR = 0x0fffffff
 BUS_INTERFACE PPC440MC = ppc440_0_PPC440MC
 PORT mc_mibclk = clk_125_0000MHzPLL0_ADJUST
 PORT mi_mcclk90 = clk_125_0000MHz90PLL0_ADJUST
 PORT mi_mcreset = sys_bus_reset
 PORT mi_mcclkdiv2 = clk_62_5000MHzPLL0_ADJUST
 PORT mi_mcclk_200 = clk_200_0000MHz
 PORT DDR2_DQ = fpga_0_DDR2_SDRAM_DDR2_DQ_pin
 PORT DDR2_DQS = fpga_0_DDR2_SDRAM_DDR2_DQS_pin
 PORT DDR2_DQS_N = fpga_0_DDR2_SDRAM_DDR2_DQS_N_pin
 PORT DDR2_A = fpga_0_DDR2_SDRAM_DDR2_A_pin
 PORT DDR2_BA = fpga_0_DDR2_SDRAM_DDR2_BA_pin
 PORT DDR2_RAS_N = fpga_0_DDR2_SDRAM_DDR2_RAS_N_pin
 PORT DDR2_CAS_N = fpga_0_DDR2_SDRAM_DDR2_CAS_N_pin
 PORT DDR2_WE_N = fpga_0_DDR2_SDRAM_DDR2_WE_N_pin
 PORT DDR2_CS_N = fpga_0_DDR2_SDRAM_DDR2_CS_N_pin
 PORT DDR2_ODT = fpga_0_DDR2_SDRAM_DDR2_ODT_pin
 PORT DDR2_CKE = fpga_0_DDR2_SDRAM_DDR2_CKE_pin
 PORT DDR2_DM = fpga_0_DDR2_SDRAM_DDR2_DM_pin
 PORT DDR2_CK = fpga_0_DDR2_SDRAM_DDR2_CK_pin
 PORT DDR2_CK_N = fpga_0_DDR2_SDRAM_DDR2_CK_N_pin
END

BEGIN xps_sysace
 PARAMETER INSTANCE = SysACE_CompactFlash
 PARAMETER C_MEM_WIDTH = 16
 PARAMETER C_FAMILY = virtex5
 PARAMETER HW_VER = 1.01.a
 PARAMETER C_BASEADDR = 0x83600000
 PARAMETER C_HIGHADDR = 0x8360ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT SysACE_MPA = fpga_0_SysACE_CompactFlash_SysACE_MPA_pin
 PORT SysACE_CLK = fpga_0_SysACE_CompactFlash_SysACE_CLK_pin
 PORT SysACE_MPIRQ = fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin
 PORT SysACE_CEN = fpga_0_SysACE_CompactFlash_SysACE_CEN_pin
 PORT SysACE_OEN = fpga_0_SysACE_CompactFlash_SysACE_OEN_pin
 PORT SysACE_WEN = fpga_0_SysACE_CompactFlash_SysACE_WEN_pin
 PORT SysACE_MPD = fpga_0_SysACE_CompactFlash_SysACE_MPD_pin
END

BEGIN fcb_v20
 PARAMETER INSTANCE = ppc440_0_fcb_v20
 PARAMETER HW_VER = 1.00.a
 PORT FCB_CLK = clk_125_0000MHzPLL0_ADJUST
 PORT SYS_RST = sys_bus_reset
END

BEGIN apu_fpu_virtex5
 PARAMETER INSTANCE = ppc440_0_apu_fpu_virtex5
 PARAMETER C_DOUBLE_PRECISION = 0
 PARAMETER HW_VER = 1.01.a
 BUS_INTERFACE SFCB2 = ppc440_0_fcb_v20
END

BEGIN clock_generator
 PARAMETER INSTANCE = clock_generator_0
 PARAMETER C_CLKIN_FREQ = 100000000
 PARAMETER C_CLKFBIN_FREQ = 125000000
 PARAMETER C_CLKOUT0_FREQ = 125000000
 PARAMETER C_CLKOUT0_PHASE = 90
 PARAMETER C_CLKOUT0_GROUP = PLL0_ADJUST
 PARAMETER C_CLKOUT0_BUF = TRUE
 PARAMETER C_CLKOUT1_FREQ = 125000000
 PARAMETER C_CLKOUT1_PHASE = 0
 PARAMETER C_CLKOUT1_GROUP = PLL0
 PARAMETER C_CLKOUT1_BUF = TRUE
 PARAMETER C_CLKOUT2_FREQ = 125000000
 PARAMETER C_CLKOUT2_PHASE = 0
 PARAMETER C_CLKOUT2_GROUP = PLL0_ADJUST
 PARAMETER C_CLKOUT2_BUF = TRUE
 PARAMETER C_CLKOUT3_FREQ = 200000000
 PARAMETER C_CLKOUT3_PHASE = 0
 PARAMETER C_CLKOUT3_GROUP = NONE
 PARAMETER C_CLKOUT3_BUF = TRUE
 PARAMETER C_CLKOUT4_FREQ = 62500000
 PARAMETER C_CLKOUT4_PHASE = 0
 PARAMETER C_CLKOUT4_GROUP = PLL0_ADJUST
 PARAMETER C_CLKOUT4_BUF = TRUE
 PARAMETER C_CLKFBOUT_FREQ = 125000000
 PARAMETER C_CLKFBOUT_BUF = TRUE
 PARAMETER HW_VER = 3.00.a
 PORT CLKIN = dcm_clk_s
 PORT CLKFBIN = SRAM_CLK_FB_s
 PORT CLKOUT0 = clk_125_0000MHz90PLL0_ADJUST
 PORT CLKOUT1 = clk_125_0000MHzPLL0
 PORT CLKOUT2 = clk_125_0000MHzPLL0_ADJUST
 PORT CLKOUT3 = clk_200_0000MHz
 PORT CLKOUT4 = clk_62_5000MHzPLL0_ADJUST
 PORT CLKFBOUT = SRAM_CLK_OUT_s
 PORT RST = net_gnd
 PORT LOCKED = Dcm_all_locked
END

BEGIN jtagppc_cntlr
 PARAMETER INSTANCE = jtagppc_cntlr_inst
 PARAMETER HW_VER = 2.01.c
 BUS_INTERFACE JTAGPPC0 = ppc440_0_jtagppc_bus
END

BEGIN proc_sys_reset
 PARAMETER INSTANCE = proc_sys_reset_0
 PARAMETER C_EXT_RESET_HIGH = 0
 PARAMETER HW_VER = 2.00.a
 BUS_INTERFACE RESETPPC0 = ppc_reset_bus
 PORT Slowest_sync_clk = clk_125_0000MHzPLL0_ADJUST
 PORT Ext_Reset_In = sys_rst_s
 PORT Dcm_locked = Dcm_all_locked
 PORT Bus_Struct_Reset = sys_bus_reset
 PORT Peripheral_Reset = sys_periph_reset
END

BEGIN xps_intc
 PARAMETER INSTANCE = xps_intc_0
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_BASEADDR = 0x81800000
 PARAMETER C_HIGHADDR = 0x8180ffff
 BUS_INTERFACE SPLB = plb_v46_0
 PORT Intr = fpga_0_Ethernet_MAC_MDINT_pin&RS232_Uart_1_Interrupt
 PORT Irq = ppc440_0_EICC440EXTIRQ
END

