<?xml version="1.0" encoding="iso-8859-1"?>

<flash_board>
  <pass>
    <loader>$TOOLKIT_DIR$\config\flashloader\Atmel\AT91SAM7S64-EK\flash-at91sam7s64.flash</loader>
    <range>CODE 0x100000 0x110000</range>
    <rel_offset>0</rel_offset>
    <args>--flash
--boot
</args>
  </pass>
</flash_board>
