/*
	FreeRTOS V5.4.2 - Copyright (C) 2009 Real Time Engineers Ltd.

	This file is part of the FreeRTOS distribution.

	FreeRTOS is free software; you can redistribute it and/or modify it	under 
	the terms of the GNU General Public License (version 2) as published by the 
	Free Software Foundation and modified by the FreeRTOS exception.
	**NOTE** The exception to the GPL is included to allow you to distribute a
	combined work that includes FreeRTOS without being obliged to provide the 
	source code for proprietary components outside of the FreeRTOS kernel.  
	Alternative commercial license and support terms are also available upon 
	request.  See the licensing section of http://www.FreeRTOS.org for full 
	license details.

	FreeRTOS is distributed in the hope that it will be useful,	but WITHOUT
	ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
	FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for
	more details.

	You should have received a copy of the GNU General Public License along
	with FreeRTOS; if not, write to the Free Software Foundation, Inc., 59
	Temple Place, Suite 330, Boston, MA  02111-1307  USA.


	***************************************************************************
	*                                                                         *
	* Looking for a quick start?  Then check out the FreeRTOS eBook!          *
	* See http://www.FreeRTOS.org/Documentation for details                   *
	*                                                                         *
	***************************************************************************

	1 tab == 4 spaces!

	Please ensure to read the configuration and relevant port sections of the
	online documentation.

	http://www.FreeRTOS.org - Documentation, latest information, license and
	contact details.

	http://www.SafeRTOS.com - A version that is certified for use in safety
	critical systems.

	http://www.OpenRTOS.com - Commercial support, development, porting,
	licensing and training services.
*/

#ifndef FREERTOS_CONFIG_H
#define FREERTOS_CONFIG_H

/*-----------------------------------------------------------
 * Application specific definitions.
 *
 * These definitions should be adjusted for your particular hardware and
 * application requirements.
 *
 * THESE PARAMETERS ARE DESCRIBED WITHIN THE 'CONFIGURATION' SECTION OF THE
 * FreeRTOS API DOCUMENTATION AVAILABLE ON THE FreeRTOS.org WEB SITE.
 *
 * See http://www.freertos.org/a00110.html.
 *----------------------------------------------------------*/

#define configUSE_PREEMPTION		1
#define configUSE_IDLE_HOOK			0
#define configUSE_TICK_HOOK			1
#define configCPU_CLOCK_HZ			( ( unsigned portLONG ) 62500000 )
#define configTICK_RATE_HZ			( ( portTickType ) 1000 )
#define configMAX_PRIORITIES		( ( unsigned portBASE_TYPE ) 5 )
#define configMINIMAL_STACK_SIZE	( ( unsigned portSHORT ) 128 )
#define configTOTAL_HEAP_SIZE		( ( size_t ) ( 30 * 1024 ) )
#define configMAX_TASK_NAME_LEN		( 16 )
#define configUSE_TRACE_FACILITY	1
#define configUSE_16_BIT_TICKS		0
#define configIDLE_SHOULD_YIELD		1

/* Co-routine definitions. */
#define configUSE_CO_ROUTINES 		0
#define configMAX_CO_ROUTINE_PRIORITIES ( 2 )

#define configUSE_MUTEXES				1
#define configUSE_COUNTING_SEMAPHORES 	0
#define configUSE_ALTERNATIVE_API 		0
#define configCHECK_FOR_STACK_OVERFLOW	2
#define configUSE_RECURSIVE_MUTEXES		1
#define configQUEUE_REGISTRY_SIZE		0
#define configGENERATE_RUN_TIME_STATS	1

/* Set the following definitions to 1 to include the API function, or zero
to exclude the API function. */

#define INCLUDE_vTaskPrioritySet		1
#define INCLUDE_uxTaskPriorityGet		1
#define INCLUDE_vTaskDelete				1
#define INCLUDE_vTaskCleanUpResources	0
#define INCLUDE_vTaskSuspend			1
#define INCLUDE_vTaskDelayUntil			1
#define INCLUDE_vTaskDelay				1

/* This is the raw value as per the Cortex-M3 NVIC.  Values can be 255
(lowest) to 0 (1?) (highest). */
#define configKERNEL_INTERRUPT_PRIORITY 		255
#define configMAX_SYSCALL_INTERRUPT_PRIORITY 	191 /* equivalent to 0xb0, or priority 11. */


/* This is the value being used as per the ST library which permits 16
priority values, 0 to 15.  This must correspond to the
configKERNEL_INTERRUPT_PRIORITY setting.  Here 15 corresponds to the lowest
NVIC value of 255. */
#define configLIBRARY_KERNEL_INTERRUPT_PRIORITY	15

/*-----------------------------------------------------------
 * Ethernet configuration.
 *-----------------------------------------------------------*/

/* MAC address configuration. */
#define configMAC_ADDR0	0x00
#define configMAC_ADDR1	0x12
#define configMAC_ADDR2	0x13
#define configMAC_ADDR3	0x10
#define configMAC_ADDR4	0x15
#define configMAC_ADDR5	0x11

/* IP address configuration. */
#define configIP_ADDR0		172
#define configIP_ADDR1		25
#define configIP_ADDR2		218
#define configIP_ADDR3		202

/* Netmask configuration. */
#define configNET_MASK0		255
#define configNET_MASK1		255
#define configNET_MASK2		255
#define configNET_MASK3		0


/*-----------------------------------------------------------
 * Macros required to setup the timer for the run time stats.
 *-----------------------------------------------------------*/
/* The run time stats time base just uses the existing high frequency timer
test clock.  All these macros do is clear and return the high frquency
interrupt count respectively. */
extern unsigned long ulRunTimeStatsClock;
#define portCONFIGURE_TIMER_FOR_RUN_TIME_STATS() ulRunTimeStatsClock = 0
#define portGET_RUN_TIME_COUNTER_VALUE() ulRunTimeStatsClock


#endif /* FREERTOS_CONFIG_H */

