# ##############################################################################
# Created by Base System Builder Wizard for Xilinx EDK 7.1.2 Build EDK_H.12.5.1
# Sun Nov 13 16:46:19 2005
# Target Board:  Xilinx Virtex 4 ML403 Evaluation Platform Rev 1
# Family:	 virtex4
# Device:	 xc4vfx12
# Package:	 ff668
# Speed Grade:	 -10
# Processor: Microblaze
# System clock frequency: 100.000000 MHz
# Debug interface: On-Chip HW Debug Module
# On Chip Memory :  64 KB
# ##############################################################################


 PARAMETER VERSION = 2.1.0


 PORT fpga_0_RS232_Uart_RX_pin = fpga_0_RS232_Uart_RX, DIR = INPUT
 PORT fpga_0_RS232_Uart_TX_pin = fpga_0_RS232_Uart_TX, DIR = OUTPUT
 PORT fpga_0_LEDs_4Bit_GPIO_IO_pin = fpga_0_LEDs_4Bit_GPIO_IO, DIR = INOUT, VEC = [0:3]
 PORT fpga_0_LEDs_Positions_GPIO_IO_pin = fpga_0_LEDs_Positions_GPIO_IO, DIR = INOUT, VEC = [0:4]
 PORT sys_clk_pin = dcm_clk_s, DIR = INPUT, SIGIS = DCMCLK
 PORT sys_rst_pin = sys_rst_s, DIR = INPUT


BEGIN microblaze
 PARAMETER INSTANCE = microblaze_0
 PARAMETER HW_VER = 4.00.a
 PARAMETER C_DEBUG_ENABLED = 1
 PARAMETER C_NUMBER_OF_PC_BRK = 2
 PARAMETER C_NUMBER_OF_RD_ADDR_BRK = 1
 PARAMETER C_NUMBER_OF_WR_ADDR_BRK = 1
 BUS_INTERFACE DLMB = dlmb
 BUS_INTERFACE ILMB = ilmb
 BUS_INTERFACE DOPB = mb_opb
 BUS_INTERFACE IOPB = mb_opb
 PORT CLK = sys_clk_s
 PORT DBG_CAPTURE = DBG_CAPTURE_s
 PORT DBG_CLK = DBG_CLK_s
 PORT DBG_REG_EN = DBG_REG_EN_s
 PORT DBG_TDI = DBG_TDI_s
 PORT DBG_TDO = DBG_TDO_s
 PORT DBG_UPDATE = DBG_UPDATE_s
 PORT Interrupt = Interrupt
END

BEGIN opb_v20
 PARAMETER INSTANCE = mb_opb
 PARAMETER HW_VER = 1.10.c
 PARAMETER C_EXT_RESET_HIGH = 0
 PORT SYS_Rst = sys_rst_s
 PORT OPB_Clk = sys_clk_s
END

BEGIN opb_mdm
 PARAMETER INSTANCE = debug_module
 PARAMETER HW_VER = 2.00.a
 PARAMETER C_MB_DBG_PORTS = 1
 PARAMETER C_USE_UART = 1
 PARAMETER C_UART_WIDTH = 8
 PARAMETER C_BASEADDR = 0x41400000
 PARAMETER C_HIGHADDR = 0x4140ffff
 BUS_INTERFACE SOPB = mb_opb
 PORT OPB_Clk = sys_clk_s
 PORT DBG_CAPTURE_0 = DBG_CAPTURE_s
 PORT DBG_CLK_0 = DBG_CLK_s
 PORT DBG_REG_EN_0 = DBG_REG_EN_s
 PORT DBG_TDI_0 = DBG_TDI_s
 PORT DBG_TDO_0 = DBG_TDO_s
 PORT DBG_UPDATE_0 = DBG_UPDATE_s
END

BEGIN lmb_v10
 PARAMETER INSTANCE = ilmb
 PARAMETER HW_VER = 1.00.a
 PARAMETER C_EXT_RESET_HIGH = 0
 PORT SYS_Rst = sys_rst_s
 PORT LMB_Clk = sys_clk_s
END

BEGIN lmb_v10
 PARAMETER INSTANCE = dlmb
 PARAMETER HW_VER = 1.00.a
 PARAMETER C_EXT_RESET_HIGH = 0
 PORT SYS_Rst = sys_rst_s
 PORT LMB_Clk = sys_clk_s
END

BEGIN lmb_bram_if_cntlr
 PARAMETER INSTANCE = dlmb_cntlr
 PARAMETER HW_VER = 1.00.b
 PARAMETER C_BASEADDR = 0x00000000
 PARAMETER C_HIGHADDR = 0x0000ffff
 BUS_INTERFACE SLMB = dlmb
 BUS_INTERFACE BRAM_PORT = dlmb_port
END

BEGIN lmb_bram_if_cntlr
 PARAMETER INSTANCE = ilmb_cntlr
 PARAMETER HW_VER = 1.00.b
 PARAMETER C_BASEADDR = 0x00000000
 PARAMETER C_HIGHADDR = 0x0000ffff
 BUS_INTERFACE SLMB = ilmb
 BUS_INTERFACE BRAM_PORT = ilmb_port
END

BEGIN bram_block
 PARAMETER INSTANCE = lmb_bram
 PARAMETER HW_VER = 1.00.a
 BUS_INTERFACE PORTA = ilmb_port
 BUS_INTERFACE PORTB = dlmb_port
END

BEGIN opb_uartlite
 PARAMETER INSTANCE = RS232_Uart
 PARAMETER HW_VER = 1.00.b
 PARAMETER C_BAUDRATE = 9600
 PARAMETER C_DATA_BITS = 8
 PARAMETER C_ODD_PARITY = 0
 PARAMETER C_USE_PARITY = 0
 PARAMETER C_CLK_FREQ = 100000000
 PARAMETER C_BASEADDR = 0x40600000
 PARAMETER C_HIGHADDR = 0x4060ffff
 BUS_INTERFACE SOPB = mb_opb
 PORT OPB_Clk = sys_clk_s
 PORT Interrupt = RS232_Uart_Interrupt
 PORT RX = fpga_0_RS232_Uart_RX
 PORT TX = fpga_0_RS232_Uart_TX
END

BEGIN opb_gpio
 PARAMETER INSTANCE = LEDs_4Bit
 PARAMETER HW_VER = 3.01.b
 PARAMETER C_GPIO_WIDTH = 4
 PARAMETER C_IS_DUAL = 0
 PARAMETER C_IS_BIDIR = 1
 PARAMETER C_ALL_INPUTS = 0
 PARAMETER C_BASEADDR = 0x40020000
 PARAMETER C_HIGHADDR = 0x4002ffff
 BUS_INTERFACE SOPB = mb_opb
 PORT OPB_Clk = sys_clk_s
 PORT GPIO_IO = fpga_0_LEDs_4Bit_GPIO_IO
END

BEGIN opb_gpio
 PARAMETER INSTANCE = LEDs_Positions
 PARAMETER HW_VER = 3.01.b
 PARAMETER C_GPIO_WIDTH = 5
 PARAMETER C_IS_DUAL = 0
 PARAMETER C_IS_BIDIR = 1
 PARAMETER C_ALL_INPUTS = 0
 PARAMETER C_BASEADDR = 0x40000000
 PARAMETER C_HIGHADDR = 0x4000ffff
 BUS_INTERFACE SOPB = mb_opb
 PORT OPB_Clk = sys_clk_s
 PORT GPIO_IO = fpga_0_LEDs_Positions_GPIO_IO
END

BEGIN opb_timer
 PARAMETER INSTANCE = opb_timer_1
 PARAMETER HW_VER = 1.00.b
 PARAMETER C_COUNT_WIDTH = 32
 PARAMETER C_ONE_TIMER_ONLY = 1
 PARAMETER C_BASEADDR = 0x41c00000
 PARAMETER C_HIGHADDR = 0x41c0ffff
 BUS_INTERFACE SOPB = mb_opb
 PORT OPB_Clk = sys_clk_s
 PORT Interrupt = opb_timer_1_Interrupt
END

BEGIN opb_intc
 PARAMETER INSTANCE = opb_intc_0
 PARAMETER HW_VER = 1.00.c
 PARAMETER C_BASEADDR = 0x41200000
 PARAMETER C_HIGHADDR = 0x4120ffff
 PARAMETER C_HAS_IPR = 0
 BUS_INTERFACE SOPB = mb_opb
 PORT Irq = Interrupt
 PORT Intr = RS232_Uart_Interrupt & opb_timer_1_Interrupt
END

BEGIN dcm_module
 PARAMETER INSTANCE = dcm_0
 PARAMETER HW_VER = 1.00.a
 PARAMETER C_CLK0_BUF = TRUE
 PARAMETER C_CLKIN_PERIOD = 10.000000
 PARAMETER C_CLK_FEEDBACK = 1X
 PARAMETER C_EXT_RESET_HIGH = 1
 PORT CLKIN = dcm_clk_s
 PORT CLK0 = sys_clk_s
 PORT CLKFB = sys_clk_s
 PORT RST = net_gnd
 PORT LOCKED = dcm_0_lock
END

