(footprint "molex_5052781533" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 742128fa-64a1-4015-9186-c0951cc37934)
  )
  (fp_text value "molex_5052781533" (at 0 2.8) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 852ed249-f0a2-4241-b7a7-a8a324f5d01b)
  )
  (fp_line (start -7.16 1.81) (end -3.75 1.81)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8bdf82d2-53f4-4739-b395-3db85bf96110))
  (fp_line (start -7.16 3.47) (end -7.16 1.81)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp f2f6e15b-864b-4373-a1ef-93429f59d5a5))
  (fp_line (start -3.75 -0.68) (end 3.75 -0.68)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp dc747e05-73de-4dab-a37e-8135109842f0))
  (fp_line (start -3.75 0.68) (end -3.75 3.47)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 90a6a11d-100f-4c43-9f4b-16f2602b8f0d))
  (fp_line (start -3.75 0.68) (end 3.75 0.68)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 94114ff9-90f6-46cd-9a65-b881915be36e))
  (fp_line (start -3.75 1.81) (end -3.75 -0.68)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b3f7d884-d03f-4776-a23e-8efe0887b2b2))
  (fp_line (start -3.75 3.47) (end -7.16 3.47)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b033cc0e-d7a4-4bb8-9ff9-deef6f99f7cd))
  (fp_line (start 3.75 0.68) (end 3.75 3.47)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 782b9ddc-444a-455e-92e4-1235c614762c))
  (fp_line (start 3.75 1.81) (end 3.75 -0.68)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp bf61ef0d-e5ce-40c8-9c5c-79f3835b610b))
  (fp_line (start 3.75 3.47) (end 7.16 3.47)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 595632a7-e118-4a26-a3d2-138a67d36148))
  (fp_line (start 7.16 1.81) (end 3.75 1.81)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 3119c637-1eae-412b-8756-78c57abc5bd8))
  (fp_line (start 7.16 3.47) (end 7.16 1.81)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp eb5fa637-1246-4a06-bcbe-187a0666ae87))
  (fp_line (start -7.4 -0.9) (end -7.4 3.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c0776079-7b04-44e6-b684-4cde2dce3c2e))
  (fp_line (start -7.4 -0.9) (end 7.4 -0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 143ff291-19aa-4e8b-acba-6eb9eeb28911))
  (fp_line (start -7.4 3.7) (end 7.4 3.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a0e5c667-5c1d-43ca-a9c5-05941476e811))
  (fp_line (start 7.4 -0.9) (end 7.4 3.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb9f0c8e-335c-45af-ae5d-19bea371eb1f))
  (pad "0" smd rect (at -5.8 2.7) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp e5dd2cd0-0bca-440f-86bb-fa74c03bb0df))
  (pad "0" smd rect (at 5.8 2.7) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp e9cc22d4-936f-45a3-9348-a2524ab1b555))
  (pad "1" smd rect (at -3.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 4caa7b8d-9508-4606-b60f-be64151090af))
  (pad "2" smd rect (at -3 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fe349ef2-4b64-4e7f-b498-1d292be98d08))
  (pad "3" smd rect (at -2.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cade5c23-30c7-4fd3-9945-1b7ad5887d50))
  (pad "4" smd rect (at -2 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 115c5665-0ce3-4e30-b29a-aff4c074393a))
  (pad "5" smd rect (at -1.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 61b2da59-3aae-4e42-8dea-b8509536f15c))
  (pad "6" smd rect (at -1 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 58b74605-8f58-4737-8e73-4306eff213bc))
  (pad "7" smd rect (at -0.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b3c84592-abe3-4300-b9b9-e36b5c75b708))
  (pad "8" smd rect (at 0 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9e645c61-7ca5-46e8-9797-3d8e37e1fc49))
  (pad "9" smd rect (at 0.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 5dd6f4ee-8b17-4a9c-8e6a-64dc90bc7a6c))
  (pad "10" smd rect (at 1 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6031d0f0-2c08-4f2e-a223-e9e71225470f))
  (pad "11" smd rect (at 1.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9342f893-56d8-445d-9762-0866df50b116))
  (pad "12" smd rect (at 2 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 4d8a297d-877d-43bc-9cb7-509a3ec47b7c))
  (pad "13" smd rect (at 2.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 948d41aa-6789-41f1-84c2-b6399f40a010))
  (pad "14" smd rect (at 3 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a9959dc6-778b-4b44-8a78-0c87fc2c4136))
  (pad "15" smd rect (at 3.5 0) (size 0.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d19f90c8-d802-4aba-86b3-806f4b918a58))
)
