(footprint "QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=274), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 21c0b8c3-f1f8-4216-88df-c98091394b0c)
  )
  (fp_text value "QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias2" (at 0 3.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ae8f8834-6dd1-4684-81b3-acde8b33ce3d)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b88e3d60-deec-4f4e-98b3-40d3f8976945)
  )
  (fp_line (start -2.11 2.11) (end -2.11 1.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e49b3075-f586-482d-a045-0030bc998947))
  (fp_line (start -1.385 -2.11) (end -2.11 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2132722-7fa4-42de-9018-c40471d71cd8))
  (fp_line (start -1.385 2.11) (end -2.11 2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f8c03f5-da9c-4330-be67-922c0435d4fe))
  (fp_line (start 1.385 -2.11) (end 2.11 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e17beb02-f77a-46f8-9393-e4b70481efe1))
  (fp_line (start 1.385 2.11) (end 2.11 2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 363cede7-da5e-4347-b80e-d60c5a97ddf5))
  (fp_line (start 2.11 -2.11) (end 2.11 -1.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f144b8e6-7df5-4706-8884-8e07af52a83d))
  (fp_line (start 2.11 2.11) (end 2.11 1.385)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09af8ea7-6a3b-485a-b9c2-755cdd158210))
  (fp_line (start -2.6 -2.6) (end -2.6 2.6)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp daa1aaa8-ed10-4a00-a017-7a1033276046))
  (fp_line (start -2.6 2.6) (end 2.6 2.6)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9180995e-c6c1-4251-8822-d23271e2d29d))
  (fp_line (start 2.6 -2.6) (end -2.6 -2.6)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c7b477e6-ba04-4d68-a6e6-2ab58a83ace7))
  (fp_line (start 2.6 2.6) (end 2.6 -2.6)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b10281e8-a5d3-4101-a95f-f6fa4d1d1d5e))
  (fp_line (start -2 -1) (end -1 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82c83875-48f9-476f-a25c-b685042faa67))
  (fp_line (start -2 2) (end -2 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b58cf903-2e85-40bc-b628-ff783ab7bf0f))
  (fp_line (start -1 -2) (end 2 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25862eef-a976-4949-b440-f096517a8761))
  (fp_line (start 2 -2) (end 2 2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8a39e4ae-e0e6-4403-8188-5430718c9a92))
  (fp_line (start 2 2) (end -2 2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1823a36-1086-459b-ba57-61d6fc6dc56e))
  (pad "" smd roundrect (at -0.625 -0.625) (size 1.08 1.08) (layers "F.Paste") (roundrect_rratio 0.231481) (tstamp 50d2398a-228e-434d-a1fc-da08de1cbc54))
  (pad "" smd roundrect (at -0.625 0.625) (size 1.08 1.08) (layers "F.Paste") (roundrect_rratio 0.231481) (tstamp 5ceca9ad-9ba5-4791-a0ca-c57f98a450ee))
  (pad "" smd roundrect (at 0.625 -0.625) (size 1.08 1.08) (layers "F.Paste") (roundrect_rratio 0.231481) (tstamp a47b07a8-c41a-49e4-86c5-f25d0af1b9f4))
  (pad "" smd roundrect (at 0.625 0.625) (size 1.08 1.08) (layers "F.Paste") (roundrect_rratio 0.231481) (tstamp e998ea71-bcc3-4add-89d8-ccd8d76543c6))
  (pad "1" smd roundrect (at -1.9375 -1) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 84c3cdf6-a958-44c4-a733-7d7eb0ed1bff))
  (pad "2" smd roundrect (at -1.9375 -0.5) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c5d86626-f8c2-48af-97e5-8c3e23683b51))
  (pad "3" smd roundrect (at -1.9375 0) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 44349d44-0f33-419b-867c-1e9f3e2fa43b))
  (pad "4" smd roundrect (at -1.9375 0.5) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 22ddca70-69a4-4606-8c3b-9cb02ec31f52))
  (pad "5" smd roundrect (at -1.9375 1) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5d484f2e-a034-4155-b403-704d5d5de13e))
  (pad "6" smd roundrect (at -1 1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5a7f2936-1ef9-4f49-a75f-b9fd76385696))
  (pad "7" smd roundrect (at -0.5 1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp eee6650d-a61b-4a03-b88a-de5f558c9737))
  (pad "8" smd roundrect (at 0 1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 23ca50c4-4763-4c23-8116-41a650b50084))
  (pad "9" smd roundrect (at 0.5 1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cc6fe8a2-5fab-4f45-a5a9-a95ec2bb4c48))
  (pad "10" smd roundrect (at 1 1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c446419e-1096-4ee0-9747-e98bdc561381))
  (pad "11" smd roundrect (at 1.9375 1) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7536ad7a-f837-475d-bfb7-17eb5210a4ef))
  (pad "12" smd roundrect (at 1.9375 0.5) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f7235531-a611-47ff-8c55-c22d858e61c8))
  (pad "13" smd roundrect (at 1.9375 0) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 71cfb449-211f-4c1b-8ef9-e2f417302ecc))
  (pad "14" smd roundrect (at 1.9375 -0.5) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ae97d746-be11-4366-8bb2-0c36715008c7))
  (pad "15" smd roundrect (at 1.9375 -1) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5f7d339b-624f-4767-a82f-9db76c53b589))
  (pad "16" smd roundrect (at 1 -1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2e4ed629-e14b-4313-aed2-f5636f485ded))
  (pad "17" smd roundrect (at 0.5 -1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5bae3966-05df-4ddc-b49d-8b6e84856af2))
  (pad "18" smd roundrect (at 0 -1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d6c96754-8607-45be-995e-c6c5a1636755))
  (pad "19" smd roundrect (at -0.5 -1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8cd34855-8bf1-4b5f-9a7a-cf0b0aa744ff))
  (pad "20" smd roundrect (at -1 -1.9375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3e986b39-f3c3-4497-b831-d39ca6b65738))
  (pad "21" thru_hole circle (at -0.85 -0.85) (size 0.5 0.5) (drill 0.2) (layers "*.Cu") (tstamp edcfb17a-74ca-4605-96e5-a85ead22d1b3))
  (pad "21" thru_hole circle (at -0.85 0.85) (size 0.5 0.5) (drill 0.2) (layers "*.Cu") (tstamp b2001083-e153-4fd3-9469-53f064da2d1a))
  (pad "21" thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.2) (layers "*.Cu") (tstamp bb820de0-2040-486c-875d-210aa2819d58))
  (pad "21" smd rect (at 0 0) (size 2.5 2.5) (layers "F.Cu" "F.Mask") (tstamp f0ab5a07-5984-435f-ab1e-010d349506b5))
  (pad "21" smd rect (at 0 0) (size 2.5 2.5) (layers "B.Cu") (tstamp 5fdace69-b414-4278-ade0-879fd5396445))
  (pad "21" thru_hole circle (at 0.85 -0.85) (size 0.5 0.5) (drill 0.2) (layers "*.Cu") (tstamp ccf2e987-6edf-4075-8add-5785bc357962))
  (pad "21" thru_hole circle (at 0.85 0.85) (size 0.5 0.5) (drill 0.2) (layers "*.Cu") (tstamp d4b9d995-c367-4731-ae42-590cfa7d1d5e))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
