(footprint "SAMDSWD" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.4 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp c40dbe6b-200a-46e5-87e2-283fa7c232cd)
  )
  (fp_text value "SAMDSWD" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2add179c-a99c-4f5d-8cdf-9fe1f3b9929f)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 887a634d-dd52-4942-a70a-ae2040827809)
  )
  (pad "1" smd roundrect (at -2.55 0.05) (size 0.8 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5) (tstamp fee5d0d0-e381-480f-adb1-1ef8f9c7b25e))
  (pad "2" smd roundrect (at -1.28 0.05) (size 0.8 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5) (tstamp 75657567-2b61-4b28-a745-23c68b8191a5))
  (pad "3" smd roundrect (at -0.01 0.05) (size 0.8 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5) (tstamp 40e11af3-0302-46cf-8a73-ca67774fb095))
  (pad "4" smd roundrect (at 1.26 0.05) (size 0.8 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5) (tstamp 69a43ffd-ccbf-4121-a379-20709ce9c306))
  (pad "5" smd roundrect (at 2.53 0.05) (size 0.8 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5) (tstamp 4bc4ec74-6cce-4250-a338-66edb592f10d))
)
