% $Id$ %
\section{Settings}
\begin{center}
  \begin{longtable}{@{}lll@{}}\toprule
    \textbf{Setting} & \textbf{Allowed Values} & \textbf{Unit}\\
    \midrule
    \endhead
    volume & \opt{player}{-78 to +18}
             \opt{recorder,recorderv2fm,ondiosp,ondiofm}{-100 -to +12}
             \opt{h1xx,h300}{-84 to 0}
             \opt{ipodnano}{-72 to +6}
             \opt{ipodvideo}{-57 to +6}
             \opt{ipodcolor,x5}{-\fixme{??} to +\fixme{??}}
                    & dB\\
    \nopt{x5}{
      bass & \opt{MASCODEC}{-15 to +15}
             \opt{h1xx,h300}{0 to +24}
             \opt{ipod}{-6 to +9}
                    & dB\\
      treble & \opt{MASCODEC}{-15 to +15}
               \opt{h1xx,h300}{0 to +6}
               \opt{ipod}{-6 to +9}
                    & dB\\
    }
    balance & -100 to +100 & \%\\
    channels & stereo, mono, custom & N/A\\
             & mono left, mono right, karaoke & \\
    shuffle & on, off & N/A\\
    repeat & off, all, one, shuffle, ab & N/A\\
    play selected & on, off & N/A\\
    resume & on, off & N/A\\
    scan min step & 1, 2, 3, 4, 5, 6, 8, 10, 15, & seconds\\
                  & 20, 25, 30, 45, 60 &\\
    scan accel & 0 to 15 & seconds\\
    antiskip & 0 to 7 & seconds\\
    volume fade & on, off & N/A\\
    id3 tag priority & v2-v1, v1-v2 & N/A\\
    sort case & on, off & N/A\\
    show files & all, supported, music, playlists & N/A\\
    follow playlist & on, off & N/A\\
    playlist viewer icons & on, off & N/A\\
    playlist viewer indices & on, off & N/A\\
    playlist viewer track display & track name,full path & N/A\\
    recursive directory insert & on, off & N/A\\
    scroll speed & 1 to 25 & Hz\\
    scroll delay & 0 to 250 & 1/10s\\
    scroll step & 1 to 112 & pixels\\
    bidir limit & 0 to 200 & \% screen\\
    contrast & 0 to 63 & N/A\\
    backlight timeout & off, on, 1, 2, 3, 4, 5, & seconds\\
                      & 6, 7, 8, 9, 10, 15, 20, & \\
                      & 25, 30, 45, 60, 90 & \\
    backlight timeout plugged & off, on, 1, 2, 3, 4, 5, & seconds\\
                              & 6, 7, 8, 9, 10, 15, 20, & \\
                              & 25, 30, 45, 60, 90 & \\
    disk spindown & 3 to 254 & seconds\\
    battery capacity & 1500 - 3200 & mAh\\
    idle poweroff & off, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, & minutes\\
                  & 15, 30, 45, 60 & \\
    lang & /path/filename.lng & N/A\\
    wps & /path/filename.wps & N/A\\
    autocreate bookmarks & off,on & N/A\\
    autoload bookmarks & off,on & N/A\\
    use most-recent-bookmarks & off,on & N/A\\
    talk dir & off, number, spell, enter, hover & N/A\\
    talk file & off, number, spell & N/A\\
    talk menu & off, on & N/A\\
    tagcache\_autoupdate & on, off & N/A\\
    warn when erasing dynamic playlist & on, off & N/A\\
    
    \opt{SWCODEC}{
      replaygain & on, off & N/A\\
      replaygain type & track, album, track shuffle & N/A\\
      replaygain noclip & on, off & N/A\\
      replaygain preamp & -120 to 120 & 0.1dB\\
%
      crossfade & off, shuffle, track skip, always & N/A\\
      crossfade fade in delay & 0 to 7 & seconds\\
      crossfade fade out delay & 0 to 7 & seconds\\
      crossfade fade in duration & 0 to 15 & seconds\\
      crossfade fade out duration & 0 to 15 & seconds\\
      crossfade fade out mode & crossfade, mix & N/A\\
%
      crossfeed & on, off & N/A\\
      crossfeed direct gain & 0 to 60 & 0.1dB\\
      crossfeed cross gain & 30 to 120 & 0.1dB\\
      crossfeed hf attenuation & 60 to 240 & 0.1dB\\
      crossfeed hf cutoff & 500 to 2000 & Hz\\
%
      eq enabled & on, off & N/A\\
      eq precut& 0 to 240 & 0.1dB\\
      eq band 0 cutoff & 0 to 32768 & Hz\\
      eq band 1 cutoff & 0 to 32768 & Hz\\
      eq band 2 cutoff & 0 to 32768 & Hz\\
      eq band 3 cutoff & 0 to 32768 & Hz\\
      eq band 4 cutoff & 0 to 32768 & Hz\\
      eq band 0 q & 0 to 64 & N/A\\
      eq band 1 q & 0 to 64 & N/A\\
      eq band 2 q & 0 to 64 & N/A\\
      eq band 3 q & 0 to 64 & N/A\\
      eq band 4 q & 0 to 64 & N/A\\
      eq band 0 gain & -240 to 240 & 0.1dB\\
      eq band 1 gain & -240 to 240 & 0.1dB\\
      eq band 2 gain & -240 to 240 & 0.1dB\\
      eq band 3 gain & -240 to 240 & 0.1dB\\
      eq band 4 gain & -240 to 240 & 0.1dB\\
%
      beep & off, weak, moderate, strong & N/A\\
      dircache & on, off & N/A\\
      tagcache\_ram & on, off & N/A\\
    }

    \opt{recorder,recorderv2fm}{
      loudness & 0 to 17 & N/A\\
      superbass & on, off & N/A\\
      auto volume & off, 20ms, 2s, 4s, 8s & seconds\\
      mdb enable & on,off & N/A\\
      mdb strength & 0 to 127 & dB\\
      mdb harmonics & 0 to 100 & \%\\
      mdb center & 20 to 300 & Hz\\
      mdb shape & 50 to 300 & Hz\\
    }

    \opt{HAVE_LCD_BITMAP}{
      peak meter release & 1 to 126 & ?\\
      peak meter hold & off, 200ms, 300ms, 500ms, & N/A \\
                     & 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 15, &\\ 
                     & 20, 30, 1min & \\
      peak meter clip hold & on, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10,& N/A \\
                           & 15, 20, 25, 30, 45, 60, 90, 2min, &\\
                           & 3min, 5min, 10min, 20min, &\\
                           & 45min, 90min & \\
      peak meter busy & on, off & N/A\\
      peak meter dbfs & on, off & on:~dbfs,\\
                      &         & off:~linear\\
      peak meter min  & 0 to 89 (dB) or 0 to 100 (\%) & dB or \%\\
      peak meter max  & 0 to 89 /(dB) or 0 to 100 (\%) & dB or \%\\
      statusbar & on, off & N/A\\
      scrollbar & on, off & N/A\\
      volume display & graphic, numeric & N/A\\
      battery display & graphic, numeric & N/A\\
      font & /path/filename.fnt & N/A\\
      invert & on, off & N/A\\
      disk poweroff & on, off & N/A\\
    }
    
    \opt{HAVE_LCD_COLOR}{
      backdrop & /path/filename.bmp & N/A\\
      foreground color & 000000 to FFFFFF & RRGGBB\\
      background color & 000000 to FFFFFF & RRGGBB\\ 
    }
    
    \opt{HAVE_REMOTE_LCD}{
      rwps & /path/filename.rwps & N/A\\
      remote contrast & 5 to 63 & N/A\\
      remote invert & on, off & N/A\\
      remote flip display & on, off & N/A\\
      remote backlight timeout & off, on, 1, 2, 3, 4, 5, & seconds\\
                               & 6, 7, 8, 9, 10, 15, 20, & \\
                               & 25, 30, 45, 60, 90 & \\
      remote backlight timeout plugged & off, on, 1, 2, 3, 4, 5, & seconds\\
                                       & 6, 7, 8, 9, 10, 15, 20, & \\
                                       & 25, 30, 45, 60, 90 & \\
      remote caption backlight & on, off & N/A\\
      remote scroll speed & 0 to 15 & N/A\\
      remote scroll step & 1 to 160 & N/A\\
      remote scroll delay & 0 to 250 & N/A\\ 
      remote bidir limit & 0 to 200 & N/A\\
      backlight filters first remote keypress & on, off & N/A\\
      \opt{h1xx,h300}{
        remote reduce ticking & on, off & N/A\\
      }
    }
    \opt{CONFIG_RTC}{
      time format & 12hour, 24hour & N/A\\      
    }
    \opt{HAVE_RECORDING}{
     rec quality & 0 to 7 & 0: small size,\\
                 &        & 7: high quality\\
     rec frequency & 48, 44, 32, 24, 22, 16 & kHz\\
     rec source & mic, line, spdif & N/A\\
     rec channels & mono, stereo & N/A\\
     rec mic gain & 0 to 15 & N/A\\
     rec left gain & 0 to 15 & N/A\\
     rec right gain & 0 to 15 & N/A\\
     editable recordings & off,on & N/A\\
     rec timesplit & off, 0:05, 0:10, 0:15, 0:30, 1:00, & h:mm\\
                   & 2:00, 4:00, 6:00, 8:00, 16:00, 24:00 & \\
     pre-recording time & off, 1 to 30 & seconds\\
     rec directory & /recordings,current & N/A\\
    }
    \opt{CONFIG_TUNER}{
      force fm mono & off, on & N/A\\
    }
    \opt{player}{
      jump scroll & 0 to 5 & N/A\\
      jump scroll delay & 0 to 250 & 0.01s\\
    }
    \bottomrule
  \end{longtable}
\end{center}
