\subsection{Mikmod}

Mikmod plays most common tracker music formats.

\begin{btnmap}
    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,GIGABEAT_PAD,GIGABEAT_S_PAD%
        ,IAUDIO_X5_PAD,MROBE100_PAD,PBELL_VIBE500_PAD,SANSA_FUZEPLUS_PAD,SAMSUNG_YH92X_PAD%
        ,SAMSUNG_YH820_PAD}{\ButtonUp/ \ButtonDown}
    \opt{IPOD_3G_PAD,IPOD_4G_PAD,SANSA_E200_PAD,SANSA_FUZE_PAD}{\ButtonScrollFwd/ \ButtonScrollBack}
    \opt{IRIVER_H10_PAD,MPIO_HD300_PAD}{\ButtonScrollUp/ \ButtonScrollDown}
    \opt{SANSA_C200_PAD,SANSA_CLIP_PAD,MPIO_HD200_PAD}{\ButtonVolUp/ \ButtonVolDown}
    \opt{COWON_D2_PAD}{\TouchTopMiddle{} / \TouchBottomMiddle}
    \opt{XDUOO_X3_PAD}{\ButtonVolUp/ \ButtonVolDown}
       \opt{HAVEREMOTEKEYMAP}{& }
    & Volume up/ Volume down\\
    %
    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,GIGABEAT_PAD,GIGABEAT_S_PAD%
        ,IAUDIO_X5_PAD,MROBE100_PAD,IPOD_3G_PAD,IPOD_4G_PAD,SANSA_E200_PAD%
        ,SANSA_FUZE_PAD,IRIVER_H10_PAD,SANSA_C200_PAD,SANSA_CLIP_PAD,PBELL_VIBE500_PAD%
        ,SANSA_FUZEPLUS_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}
        {\ButtonRight/ \ButtonLeft}
    \opt{MPIO_HD200_PAD,MPIO_HD300_PAD}{\ButtonFF / \ButtonRew}
    \opt{COWON_D2_PAD}{\TouchMidRight{} / \TouchMidLeft}
    \opt{XDUOO_X3_PAD}{\ButtonNext/ \ButtonPrev}
       \opt{HAVEREMOTEKEYMAP}{& }
    & Skip to next/prev file\\
    %
    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,GIGABEAT_PAD,GIGABEAT_S_PAD%
        ,IAUDIO_X5_PAD,MROBE100_PAD,IPOD_3G_PAD,IPOD_4G_PAD,SANSA_E200_PAD%
        ,SANSA_FUZE_PAD,IRIVER_H10_PAD,SANSA_C200_PAD,SANSA_CLIP_PAD,PBELL_VIBE500_PAD%
        ,SANSA_FUZEPLUS_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}
        {Long \ButtonRight/ Long \ButtonLeft}
    \opt{MPIO_HD200_PAD,MPIO_HD300_PAD}{Long \ButtonFF / Long \ButtonRew}
    \opt{COWON_D2_PAD}{Long \TouchMidRight{} / Long \TouchMidLeft}
    \opt{XDUOO_X3_PAD}{Long \ButtonNext/ Long \ButtonPrev}
       \opt{HAVEREMOTEKEYMAP}{& }
    & Skip to next/prev sequence\\
    %
    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOn}
    \opt{IPOD_3G_PAD,IPOD_4G_PAD,GIGABEAT_S_PAD,IAUDIO_X5_PAD,IRIVER_H10_PAD,PBELL_VIBE500_PAD%
        ,MPIO_HD200_PAD,MPIO_HD300_PAD,SANSA_FUZEPLUS_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}
        {\ButtonPlay}
    \opt{SANSA_E200_PAD,SANSA_FUZE_PAD,SANSA_C200_PAD,SANSA_CLIP_PAD}{\ButtonUp}
    \opt{GIGABEAT_PAD}{\ButtonA}
    \opt{MROBE100_PAD}{\ButtonDisplay}
    \opt{COWON_D2_PAD}{\TouchCenter}
    \opt{XDUOO_X3_PAD}{\ButtonPlay}
       \opt{HAVEREMOTEKEYMAP}{& }
    & Pause/Resume playback\\
    %
    \opt{XDUOO_X3_PAD}{\ButtonOption}
       \opt{HAVEREMOTEKEYMAP}{& }
    & Enter configuration menu\\
    %
    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOff}
    \opt{IPOD_3G_PAD,IPOD_4G_PAD}{\ButtonSelect+\ButtonMenu}
    \opt{GIGABEAT_PAD,GIGABEAT_S_PAD,SANSA_E200_PAD,SANSA_C200_PAD,SANSA_CLIP_PAD,IAUDIO_X5_PAD%
        ,IRIVER_H10_PAD,MROBE100_PAD,COWON_D2_PAD,SANSA_FUZEPLUS_PAD}{\ButtonPower}
    \opt{SANSA_FUZE_PAD}{Long \ButtonHome}
    \opt{PBELL_VIBE500_PAD}{\ButtonRec}
    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{Long \ButtonPlay}
    \opt{MPIO_HD200_PAD}{\ButtonRec + \ButtonPlay}
    \opt{MPIO_HD300_PAD}{Long \ButtonMenu}
    \opt{XDUOO_X3_PAD}{\ButtonPower}
       \opt{HAVEREMOTEKEYMAP}{& }
    & Stop playback and quit\\
\end{btnmap}

Mikmod is highly configurable, and has many setting that affect output quality.  However, 
less powerful \dap{}s may lack the cpu resources that higher quality settings require, expecially
on more complex modules.  Settings are saved and re-loaded automatically.

\subsubsection{Configuration}
\begin {description}
\item [Panning Separation]
    Specifies how far to separate Left and Right channels.  128 is full separation, 0 is none, effectively resulting in mono sound.
\item [Reverberation]
    Specifies the amount of reberb (echo) to add to the mix.  0 is disabled.
\item [Interpolation]
    Enabling this improves the sound of lower-quality instruments.  Recommended.
\item [Swap Channels]
    Swaps the left and right channels.
\item [Surround]
    Enables a faux-surround effect.
\item [HQ Mixer]
    Enables a high quality audio mixer that is very CPU intensive.  Must restart the plugin to take effect.
\item [Sample Rate]
    Select the sample/mixing rate for playback.  44.1KHz or higher is recommended, but you can select from any rate the \dap{} natively supports.
\end {description}
