(footprint "qtouch-button" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 496b315d-fd3c-44c2-82f5-3c8cccbd57f6)
  )
  (fp_text value "qtouch-button" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0b072238-3f0b-4e49-9cf1-e4999626471f)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c5d799e9-aa64-4815-b5df-94355890efbe)
  )
  (fp_circle (center 0 0) (end 2.5 0)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp ebb1347e-43ce-4ede-81fd-1525081de778))
  (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.2) (layers "*.Cu") (tstamp bb5ba437-b5e3-47b4-9ad6-c4769338f968))
)
