(footprint "MountingHole_2.2mm_M2_Pad_Via2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Mounting Hole 2.2mm, M2")
  (tags "mounting hole 2.2mm m2")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fd72721f-a1f0-4d78-99b7-3f27b5dd3859)
  )
  (fp_text value "MountingHole_2.2mm_M2_Pad_Via2" (at 0 3.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4db890d3-f11e-4e7c-ae4d-c99f86e181f8)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 54dee16e-e948-408e-8c8b-f49f5cd7d828)
  )
  (fp_circle (center 0 0) (end 2.2 0)
    (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp aea6c94c-a561-481c-b6bf-1ba6765c9e6f))
  (fp_circle (center 0 0) (end 2.45 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 2bfe1ee3-de75-4e79-ba13-9937c3e3e692))
  (pad "1" thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp 2f08161d-698c-4b06-a92e-718f0d36f3db))
  (pad "1" thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp 293a4619-7e8e-451d-90c5-d77537974af8))
  (pad "1" thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp ac15cb78-4aea-46a6-b15a-27b4f935b6d5))
  (pad "1" thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp 28e53e35-23da-4541-a8bc-31da32b5e660))
  (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask") (tstamp e40ffd4d-af4a-4e36-aedd-777adf927ef1))
  (pad "1" thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp d1d93a02-33d2-4fb1-910e-1b0a08c69f3d))
  (pad "1" thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp 63e68424-98d6-47d2-808e-02bc0c9c665a))
  (pad "1" thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp 175d379b-0ae3-45b7-9bd5-1e8675d9de65))
  (pad "1" thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.2) (layers "*.Cu" "*.Mask") (tstamp f9ce87bf-5f89-4bd3-b699-c9a46d04dbad))
)
